SPLP has made revisions to the proposed workspaces in Delaware County since submittal of the original application.  These revisions have been the result of landowner requests, agency requests, the avoidance of sensitive species or their habitats, and/or to further reduce impacts to aquatic resources.  The additions and subtractions to the workspaces are listed and quantified within Table 1.  In addition, this attachment highlights the location and extent of these additions and subtractions to the workspaces on a set of site plans.  Each addition/subtraction has been assigned an identification code and that code is reflected below and on the set of site plans.  The additions and subtractions are listed from west to east. A total of approximately 22.76 acres was added and 1.93 acres subtracted for a net increase of 20.83 acres of earth disturbance.

**Table 1.  Pennsylvania Pipeline Project LOD Additions and Subtractions.**

| **CHANGE ID** | **COUNTY** | **REASON FOR CHANGE** | **ACREAGE** | **LOD ADDITION OR SUBTRACTION** | **WETLAND DELINEATION1** | **PNDI EVALUATION2** | **SHEET NUMBER** | **E&S SHEET NUMBER** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Twin Oaks Station | DELAWARE | Station design | 6.46 | Addition  | Yes | YesA | 23 | 6.35 |
| Sub-205 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.02 | Subtraction | NA | NA | 1 | 6.02 |
| Sub-206 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.05 | Subtraction | NA | NA | 1 | 6.02 |
| Sub-207 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.01 | Subtraction | NA | NA | 1 | 6.02 |
| Sub-208 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.16 | Subtraction | NA | NA | 1 | 6.02 |
| Add-208 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.16 | Addition | Yes | YesA | 1 | 6.02 |
| Add-209 | DELAWARE | Temporary Access Road added to facilitate installation. No additional aquatic resources impacted. | 0.29 | Addition | Yes | YesA | 3 | 6.04 |
| Add-210 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.05 | Addition | Yes | YesA | 6 | 6.09 |
| Add-211 | DELAWARE | Additional LOD determined to be available and acquired to allow safe installation in vicinity of home | 0.28 | Addition | Yes | YesA | 7 | 6.11 |
| Sub-209 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.05 | Subtraction | NA | NA | 7 | 6.11 |
| Add-212 | DELAWARE | Additional LOD determined to be available and acquired to allow safe installation | 0.80 | Addition | Yes | YesA | 7 | 6.11 |
| Sub-210 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.07 | Subtraction | NA | NA | 7 | 6.11 |
| Add-213 | DELAWARE | Temporary Access Road added to facilitate installation. No additional aquatic resources impacted. | 0.27 | Addition | Yes | YesA | 9 | 6.14 |
| Sub-211 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.05 | Subtraction | NA | NA | 9 | 6.14 |
| Add-214 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Addition | Yes | YesA | 10 | 6.16 |
| Add-215 | DELAWARE | Temporary Access Road added to facilitate installation. No additional aquatic resources impacted. | 0.27 | Addition | Yes | YesA | 10 | 6.16 |
| Add-216 | DELAWARE | HDD Entry/Exit workspace revision. No additional aquatic resource impacts. | 0.38 | Addition | Yes | YesA | 11 | 6.17 |
| Add-217 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.11 | Addition | Yes | YesA | 11 | 6.17 |
| Add-218 | DELAWARE | Lengthening of permanent access road for valve setting. | 0.51 | Addition | Yes | YesA | 11 | 6.17 |
| Sub-212 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Subtraction | NA | NA | 11 | 6.18 |
| Add-219 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.09 | Addition | Yes | YesA | 12 | 6.18 |
| Sub-213 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.02 | Subtraction | NA | NA | 12 | 6.18 |
| Sub-214 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.05 | Subtraction | NA | NA | 12 | 6.18 |
| Add-220 | DELAWARE | HDD workspace revision in this area. No additional aquatic resource impacts. | 0.45 | Addition | Yes | YesA | 12 | 6.18 |
| Sub-215 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.02 | Subtraction | NA | NA | 13 | 6.20 |
| Add-221 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.17 | Addition | Yes | YesA | 13 | 6.20 |
| Sub-216 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.04 | Subtraction | NA | NA | 13 | 6.20 |
| Add-222 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.18 | Addition | Yes | YesA | 13 |  |
| Sub-217 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.04 | Subtraction | NA | NA | 13 | 6.21 |
| Add-223 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Addition | Yes | YesA | 14 | 6.21 |
| Add-224 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.13 | Addition | Yes | YesA | 23 | 6.35 |
| Sub-218 | DELAWARE | Reduction of LOD as a result of a reroute to minimize impacts to wetlands | 0.53 | Subtraction | NA | NA | 23 | 6.20 |
| Add-225 | DELAWARE | Twin Oaks reroute - designed to reduce wetland impacts | 2.92 | Addition | Yes | YesA | 22 | 6.35 |
| Add-226 | DELAWARE | Temporary Access Road added to facilitate installation. No additional aquatic resources impacted. | 0.30 | Addition | Yes | YesA | 17 | 6.26 |
| Add-227 | DELAWARE | Twin Oaks reroute ATWS revised to reduce wetland impacts | 0.79 | Addition | Yes | YesA | 22 | 6.34 |
| Add-228 | DELAWARE | Tree clearing only LOD added to maximize aerial DOT inspections | 0.92 | Addition | Yes | YesA | 17 | 6.26 |
| Sub-219 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.67 | Subtraction | NA | NA | 16 | 6.25 |
| Add-229 | DELAWARE | Shift of LOD to southeast at request of landowner | 0.83 | Addition | Yes | YesA | 16 | 6.25 |
| Add-230 | DELAWARE | Tree clearing only LOD added to maximize aerial DOT inspections | 1.95 | Addition | Yes | YesA | 18 | 6.27 |
| Add-231 | DELAWARE | Tree clearing only LOD added to maximize aerial DOT inspections | 1.00 | Addition | Yes | YesA | 18 | 6.28 |
| Add-232 | DELAWARE | Travel lane perm ROW added on top of HDD to allow clearing and travel to HDD Entry/Exit. No additional impacts to aquatic resources. | 0.72 | Addition | Yes | YesA | 19 | 6.29 |
| Add-233 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.43 | Addition | Yes | YesA | 21 | 6.32 |
| Add-234 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.13 | Addition | Yes | YesA | 21 | 6.32 |
| Sub-220 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.05 | Subtraction | NA | NA | 21 | 6.32 |
| Add-235 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Addition | Yes | YesA | 19 | 6.29 |
| Add-236 | DELAWARE | Temporary Access Road added to facilitate installation. No additional aquatic resources impacted. | 0.32 | Addition | Yes | YesA | 20 | 6.31 |
| Sub-221 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Subtraction | NA | NA | 20 | 6.31 |
| Add-237 | DELAWARE | Tree clearing only LOD added to maximize aerial DOT inspections | 1.76 | Addition | Yes | YesA | 20 | 6.30 |
| Sub-222 | DELAWARE | Minor LOD adjustment needed to facilitate safe installation | 0.04 | Subtraction | NA | NA | 20 | 6.31 |

1 – The added area was field investigated for aquatic resources. Not applicable is listed for LOD subtractions.

2 – The added area was originally evaluated for PNDIA or PNDI was revisited through interim correspondence and analysisB. Not applicable is listed for LOD subtractions.