SPLP has had revisions to the proposed workspaces in Westmoreland County since submittal of the original application.  These revisions have been the result of landowner requests, agency requests, the avoidance of sensitive species or their habitats, and/or to further reduce impacts to aquatic resources.  The additions and subtractions to the workspaces are listed and quantified within Table 1.  In addition, this attachment highlights the location and extent of these additions and subtractions to the workspaces on a set of site plans.  Each addition/subtraction has been assigned an identification code and that code is reflected below and on the set of site plans.  The additions and subtractions are listed from west to east. A total of approximately 30.24 acres was added and 13.60 acres subtracted for a net increase of 16.64 acres of earth disturbance.

**Table 1.  Pennsylvania Pipeline Project LOD Additions and Subtractions.**

| **CHANGE ID** | **COUNTY** | **REASON FOR CHANGE** | **ACREAGE** | **LOD ADDITION OR SUBTRACTION** | **WETLAND DELINEATION1** | **PNDI EVALUATION2** | **SHEET NUMBER** | **E&S SHEET NUMBER** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Delmont Station | WESTMORELAND | Station design | 10.34 | Addition | Yes | YesA | 52 | 2.01 |
| Sub-33 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.01 | Subtraction | NA | NA | 2 | 1.73 |
| Sub-34 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.08 | Subtraction | NA | NA | 2 | 1.73 |
| Add-17 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.08 | Addition | Yes | YesA | 2 | 1.73 |
| Sub-35 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.05 | Subtraction | NA | NA | 2 | 1.72 |
| Add-18 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.05 | Addition | Yes | YesA | 2 | 1.72 |
| Sub-36 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.02 | Subtraction | NA | NA | 3 | 1.03 |
| Add-19 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.02 | Addition | Yes | YesA | 3 | 1.03 |
| Add-20 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Addition | Yes | YesA | 4 | 1.04 |
| Sub-37 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Subtraction | NA | NA | 7 | 1.10 |
| Add-21 | WESTMORELAND | Temporary Access Road added to facilitate installation. No additional aquatic resources impacted. | 0.56 | Addition | Yes | YesA | 10 | 1.13 |
| Sub-38 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.20 | Subtraction | NA | NA | 19 | 1.26 |
| Add-22 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.06 | Addition | Yes | YesA | 19 | 1.26 |
| Sub-39 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Subtraction | NA | NA | 19 | 1.26 |
| Sub-40 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.29 | Subtraction | NA | NA | 19 | 1.26 |
| Add-23 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Addition | Yes | YesA | 24 | 1.33 |
| Add-24 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.08 | Addition | Yes | YesA | 26 | 1.35 |
| Add-25 | WESTMORELAND | HDD Revision, no additional aquatic resource impacts. | 0.66 | Addition | Yes | YesA | 31 | 1.82 |
| Add-26 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.21 | Addition | Yes | YesA | 31 | 1.42 |
| Sub-41 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.14 | Subtraction | NA | NA | 31 | 1.42 |
| Add-27 | WESTMORELAND | HDD design revision in this area. No additional aquatic resource impacts. | 0.60 | Addition | Yes | YesA | 31 | 1.41 |
| Sub-42 | WESTMORELAND | HDD entry/exit redesigned to facilitate safe installation | 0.79 | Subtraction | NA | NA | 31 | 1.42 |
| Sub-43 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.01 | Subtraction | NA | NA | 32 | 1.43 |
| Sub-44 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.06 | Subtraction | NA | NA | 37 | 1.50 |
| Sub-45 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.07 | Subtraction | NA | NA | 37 | 1.50 |
| Sub-46 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.06 | Subtraction | NA | NA | 34 | 1.46 |
| Add-28 | WESTMORELAND | Change of crossing method from HDD to open cut due to access constraints. Wetland impacts increased in this area. | 0.68 | Addition | Yes | YesA | 41 | 1.55 |
| Add-29 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Addition | Yes | YesA | 47 | 1.62 |
| Sub-47 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.24 | Subtraction | NA | NA | 51 | 1.69 |
| Add-30 | WESTMORELAND | Temporary access road mapping shifted to west. No additional aquatic resource impacts. | 0.26 | Addition | Yes | YesA | 51 | 1.69 |
| Add-31 | WESTMORELAND | Travel through this area was determined to be required. No additional aquatic resource impacts. | 0.44 | Addition | Yes | YesA | 52 | 1.7 |
| Add-32 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Addition | Yes | YesA | 52 | 1.71 |
| Add-33 | WESTMORELAND | Delmont Pump Station related added LOD | 1.36 | Addition | Yes | YesA | 53 | 2.01 |
| Add-34 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.10 | Addition | Yes | YesA | 53 | 2.01 |
| Sub-48 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.01 | Subtraction | NA | NA | 53 | 2.01 |
| Add-35 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.14 | Addition | Yes | YesA | 54 | 2.02 |
| Add-36 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.21 | Addition | Yes | YesA | 54 | 2.04 |
| Sub-49 | WESTMORELAND | Minor reroute required in this area at landowners’ request. | 0.41 | Subtraction | NA | NA | 56 | 2.06 |
| Add-37 | WESTMORELAND | Minor ROW shift at request of landowner. No additional aquatic resource impacts. | 0.32 | Addition | Yes | YesA | 37 | 2.06 |
| Sub-50 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.01 | Subtraction | NA | NA | 65 | 2.21 |
| Sub-51 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.19 | Subtraction | NA | NA | 65 | 2.21 |
| Sub-52 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.17 | Subtraction | NA | NA | 65 | 2.21 |
| Add-38 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.05 | Addition | Yes | YesA | 65 | 2.21 |
| Sub-53 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.09 | Subtraction | NA | NA | 65 | 2.21 |
| Sub-54 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.01 | Subtraction | NA | NA | 65 | N/A |
| Add-39 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.11 | Addition | Yes | YesA | 65 | 2.21 |
| Add-40 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.06 | Addition | Yes | YesA | 65 | 2.21 |
| Sub-55 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Subtraction | NA | NA | 67 | 2.24 |
| Add-41 | WESTMORELAND | Valve setting and road crossing workspace revision. Additional workspaces determined to be available and helpful to allow safe installation. No additional aquatic resource impacts. | 0.19 | Addition | Yes | YesA | 67 | 2.24 |
| Sub-56 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Subtraction | NA | NA | 67 | 2.24 |
| Add-42 | WESTMORELAND | Valve setting and road crossing workspace revision. Additional workspaces determined to be available and helpful to allow safe installation. No additional aquatic resource impacts. | 0.57 | Addition | Yes | YesA | 67 | 2.24 |
| Add-43 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Addition | Yes | YesA | 67 | 2.25 |
| Sub-57 | WESTMORELAND | Block valve location adjustment, due to landowner request, overall LOD reduction. | 1.83 | Subtraction | NA | NA | 67 | 2.25 |
| Sub-58 | WESTMORELAND | Block valve location adjustment, due to landowner request, overall LOD reduction. | 0.56 | Subtraction | NA | NA | 67 | 2.25 |
| Add-44 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.14 | Addition | Yes | YesA | 70 | 2.29 |
| Add-45 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.14 | Addition | Yes | YesA | 72 | 2.32 |
| Add-46 | WESTMORELAND | Travel Lane determined to be needed along small section of HDD. No additional aquatic resource impacts. | 0.79 | Addition | Yes | YesA | 75 | 2.37 |
| Sub-59 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.02 | Subtraction | NA | NA | 78 | 2.42 |
| Add-47 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.16 | Addition | Yes | YesA | 79 | 2.43 |
| Add-48 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.10 | Addition | Yes | YesA | 79 | 2.43 |
| Add-49 | WESTMORELAND | Westinghouse Reroute - Required to avoid potential contaminated soils. This reroute significantly reduced crossing lengths of forested wetlands. | 3.70 | Addition | Yes | YesB | 79 | 2.43 |
| Sub-60 | WESTMORELAND | Reroute to avoid potentially contaminated soils. Reroute also significantly reduced impacts to wetlands. | 8.02 | Subtraction | NA | NA | 79 | 2.43 |
| Add-50 | WESTMORELAND | Westinghouse Reroute - Required to avoid potential contaminated soils. This reroute significantly reduced crossing lengths of forested wetlands. | 7.91 | Addition | Yes | YesA | 81 | 2.45 |
| Sub-61 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.02 | Subtraction | NA | NA | 82 | 2.47.01 |
| Sub-62 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.05 | Subtraction | NA | NA | 82 | 2.47.01 |
| Sub-63 | WESTMORELAND | Minor LOD adjustment needed to facilitate safe installation | 0.07 | Subtraction | NA | NA | 82 | 2.47.01 |

1 – The added area was field investigated for aquatic resources. Not applicable is listed for LOD subtractions.

2 – The added area was originally evaluated for PNDIA or PNDI was revisited through interim correspondence and analysisB. Not applicable is listed for LOD subtractions.