SPLP has made revisions to the proposed workspaces in Berks County since submittal of the original application.  These revisions have been the result of landowner requests, agency requests, the avoidance of sensitive species or their habitats, and/or to further reduce impacts to aquatic resources.  The additions and subtractions to the workspaces are listed and quantified within Table 1.  In addition, this attachment highlights the location and extent of these additions and subtractions to the workspaces on a set of site plans.  Each addition/subtraction has been assigned an identification code and that code is reflected below and on the set of site plans.  The additions and subtractions are listed from west to east. A total of approximately 16.31 acres was added and 1.51 acres subtracted for a net increase of 14.80 acres of earth disturbance.

**Table 1.  Pennsylvania Pipeline Project LOD Additions and Subtractions.**

| **CHANGE ID** | **COUNTY** | **REASON FOR CHANGE** | **ACREAGE** | **LOD ADDITION OR SUBTRACTION** | **WETLAND DELINEATION1** | **PNDI EVALUATION2** | **SHEET NUMBER** | **E&S SHEET NUMBER** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Beckersville Station | BERKS | Station design | 4.95 | Addition | Yes | YesA and B | 28 | 5.77 |
| Add-135 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.10 | Addition | Yes | YesA | 1 | 5.01 |
| Add-136 | BERKS | Additional workspace determined to be available and helpful to allow safe installation. No additional aquatic resource impacts. | 0.05 | Addition | Yes | YesA | 6 | 5.11 |
| Sub-153 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.28 | Subtraction | NA | NA | 6 | 5.12 |
| Add-137 | BERKS | Small 15-20 foot shift of the route to the south east in this section. No additional aquatic resource impacts. | 0.43 | Addition | Yes | YesA | 6 | 5.12 |
| Sub-154 | BERKS | Temporary workspace shifted to south side of perm workspace in this area. | 0.43 | Subtraction | NA | NA | 7 | 5.12 |
| Add-138 | BERKS | Small 15-20 foot shift of the route to the south east in this section. No additional aquatic resource impacts. | 0.75 | Addition | Yes | YesA | 7 | 5.12 |
| Add-139 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.04 | Addition | Yes | YesA | 8 | 5.15 |
| Add-140 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.06 | Addition | Yes | YesA | 8 | 5.15 |
| Sub-155 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.01 | Subtraction | NA | NA | 8 | 5.15 |
| Add-141 | BERKS | Added Montello pump station connection line routing. No additional impacts to aquatic resources. | 0.70 | Addition | Yes | YesA | 8 | 5.15 |
| Sub-156 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.01 | Subtraction | NA | NA | 8 | 5.15 |
| Add-142 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Addition | Yes | YesA | 8 | 5.15 |
| Add-143 | BERKS | Added permanent road. | 0.06 | Addition | Yes | YesA | 8 | 5.15 |
| Sub-157 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.04 | Subtraction | NA | NA | 8 | 5.15 |
| Add-144 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.04 | Addition | Yes | YesA | 8 | 5.15 |
| Sub-158 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.08 | Subtraction | NA | NA | 15 | 5.74 |
| Add-145 | BERKS | LOD Shift to Increase Accuracy of Access Road Mapping | 0.08 | Addition | Yes | YesA | 15 | 5.74 |
| Sub-159 | BERKS | Minor LOD adjustment to reduce wetland impacts | 0.01 | Subtraction | NA | NA | 15 | 5.74 |
| Sub-160 | BERKS | Minor LOD adjustment to reduce wetland impacts | 0.02 | Subtraction | NA | NA | 15 | 5.74 |
| Add-146 | BERKS | LOD Shift to Reduce Impacts to Wetlands | 0.02 | Addition | Yes | YesA | 15 | 5.74 |
| Sub-161 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.02 | Subtraction | NA | NA | 15 | 5.74 |
| Add-147 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.08 | Addition | Yes | YesA | 16 | 5.29 |
| Sub-162 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.01 | Subtraction | NA | NA | 17 | 5.30 |
| Sub-163 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.11 | Subtraction | NA | NA | 19 | 5.33 |
| Add-148 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.11 | Addition | Yes | YesA | 19 | 5.33 |
| Sub-163A | BERKS | Reroute to avoid potential bog turtle impacts | 0.41 | Subtraction | NA | NA | 20 | 5.35 |
| Add-149 | BERKS | Reroute to avoid potential bog turtle impacts | 3.36 | Addition | Yes | YesA | 20 | 5.35 |
| Add-150 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.12 | Addition | Yes | YesA | 26 | 5.44 |
| Sub-164 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.04 | Subtraction | NA | NA | 29 | 5.51 |
| Add-151 | BERKS | Additional workspace determined to be available and helpful to allow safe installation. No additional aquatic resource impacts. | 0.73 | Addition | Yes | YesA | 35 | 5.60 |
| Add-152 | BERKS | Additional workspace determined to be required to facilitate safe installation. | 3.40 | Addition | Yes | YesA | 35 | 5.60 |
| Sub-165 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.02 | Subtraction | NA | NA | 38 | 5.64 |
| Add-153 | BERKS | Additional workspace determined to be required to facilitate safe installation. No additional aquatic resource impacts. | 0.28 | Addition | Yes | YesA | 38 | 5.64 |
| Add-154 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.09 | Addition | Yes | YesA | 38 | 5.64 |
| Add-155 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.20 | Addition | Yes | YesA | 38 | 5.64 |
| Sub-166 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.02 | Subtraction | NA | NA | 38 | 5.64 |
| Add-156 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.16 | Addition | Yes | YesA | 39 | 5.65 |
| Add-157 | BERKS | Additional workspace determined to be required to facilitate safe installation. No additional aquatic resource impacts. | 0.44 | Addition | Yes | YesA | 38 | 5.64 |
| Add-158 | BERKS | Minor LOD adjustment needed to facilitate safe installation | 0.03 | Addition | Yes | YesA | 40 | 5.67 |

1 – The added area was field investigated for aquatic resources. Not applicable is listed for LOD subtractions.

2 – The added area was originally evaluated for PNDIA or PNDI was revisited through interim correspondence and analysisB. Not applicable is listed for LOD subtractions.