{"text_format":"1","workbook":"xlsx","n_sheets":57,"sheets":["Instructions","Inputs","Results","Site-Specific Data","Versions","WQN0100","WQN0178","WQN0181","WQN0183","WQN0191","WQN0195","WQN0196","WQN0197","WQN0199","WQN0275","WQN0276","WQN0279","WQN0290","WQN0291","WQN0292","WQN0294","WQN0296","WQN0297","WQN0409","WQN0411","WQN0428","WQN0443","WQN0452","WQN0453","WQN0454","WQN0455","WQN0456","WQN0457","WQN0458","WQN0459","WQN0463","WQN0464","WQN0465","WQN0466","WQN0500","WQN0514","WQN0626","WQN0627","WQN0628","WQN0629","WQN0630","WQN0634","WQN0723","WQN0724","WQN0733","WQN0734","WQN0735","WQN0870","WQN0873","WQN0877","WQN0879","WQN0885"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":5,"defined_names":178,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":19,"n_cols":2,"rows_kept":19,"cut":false,"hidden":false,"merged":[[12,1,12,30],[7,1,8,29],[14,1,14,29],[6,1,6,30],[0,1,0,30],[1,1,1,30],[5,1,5,30],[10,1,10,19],[10,20,10,23]]}
[null,"Anti-degradation Limits Spreadsheet"]
[null,"Version 1.0, April 2024"]
[]
[]
[]
[]
[]
[null,"If prompted by Excel after opening the DEP Anti-degradation Limits Spreadsheet, enable editing and macros.  This spreadsheet consists of three hyperlink tabs: Instructions, Inputs and Results.  Each tab has a corresponding worksheet."]
[]
[]
[null,"Only those cells that are highlighted are available for data entry by the user:"]
[]
[null,"Red asterisks (*) are shown where cells may not be blank in order to calculate effluent limitations."]
[]
[null,"Click on the button below to open detailed instructions on the use of the Non-degrading Limits Spreadsheet:"]
[]
[]
[]
[null,"If you have questions concerning use of this spreadsheet, contact the Bureau of Clean Water at 717-787-5017."]

{"sheet":"Inputs","index":1,"n_rows":217,"n_cols":64,"rows_kept":217,"cut":false,"hidden":false,"merged":[[144,25,144,27],[145,9,145,13],[133,9,133,13],[133,14,133,16],[132,14,132,16],[132,17,132,20],[118,11,118,15],[119,11,119,15],[119,16,119,18],[122,23,122,25],[127,21,129,24],[124,23,124,25],[125,23,125,25],[120,23,120,25],[122,19,122,22],[121,16,121,18],[122,16,122,18],[120,16,120,18],[137,14,137,16],[140,14,140,16],[140,17,140,20],[140,25,140,27],[141,9,141,13],[123,19,123,22],[124,19,124,22],[125,19,125,22],[123,11,123,15],[124,11,124,15],[125,11,125,15],[134,9,134,13],[133,25,133,27],[132,21,132,24],[7,23,7,27],[150,40,150,42],[150,43,150,45],[150,46,150,49],[148,21,148,24],[148,25,148,27],[149,9,149,13],[149,14,149,16],[149,17,149,20],[149,21,149,24],[149,25,149,27],[150,9,150,13],[150,14,150,16],[150,17,150,20],[150,21,150,24],[150,25,150,27],[115,40,115,42],[115,43,115,45],[115,46,115,49],[96,16,96,18],[97,16,97,18],[48,40,48,42],[48,43,48,45],[48,46,48,49],[36,40,36,42],[36,43,36,45],[36,46,36,49],[37,40,37,42],[37,43,37,45],[37,46,37,49],[38,40,38,42],[38,43,38,45],[143,9,143,13],[143,14,143,16],[143,17,143,20],[143,21,143,24],[143,25,143,27],[90,11,90,16],[90,17,90,19],[90,20,90,21],[99,40,99,42],[100,40,100,42],[101,40,101,42],[102,40,102,42],[99,43,99,45],[108,55,108,58],[109,55,109,58],[93,59,95,62],[96,59,96,62],[97,59,97,62],[132,9,132,13],[117,23,117,25],[91,56,91,58],[91,59,91,62],[93,11,95,15],[93,19,95,22],[96,11,96,15],[106,23,106,25],[96,19,96,22],[98,59,98,62],[99,59,99,62],[100,59,100,62],[107,59,107,62],[103,16,103,18],[104,16,104,18],[110,59,110,62],[111,55,111,58],[111,59,111,62],[112,59,112,62],[113,40,113,42],[113,43,113,45],[113,46,113,49],[112,11,112,15],[112,16,112,18],[112,19,112,22],[112,23,112,25],[114,11,114,15],[114,16,114,18],[114,19,114,22],[114,23,114,25],[115,11,115,15],[115,16,115,18],[115,19,115,22],[115,23,115,25],[111,16,111,18],[111,19,111,22],[111,23,111,25],[113,11,113,15],[108,40,108,42],[115,59,115,62],[112,52,112,54],[114,52,114,54],[111,46,111,49],[111,40,111,42],[110,43,110,45],[110,40,110,42],[100,11,100,15],[109,11,109,15],[107,11,107,15],[110,11,110,15],[110,16,110,18],[87,63,87,66],[88,59,88,62],[88,63,88,66],[89,63,89,66],[90,40,90,42],[90,43,90,45],[90,46,90,49],[90,50,90,53],[90,54,90,55],[90,56,90,58],[90,59,90,62],[90,63,90,66],[89,43,89,45],[89,40,89,42],[91,63,91,66],[107,16,107,18],[108,16,108,18],[101,23,101,25],[103,19,103,22],[106,19,106,22],[107,19,107,22],[109,16,109,18],[106,11,106,15],[91,43,91,45],[91,46,91,49],[91,50,91,53],[91,54,91,55],[44,13,44,18],[52,55,52,58],[53,13,53,18],[53,19,53,21],[53,22,53,23],[53,40,53,42],[53,43,53,45],[53,55,53,58],[52,40,52,42],[52,43,52,45],[50,55,50,58],[51,50,51,51],[51,52,51,54],[87,56,87,58],[87,59,87,62],[88,56,88,58],[89,46,89,49],[89,50,89,53],[89,54,89,55],[89,56,89,58],[89,59,89,62],[79,20,79,21],[80,20,80,21],[81,20,81,21],[77,20,77,21],[72,17,72,19],[72,22,72,25],[84,59,84,62],[47,52,47,54],[48,52,48,54],[50,43,50,45],[47,50,47,51],[84,63,84,66],[85,46,85,49],[85,50,85,53],[85,54,85,55],[85,56,85,58],[85,59,85,62],[85,63,85,66],[86,54,86,55],[86,56,86,58],[86,59,86,62],[86,63,86,66],[45,46,45,49],[46,19,46,21],[25,22,27,23],[28,22,28,23],[29,22,29,23],[30,22,30,23],[31,22,31,23],[32,22,32,23],[33,22,33,23],[34,22,34,23],[35,22,35,23],[36,22,36,23],[37,22,37,23],[38,22,38,23],[39,22,39,23],[40,22,40,23],[41,22,41,23],[42,22,42,23],[43,22,43,23],[43,55,43,58],[48,50,48,51],[26,52,27,54],[28,52,28,54],[29,13,29,18],[30,13,30,18],[31,13,31,18],[32,13,32,18],[33,13,33,18],[59,20,61,21],[62,20,62,21],[63,20,63,21],[44,55,44,58],[45,55,45,58],[46,55,46,58],[47,55,47,58],[48,55,48,58],[49,40,49,42],[49,43,49,45],[49,46,49,49],[49,50,49,51],[49,52,49,54],[49,55,49,58],[59,11,61,16],[62,11,62,16],[63,11,63,16],[29,52,29,54],[30,52,30,54],[31,52,31,54],[32,52,32,54],[33,52,33,54],[34,52,34,54],[26,55,27,58],[28,55,28,58],[29,55,29,58],[30,55,30,58],[31,55,31,58],[32,55,32,58],[33,55,33,58],[34,55,34,58],[35,55,35,58],[36,55,36,58],[37,55,37,58],[38,55,38,58],[39,55,39,58],[40,55,40,58],[41,55,41,58],[42,55,42,58],[35,52,35,54],[36,52,36,54],[37,52,37,54],[38,52,38,54],[39,52,39,54],[40,52,40,54],[41,52,41,54],[42,52,42,54],[38,13,38,18],[39,13,39,18],[40,13,40,18],[45,50,45,51],[42,50,42,51],[43,50,43,51],[44,50,44,51],[26,40,27,42],[26,43,27,45],[26,46,27,49],[46,40,46,42],[46,43,46,45],[46,46,46,49],[47,40,47,42],[26,50,27,51],[28,50,28,51],[29,50,29,51],[30,50,30,51],[31,50,31,51],[32,50,32,51],[33,50,33,51],[34,50,34,51],[35,50,35,51],[36,50,36,51],[37,50,37,51],[38,50,38,51],[39,50,39,51],[46,50,46,51],[40,50,40,51],[45,40,45,42],[45,43,45,45],[28,46,28,49],[44,40,44,42],[41,50,41,51],[38,46,38,49],[39,40,39,42],[39,43,39,45],[39,46,39,49],[40,40,40,42],[40,43,40,45],[43,52,43,54],[44,52,44,54],[45,52,45,54],[38,19,38,21],[39,19,39,21],[40,19,40,21],[46,52,46,54],[44,22,44,23],[45,22,45,23],[43,40,43,42],[43,43,43,45],[43,46,43,49],[44,43,44,45],[44,46,44,49],[29,43,29,45],[29,46,29,49],[30,40,30,42],[30,43,30,45],[30,46,30,49],[31,40,31,42],[31,43,31,45],[31,46,31,49],[32,40,32,42],[32,43,32,45],[32,46,32,49],[33,40,33,42],[42,40,42,42],[42,43,42,45],[42,46,42,49],[29,19,29,21],[30,19,30,21],[29,40,29,42],[35,43,35,45],[51,55,51,58],[32,19,32,21],[33,19,33,21],[34,19,34,21],[34,13,34,18],[50,50,50,51],[50,52,50,54],[35,19,35,21],[36,19,36,21],[37,19,37,21],[35,13,35,18],[36,13,36,18],[37,13,37,18],[51,46,51,49],[50,13,50,18],[50,19,50,21],[51,13,51,18],[33,43,33,45],[33,46,33,49],[34,40,34,42],[34,43,34,45],[34,46,34,49],[35,40,35,42],[35,46,35,49],[44,19,44,21],[45,19,45,21],[40,46,40,49],[41,40,41,42],[41,43,41,45],[41,46,41,49],[51,40,51,42],[51,43,51,45],[60,54,61,55],[62,54,62,55],[28,40,28,42],[28,43,28,45],[9,26,9,35],[9,2,9,6],[9,7,9,19],[25,19,27,21],[56,13,56,18],[56,19,56,21],[56,22,56,23],[11,29,11,31],[20,13,20,19],[21,13,21,19],[7,2,7,3],[7,5,7,16],[54,13,54,18],[54,19,54,21],[54,22,54,23],[55,13,55,18],[55,19,55,21],[55,22,55,23],[9,21,9,24],[22,13,22,19],[41,19,41,21],[42,19,42,21],[43,19,43,21],[41,13,41,18],[42,13,42,18],[43,13,43,18],[25,13,27,18],[22,20,22,23],[15,13,15,23],[58,20,58,21],[53,46,53,49],[53,50,53,51],[53,52,53,54],[54,40,54,42],[54,43,54,45],[54,46,54,49],[54,50,54,51],[56,50,56,51],[56,52,56,54],[52,46,52,49],[52,50,52,51],[52,52,52,54],[47,19,47,21],[48,19,48,21],[49,19,49,21],[47,13,47,18],[48,13,48,18],[49,13,49,18],[50,22,50,23],[47,22,47,23],[48,22,48,23],[50,40,50,42],[50,46,50,49],[20,20,20,23],[21,20,21,23],[47,43,47,45],[47,46,47,49],[31,19,31,21],[45,13,45,18],[46,13,46,18],[63,17,63,19],[77,22,77,25],[74,17,74,19],[19,20,19,23],[11,7,11,19],[16,13,16,19],[17,13,17,19],[18,13,18,19],[19,13,19,19],[13,6,13,13],[16,20,16,23],[17,20,17,23],[18,20,18,23],[57,22,57,23],[64,11,64,16],[65,11,65,16],[66,11,66,16],[64,20,64,21],[65,20,65,21],[51,19,51,21],[66,20,66,21],[52,13,52,18],[52,19,52,21],[46,22,46,23],[28,13,28,18],[73,20,73,21],[72,20,72,21],[65,17,65,19],[65,22,65,25],[57,13,57,18],[57,19,57,21],[24,22,24,23],[78,17,78,19],[78,22,78,25],[105,16,105,18],[28,19,28,21],[93,23,95,25],[66,22,66,25],[67,17,67,19],[67,22,67,25],[49,22,49,23],[51,22,51,23],[52,22,52,23],[77,11,77,16],[78,11,78,16],[79,11,79,16],[80,11,80,16],[81,11,81,16],[93,16,95,18],[64,22,64,25],[74,11,74,16],[75,11,75,16],[59,17,61,19],[59,22,61,25],[62,17,62,19],[74,22,74,25],[75,17,75,19],[75,22,75,25],[74,20,74,21],[75,20,75,21],[76,20,76,21],[73,22,73,25],[76,17,76,19],[62,22,62,25],[84,56,84,58],[64,17,64,19],[100,16,100,18],[101,16,101,18],[102,16,102,18],[101,11,101,15],[66,17,66,19],[89,11,89,16],[89,17,89,19],[73,11,73,16],[67,11,67,16],[68,11,68,16],[69,11,69,16],[70,11,70,16],[71,11,71,16],[72,11,72,16],[76,11,76,16],[81,17,81,19],[84,11,84,16],[97,11,97,15],[98,11,98,15],[99,11,99,15],[73,17,73,19],[102,19,102,22],[102,11,102,15],[90,22,90,25],[91,11,91,16],[91,17,91,19],[91,20,91,21],[91,22,91,25],[82,11,82,16],[83,11,83,16],[54,55,54,58],[55,40,55,42],[55,43,55,45],[55,46,55,49],[55,50,55,51],[70,17,70,19],[70,22,70,25],[55,52,55,54],[55,55,55,58],[56,40,56,42],[84,17,84,19],[68,17,68,19],[68,22,68,25],[69,17,69,19],[69,22,69,25],[54,52,54,54],[71,17,71,19],[71,22,71,25],[56,43,56,45],[56,46,56,49],[82,20,82,21],[83,20,83,21],[67,20,67,21],[68,20,68,21],[69,20,69,21],[70,20,70,21],[71,20,71,21],[84,46,84,49],[74,50,74,53],[75,50,75,53],[76,50,76,53],[78,50,78,53],[82,22,82,25],[121,23,121,25],[86,22,86,25],[87,17,87,19],[79,17,79,19],[79,22,79,25],[76,22,76,25],[85,20,85,21],[85,22,85,25],[86,17,86,19],[86,20,86,21],[83,17,83,19],[83,22,83,25],[77,17,77,19],[80,17,80,19],[80,22,80,25],[84,20,84,21],[84,22,84,25],[85,17,85,19],[118,23,118,25],[119,23,119,25],[92,23,92,25],[98,16,98,18],[116,16,116,18],[116,19,116,22],[108,19,108,22],[106,16,106,18],[81,22,81,25],[82,17,82,19],[89,20,89,21],[89,22,89,25],[78,20,78,21],[116,11,116,15],[111,11,111,15],[102,23,102,25],[103,23,103,25],[104,23,104,25],[107,23,107,25],[108,23,108,25],[109,23,109,25],[99,16,99,18],[108,11,108,15],[134,14,134,16],[134,17,134,20],[134,25,134,27],[120,19,120,22],[123,16,123,18],[124,16,124,18],[125,16,125,18],[127,25,129,27],[110,23,110,25],[113,23,113,25],[113,16,113,18],[122,11,122,15],[117,11,117,15],[117,16,117,18],[117,19,117,22],[104,19,104,22],[105,19,105,22],[120,11,120,15],[121,11,121,15],[103,11,103,15],[104,11,104,15],[105,11,105,15],[135,9,135,13],[135,14,135,16],[135,17,135,20],[135,25,135,27],[134,21,134,24],[130,9,130,13],[132,25,132,27],[126,25,126,27],[130,14,130,16],[130,17,130,20],[130,25,130,27],[131,9,131,13],[131,14,131,16],[131,17,131,20],[131,25,131,27],[130,21,130,24],[131,21,131,24],[127,9,129,13],[127,14,129,16],[127,17,129,20],[138,9,138,13],[138,14,138,16],[138,17,138,20],[138,25,138,27],[154,9,154,13],[154,14,154,16],[154,17,154,20],[154,25,154,27],[118,16,118,18],[110,19,110,22],[113,19,113,22],[148,9,148,13],[148,14,148,16],[148,17,148,20],[139,9,139,13],[139,14,139,16],[139,17,139,20],[139,25,139,27],[138,21,138,24],[135,21,135,24],[136,9,136,13],[136,14,136,16],[136,17,136,20],[136,25,136,27],[137,9,137,13],[154,21,154,24],[137,17,137,20],[137,25,137,27],[121,19,121,22],[144,17,144,20],[142,9,142,13],[142,14,142,16],[142,17,142,20],[142,25,142,27],[142,21,142,24],[139,21,139,24],[140,9,140,13],[152,9,152,13],[152,14,152,16],[152,17,152,20],[152,25,152,27],[153,9,153,13],[153,14,153,16],[153,17,153,20],[153,25,153,27],[152,21,152,24],[151,9,151,13],[151,14,151,16],[151,17,151,20],[151,25,151,27],[141,14,141,16],[141,17,141,20],[141,25,141,27],[145,14,145,16],[145,17,145,20],[145,21,145,24],[145,25,145,27],[146,9,146,13],[146,14,146,16],[146,17,146,20],[146,21,146,24],[140,21,140,24],[147,9,147,13],[147,14,147,16],[147,17,147,20],[147,21,147,24],[147,25,147,27],[144,9,144,13],[144,14,144,16],[158,9,158,13],[158,14,158,16],[158,17,158,20],[158,25,158,27],[159,9,159,13],[159,14,159,16],[159,17,159,20],[159,25,159,27],[158,21,158,24],[155,21,155,24],[156,9,156,13],[156,14,156,16],[156,17,156,20],[156,25,156,27],[157,9,157,13],[157,14,157,16],[157,17,157,20],[157,25,157,27],[156,21,156,24],[155,9,155,13],[155,14,155,16],[155,17,155,20],[155,25,155,27],[159,21,159,24],[144,21,144,24],[157,21,157,24],[153,21,153,24],[141,21,141,24],[137,21,137,24],[133,21,133,24],[63,22,63,25],[104,40,104,42],[105,40,105,42],[106,40,106,42],[107,40,107,42],[103,40,103,42],[109,19,109,22],[118,19,118,22],[119,19,119,22],[123,23,123,25],[96,23,96,25],[151,21,151,24],[97,23,97,25],[98,23,98,25],[99,23,99,25],[100,23,100,25],[105,23,105,25],[91,40,91,42],[116,23,116,25],[97,19,97,22],[98,19,98,22],[99,19,99,22],[100,19,100,22],[101,19,101,22],[146,25,146,27],[136,21,136,24],[133,17,133,20],[78,40,78,42],[79,40,79,42],[86,50,86,53],[88,43,88,45],[88,46,88,49],[88,50,88,53],[88,54,88,55],[82,40,82,42],[83,40,83,42],[87,40,87,42],[80,50,80,53],[81,50,81,53],[82,50,82,53],[83,54,83,55],[85,40,85,42],[86,40,86,42],[88,40,88,42],[87,43,87,45],[87,46,87,49],[87,50,87,53],[87,54,87,55],[84,50,84,53],[84,54,84,55],[84,40,84,42],[86,43,86,45],[86,46,86,49],[80,40,80,42],[83,50,83,53],[64,40,64,42],[65,40,65,42],[66,43,66,45],[66,46,66,49],[60,50,61,53],[62,50,62,53],[63,50,63,53],[64,50,64,53],[65,50,65,53],[66,50,66,53],[67,50,67,53],[68,50,68,53],[69,50,69,53],[70,50,70,53],[71,50,71,53],[72,50,72,53],[73,50,73,53],[63,43,63,45],[67,46,67,49],[68,46,68,49],[69,46,69,49],[70,46,70,49],[71,46,71,49],[72,46,72,49],[73,46,73,49],[66,40,66,42],[70,40,70,42],[71,40,71,42],[72,40,72,42],[73,40,73,42],[78,54,78,55],[79,54,79,55],[80,54,80,55],[81,54,81,55],[82,54,82,55],[85,43,85,45],[63,54,63,55],[64,54,64,55],[65,54,65,55],[66,54,66,55],[67,54,67,55],[68,54,68,55],[69,54,69,55],[70,54,70,55],[71,54,71,55],[72,54,72,55],[73,54,73,55],[74,54,74,55],[75,54,75,55],[76,54,76,55],[77,54,77,55],[84,43,84,45],[78,43,78,45],[76,43,76,45],[78,46,78,49],[79,50,79,53],[74,43,74,45],[75,43,75,45],[77,50,77,53],[74,46,74,49],[75,46,75,49],[76,46,76,49],[124,43,124,45],[93,40,95,42],[93,43,95,45],[93,46,95,49],[96,46,96,49],[97,46,97,49],[98,46,98,49],[96,43,96,45],[96,40,96,42],[97,40,97,42],[98,40,98,42],[107,43,107,45],[108,43,108,45],[74,40,74,42],[75,40,75,42],[67,40,67,42],[68,40,68,42],[69,40,69,42],[76,40,76,42],[100,43,100,45],[97,43,97,45],[98,43,98,45],[79,46,79,49],[80,46,80,49],[81,46,81,49],[82,46,82,49],[83,46,83,49],[108,46,108,49],[81,40,81,42],[77,46,77,49],[77,40,77,42],[126,52,126,54],[127,53,127,55],[130,52,130,54],[125,43,125,45],[130,55,130,58],[147,40,147,42],[147,43,147,45],[147,46,147,49],[146,40,146,42],[148,40,148,42],[148,43,148,45],[148,46,148,49],[149,40,149,42],[149,43,149,45],[131,43,131,45],[132,43,132,45],[130,46,130,49],[141,52,141,54],[142,52,142,54],[138,40,138,42],[126,43,126,45],[125,40,125,42],[126,40,126,42],[138,43,138,45],[128,50,129,51],[130,50,130,51],[131,50,131,51],[128,40,129,42],[128,43,129,45],[131,46,131,49],[132,46,132,49],[133,46,133,49],[99,52,99,54],[116,52,116,54],[111,52,111,54],[153,52,153,54],[136,55,136,58],[137,55,137,58],[130,43,130,45],[136,46,136,49],[132,50,132,51],[132,55,132,58],[139,50,139,51],[140,50,140,51],[145,50,145,51],[151,50,151,51],[134,52,134,54],[135,52,135,54],[136,52,136,54],[151,52,151,54],[152,50,152,51],[122,52,122,54],[123,52,123,54],[124,52,124,54],[125,52,125,54],[133,43,133,45],[149,50,149,51],[134,46,134,49],[138,50,138,51],[121,52,121,54],[107,52,107,54],[101,52,101,54],[102,52,102,54],[103,52,103,54],[65,56,65,58],[66,56,66,58],[85,11,85,16],[86,11,86,16],[87,11,87,16],[87,20,87,21],[87,22,87,25],[88,11,88,16],[88,17,88,19],[88,20,88,21],[88,22,88,25],[122,50,122,51],[123,50,123,51],[124,50,124,51],[125,50,125,51],[117,50,117,51],[117,52,117,54],[113,50,113,51],[113,52,113,54],[93,52,95,54],[96,52,96,54],[97,52,97,54],[98,52,98,54],[109,43,109,45],[109,40,109,42],[118,43,118,45],[119,43,119,45],[122,46,122,49],[123,46,123,49],[124,46,124,49]],"merged_total":1407,"flags":["merged_cut"]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Instructions!B1","v":"Anti-degradation Limits Spreadsheet"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Instructions!B2","v":"Version 1.0, April 2024"},null,null,null,{"$f":"IF(AND(AA10=\"New Direct to SP Waters\",Data_Source<>\"\",OR(U17<>\"\",U18<>\"\"),U21<>\"\",No_Samples<>\"\",N29<>\"\"),\"Y\",IF(AND(AA10=\"New Upstream of SP Waters\",Data_Source<>\"\",OR(U17<>\"\",U18<>\"\"),OR(U19<>\"\",U20<>\"\")*U21<>\"\",No_Samples<>\"\",L63<>\"\"),\"Y\",IF(AND(AA10=\"Expanding Direct to SP Waters\",Data_Source<>\"\",OR(U17<>\"\",U18<>\"\"),U21<>\"\",U22<>\"\",No_Samples<>\"\",L97<>\"\"),\"Y\",IF(AND(AA10=\"Expanding Upstream of SP Waters\",Data_Source<>\"\",OR(U17<>\"\",U18<>\"\"),OR(U19<>\"\",U20<>\"\"),U21<>\"\",U22<>\"\",No_Samples<>\"\",J131<>\"\"),\"Y\",\"\"))))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Parameters",null,null,null,{"$f":"IF(AND(AA10=\"New Direct to SP Waters\",N29<>\"\"),COUNT(BD29:BG58),IF(AND(AA10=\"New Upstream of SP Waters\",L63<>\"\"),COUNT(BL63:BO92),IF(AND(AA10=\"Expanding Direct to SP Waters\",L97<>\"\"),COUNT(BH97:BK126),IF(AND(AA10=\"Expanding Upstream of SP Waters\",J131<>\"\"),COUNT(BH131:BK160),\"\"))))","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Evaluation Type",null,null,null,null,null,null,"No.Samples"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"New Direct to SP Waters",null,null,null,null,null,null,4]
[null,null,"Facility:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NPDES Permit No.",null,null,null,null,null,null,null,null,null,null,"Outfall No.:",null,null,null,null,null,null,null,null,null,"New Upstream of SP Waters",null,null,null,null,null,null,8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Expanding Direct to SP Waters",null,null,null,null,null,null,12]
[null,null,"Receiving Stream:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Evaluation Type*:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Expanding Upstream of SP Waters",null,null,null,null,null,null,20]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30]
[null,null,"SP Stream:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Distance from Discharge (mi) :"]
[]
[null,null,"Data Source*:"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Stream and Discharge Characteristics"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Q7-10 of Receiving Stream (cfs)*:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Qh of Receiving Stream (cfs):",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Qh_Stream",null,null,null,null,{"$f":"IF(U18=\"\",POWER(U17, 0.874) * 7.43,U18)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Q7-10 of SP Waters (cfs)*:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Qh of SP Waters (cfs):",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Qh_SP",null,null,null,null,{"$f":"IF(U20=\"\",POWER(U19, 0.874) * 7.43,U20)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Discharge Flow (MGD)*:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Disch Flow CFS",null,null,null,null,{"$f":"U21*1.547","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Discharge Flow (MGD)*:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Exp Flow CFS",null,null,null,null,{"$f":"U22*1.547","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"No. of Samples*:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Qh Stream + Disc",null,null,null,null,{"$f":"Qh_Stream+Disc_Flow_CFS","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Qh Stream + Exp",null,null,null,null,{"$f":"Qh_Stream+Exp_Flow_CFS","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Total for Load",null,null,null,null,{"$f":"U21+U22","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Parameter*",null,null,null,null,null,"Units",null,null,"CV       (0.5 if left blank)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SP Upstream Conc",null,null,"HQ WQ Objective ",null,null,"LTA",null,null,null,"CV",null,"AML Multiplier",null,null,"Non-Degreading AML"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N29=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N29,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N29,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N29,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N29=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N29,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N29,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N29=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N29,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N29,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,{"$f":"IF(Qh_Stream=\"\",\"\",IF(Q_Total=\"\",\"\",IF(AR29=\"\",\"\",IF(AO29=\"\",\"\",((Q_Total*AR29)-(Qh_Stream*AO29))/Disc_Flow_CFS))))","v":""},null,null,null,{"$f":"IF(W29<>\"\",W29,0.5)","v":0.5},null,{"$f":"EXP((2.326*(LN(AY29^2/No_Samples+1))^0.5)-(0.5*LN(AY29^2/No_Samples+1)))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"AU29*BA29","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N30=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N30,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N30,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N30,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N30=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N30,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N30,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N30=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N30,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N30,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,{"$f":"IF(Qh_Stream=\"\",\"\",IF(Q_Total=\"\",\"\",IF(AR30=\"\",\"\",IF(AO30=\"\",\"\",((Q_Total*AR30)-(Qh_Stream*AO30))/Disc_Flow_CFS))))","v":""},null,null,null,{"$f":"IF(W30<>\"\",W30,0.5)","v":0.5},null,{"$error":"#DIV/0!"},null,null,{"$f":"AU30*BA30","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N31=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N31,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N31,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N31,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N31=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N31,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N31,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N31=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N31,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N31,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,{"$f":"IF(Qh_Stream=\"\",\"\",IF(Q_Total=\"\",\"\",IF(AR31=\"\",\"\",IF(AO31=\"\",\"\",((Q_Total*AR31)-(Qh_Stream*AO31))/Disc_Flow_CFS))))","v":""},null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N32=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N32,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N32,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N32,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N32=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N32,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N32,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N32=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N32,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N32,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N33=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N33,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N33,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N33,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N33=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N33,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N33,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N33=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N33,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N33,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N34=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N34,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N34,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N34,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N34=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N34,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N34,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N34=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N34,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N34,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N35=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N35,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N35,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N35,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N35=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N35,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N35,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N35=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N35,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N35,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N36=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N36,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N36,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N36,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N36=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N36,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N36,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N36=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N36,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N36,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N37=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N37,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N37,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N37,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N37=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N37,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N37,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N37=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N37,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N37,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N38=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N38,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N38,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N38,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N38=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N38,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N38,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N38=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N38,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N38,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N39=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N39,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N39,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N39,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N39=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N39,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N39,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N39=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N39,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N39,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N40=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N40,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N40,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N40,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N40=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N40,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N40,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N40=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N40,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N40,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N41=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N41,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N41,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N41,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N41=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N41,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N41,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N41=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N41,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N41,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N42=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N42,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N42,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N42,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N42=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N42,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N42,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N42=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N42,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N42,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N43=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N43,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N43,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N43,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N43=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N43,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N43,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N43=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N43,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N43,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N44=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N44,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N44,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N44,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N44=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N44,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N44,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N44=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N44,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N44,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N45=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N45,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N45,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N45,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N45=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N45,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N45,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N45=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N45,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N45,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N46=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N46,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N46,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N46,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null," ",null,null,null,null,null,null,null,{"$f":"IF(N46=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N46,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N46,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N46=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N46,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N46,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N47=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N47,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N47,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N47,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N47=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N47,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N47,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N47=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N47,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N47,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N48=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N48,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N48,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N48,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N48=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N48,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N48,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N48=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N48,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N48,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N49=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N49,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N49,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N49,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N49=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N49,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N49,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N49=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N49,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N49,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N50=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N50,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N50,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N50,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N50=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N50,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N50,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N50=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N50,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N50,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,{"$f":"IF(Qh_Stream=\"\",\"\",IF(Q_Total=\"\",\"\",IF(AR50=\"\",\"\",IF(AO50=\"\",\"\",((Q_Total*AR50)-(Qh_Stream*AO50))/Disc_Flow_CFS))))","v":""},null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$f":"AU50*BA50","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N51=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N51,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N51,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N51,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N51=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N51,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N51,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N51=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N51,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N51,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N52=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N52,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N52,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N52,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N52=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N52,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N52,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N52=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N52,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N52,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N53=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N53,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N53,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N53,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N53=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N53,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N53,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N53=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N53,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N53,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N54=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N54,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N54,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N54,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N54=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N54,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N54,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N54=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N54,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N54,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N55=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N55,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N55,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N55,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N55=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N55,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N55,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N55=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N55,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N55,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,{"$f":"IF(W55<>\"\",W55,0.5)","v":0.5},null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N56=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N56,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N56,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N56,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N56=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N56,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N56,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N56=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N56,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N56,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N57=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N57,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N57,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N57,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N57=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N57,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N57,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N57=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N57,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N57,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N58=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(N58,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(N58,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(N58,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(N58=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N58,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(N58,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(N58=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(N58,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(N58,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Parameter*",null,null,null,null,null,"Units",null,null,"CV     (0.5 if left blank)",null,"Upstream Concentration"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SP Upstream Conc",null,null,"HQ WQ Objective ",null,null,"Non-Degrading LTA Direct Disc",null,null,null,"Non-Degrading LTA Upstream",null,null,null,"CV",null,"AML Mulitplier",null,null,"Non-Degrading AML Direct Disc",null,null,null,"Non-Degrading AML Upstream"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L63=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L63,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L63,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L63,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L63=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L63,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L63,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L63=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L63,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L63,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,{"$f":"IF(Qh_Stream=\"\",\"\",IF(Q_Total=\"\",\"\",IF(AR63=\"\",\"\",IF(AO63=\"\",\"\",((Q_Total*AR63)-(Qh_Stream*AO63))/Disc_Flow_CFS))))","v":""},null,null,null,{"$f":"IF(Qh_Stream=\"\",\"\",IF(Q_Total=\"\",\"\",IF(AR63=\"\",\"\",IF(AO63=\"\",\"\",AR63+((Qh_Stream*(AR63-W63)+Qh_SP*(AR63-AO63))/Disc_Flow_CFS)))))","v":""},null,null,null,{"$f":"IF(U63<\"\",U63,0.5)","v":0.5},null,{"$f":"EXP((2.326*(LN(BC63^2/No_Samples+1))^0.5)-(0.5*LN(BC63^2/No_Samples+1)))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"AU63*BE63","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"AY63*BE63","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L64=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L64,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L64,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L64,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L64=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L64,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L64,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L64=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L64,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L64,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,{"$f":"IF(Qh_Stream=\"\",\"\",IF(Q_Total=\"\",\"\",IF(AR64=\"\",\"\",IF(AO64=\"\",\"\",((Q_Total*AR64)-(Qh_Stream*AO64))/Disc_Flow_CFS))))","v":""},null,null,null,{"$f":"IF(Qh_Stream=\"\",\"\",IF(Q_Total=\"\",\"\",IF(AR64=\"\",\"\",IF(AO64=\"\",\"\",AR64+((Qh_Stream*(AR64-W64)+Qh_SP*(AR64-AO64))/Disc_Flow_CFS)))))","v":""},null,null,null,{"$f":"IF(U64<\"\",U64,0.5)","v":0.5},null,{"$f":"EXP((2.326*(LN(BC64^2/No_Samples+1))^0.5)-(0.5*LN(BC64^2/No_Samples+1)))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"AU64*BE64","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"AY64*BE64","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L65=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L65,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L65,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L65,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L65=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L65,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L65,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L65=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L65,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L65,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L66=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L66,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L66,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L66,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L66=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L66,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L66,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L66=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L66,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L66,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L67=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L67,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L67,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L67,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L67=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L67,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L67,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L67=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L67,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L67,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L68=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L68,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L68,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L68,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L68=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L68,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L68,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L68=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L68,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L68,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L69=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L69,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L69,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L69,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L69=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L69,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L69,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L69=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L69,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L69,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L70=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L70,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L70,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L70,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L70=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L70,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L70,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L70=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L70,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L70,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L71=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L71,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L71,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L71,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L71=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L71,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L71,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L71=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L71,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L71,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L72=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L72,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L72,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L72,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L72=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L72,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L72,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L72=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L72,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L72,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L73=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L73,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L73,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L73,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L73=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L73,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L73,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L73=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L73,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L73,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L74=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L74,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L74,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L74,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L74=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L74,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L74,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L74=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L74,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L74,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L75=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L75,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L75,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L75,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L75=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L75,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L75,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L75=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L75,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L75,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L76=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L76,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L76,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L76,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L76=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L76,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L76,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L76=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L76,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L76,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L77=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L77,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L77,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L77,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L77=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L77,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L77,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L77=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L77,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L77,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L78=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L78,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L78,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L78,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L78=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L78,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L78,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L78=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L78,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L78,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L79=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L79,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L79,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L79,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L79=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L79,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L79,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L79=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L79,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L79,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L80=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L80,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L80,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L80,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L80=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L80,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L80,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L80=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L80,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L80,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L81=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L81,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L81,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L81,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L81=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L81,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L81,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L81=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L81,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L81,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L82=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L82,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L82,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L82,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L82=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L82,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L82,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L82=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L82,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L82,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L83=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L83,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L83,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L83,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L83=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L83,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L83,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L83=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L83,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L83,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L84=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L84,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L84,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L84,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L84=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L84,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L84,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L84=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L84,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L84,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L85=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L85,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L85,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L85,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L85=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L85,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L85,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L85=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L85,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L85,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,{"$f":"IF(Qh_Stream=\"\",\"\",IF(Q_Total=\"\",\"\",IF(AR85=\"\",\"\",IF(AO85=\"\",\"\",((Q_Total*AR85)-(Qh_Stream*AO85))/Disc_Flow_CFS))))","v":""},null,null,null,"",null,null,null,0.5,null,{"$f":"EXP((2.326*(LN(BC85^2/No_Samples+1))^0.5)-(0.5*LN(BC85^2/No_Samples+1)))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"AU85*BE85","v":{"$error":"#VALUE!"}},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L86=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L86,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L86,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L86,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L86=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L86,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L86,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L86=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L86,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L86,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L87=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L87,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L87,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L87,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L87=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L87,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L87,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L87=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L87,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L87,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L88=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L88,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L88,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L88,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L88=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L88,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L88,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L88=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L88,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L88,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L89=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L89,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L89,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L89,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L89=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L89,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L89,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L89=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L89,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L89,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L90=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L90,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L90,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L90,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L90=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L90,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L90,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L90=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L90,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L90,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L91=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L91,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L91,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L91,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L91=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L91,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L91,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L91=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L91,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L91,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L92=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L92,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L92,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L92,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L92=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L92,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L92,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L92=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L92,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L92,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Parameter*",null,null,null,null,"Units",null,null,"Existing AML or Concentration",null,null,null,"CV           (0.5 if left blank)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SP Upstream Conc",null,null,"HQ WQ Objective ",null,null,"Non-Degrading Expansion LTA",null,null,null,"CV",null,"AML Multiplier",null,null,"Expansion AML",null,null,null,"Blended AML"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L97=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L97,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L97,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L97,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L97=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L97,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L97,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L97=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L97,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L97,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,{"$f":"IF(Qh_Stream=\"\",\"\",IF(Q_Total_Exp=\"\",\"\",IF(AR97=\"\",\"\",IF(AO97=\"\",\"\",((Q_Total_Exp*AR97)-(Qh_Stream*AO97))/Exp_Flow_CFS))))","v":""},null,null,null,{"$f":"IF(X97=\"\",0.5,X97)","v":0.5},null,{"$f":"EXP((2.326*(LN(AY97^2/No_Samples+1))^0.5)-(0.5*LN(AY97^2/No_Samples+1)))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"AU97*BA97","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"(T97*Disc_Flow_CFS+BD97*Exp_Flow_CFS)/(Disc_Flow_CFS+Exp_Flow_CFS)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L98=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L98,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L98,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L98,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L98=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L98,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L98,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L98=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L98,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L98,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$f":"EXP((2.326*(LN(AY98^2/No_Samples+1))^0.5)-(0.5*LN(AY98^2/No_Samples+1)))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"AU98*BA98","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"(T98*Disc_Flow_CFS+BD98*Exp_Flow_CFS)/(Disc_Flow_CFS+Exp_Flow_CFS)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L99=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L99,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L99,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L99,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L99=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L99,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L99,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L99=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L99,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L99,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L100=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L100,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L100,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L100,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L100=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L100,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L100,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L100=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L100,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L100,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L101=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L101,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L101,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L101,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L101=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L101,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L101,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L101=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L101,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L101,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L102=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L102,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L102,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L102,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L102=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L102,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L102,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L102=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L102,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L102,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L103=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L103,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L103,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L103,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L103=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L103,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L103,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L103=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L103,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L103,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L104=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L104,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L104,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L104,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L104=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L104,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L104,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L104=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L104,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L104,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L105=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L105,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L105,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L105,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L105=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L105,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L105,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L105=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L105,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L105,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L106=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L106,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L106,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L106,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L106=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L106,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L106,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L106=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L106,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L106,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L107=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L107,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L107,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L107,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L107=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L107,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L107,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L107=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L107,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L107,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L108=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L108,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L108,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L108,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L108=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L108,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L108,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L108=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L108,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L108,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L109=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L109,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L109,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L109,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L109=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L109,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L109,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L109=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L109,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L109,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L110=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L110,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L110,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L110,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L110=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L110,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L110,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L110=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L110,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L110,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L111=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L111,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L111,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L111,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L111=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L111,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L111,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L111=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L111,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L111,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,{"$f":"IF(Qh_Stream=\"\",\"\",IF(Q_Total_Exp=\"\",\"\",IF(AR111=\"\",\"\",IF(AO111=\"\",\"\",((Q_Total_Exp*AR111)-(Qh_Stream*AO111))/Exp_Flow_CFS))))","v":""},null,null,null,{"$f":"IF(X111=\"\",0.5,X111)","v":0.5},null,{"$f":"EXP((2.326*(LN(AY111^2/No_Samples+1))^0.5)-(0.5*LN(AY111^2/No_Samples+1)))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"AU111*BA111","v":{"$error":"#VALUE!"}},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L112=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L112,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L112,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L112,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L112=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L112,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L112,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L112=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L112,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L112,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L113=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L113,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L113,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L113,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L113=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L113,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L113,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L113=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L113,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L113,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L114=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L114,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L114,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L114,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L114=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L114,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L114,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L114=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L114,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L114,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L115=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L115,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L115,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L115,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L115=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L115,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L115,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L115=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L115,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L115,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L116=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L116,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L116,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L116,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L116=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L116,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L116,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L116=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L116,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L116,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L117=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L117,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L117,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L117,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L117=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L117,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L117,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L117=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L117,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L117,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L118=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L118,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L118,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L118,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L118=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L118,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L118,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L118=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L118,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L118,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L119=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L119,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L119,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L119,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L119=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L119,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L119,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L119=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L119,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L119,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,{"$f":"IF(X119=\"\",0.5,X119)","v":0.5},null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L120=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L120,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L120,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L120,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L120=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L120,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L120,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L120=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L120,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L120,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L121=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L121,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L121,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L121,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L121=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L121,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L121,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L121=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L121,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L121,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L122=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L122,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L122,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L122,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L122=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L122,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L122,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L122=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L122,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L122,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L123=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L123,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L123,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L123,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L123=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L123,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L123,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L123=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L123,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L123,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L124=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L124,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L124,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L124,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L124=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L124,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L124,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L124=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L124,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L124,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L125=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L125,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L125,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L125,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L125=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L125,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L125,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L125=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L125,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L125,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L126=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(L126,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\",VLOOKUP(L126,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(L126,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L126=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L126,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(L126,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(L126=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(L126,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(L126,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(I127=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(I127,'Site-Specific Data'!D$3:G$30,2,FALSE),VLOOKUP(I127,(INDIRECT(\"'\"&Data_Source&\"'!C2:K74\")),6,TRUE))))","v":""},null,null,{"$f":"IF(I127=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(I127,'Site-Specific Data'!D$3:G$30,3,FALSE),VLOOKUP(I127,(INDIRECT(\"'\"&Data_Source&\"'!C2:K74\")),7,FALSE))))","v":""}]
[null,null,null,null,null,null,null,null,null,"Parameter*",null,null,null,null,"Units",null,null,"Existing AML or Concentration",null,null,null,"Upstream Concentration",null,null,null,"CV           (0.5 if left blank)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SP Upstream Conc",null,null,"HQ WQ Objective ",null,null,"Non-Degrading Expansion Upstream LTA",null,null,null,"CV",null,"AML Multiplier",null,null,"Expansion AML",null,null,null,"Blended AML"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J131=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J131,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J131,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J131,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J131=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J131,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J131,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J131=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J131,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J131,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,{"$f":"IF(Qh_Stream=\"\",\"\",IF(Exp_Flow_CFS=\"\",\"\",IF(AR131=\"\",\"\",AR131+((Qh_Stream*(AR131-V131)+Qh_SP*(AR131-AO131))/Exp_Flow_CFS))))","v":""},null,null,null,{"$f":"IF(Z131=\"\",0.5,Z131)","v":0.5},null,{"$f":"EXP((2.326*(LN(AY131^2/No_Samples+1))^0.5)-(0.5*LN(AY131^2/No_Samples+1)))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"AU131*BA131","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"(R131*Disc_Flow_CFS+BD131*Exp_Flow_CFS)/(Disc_Flow_CFS+Exp_Flow_CFS)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J132=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J132,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J132,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J132,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J132=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J132,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J132,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J132=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J132,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J132,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,{"$f":"IF(Qh_Stream=\"\",\"\",IF(Exp_Flow_CFS=\"\",\"\",IF(AR132=\"\",\"\",AR132+((Qh_Stream*(AR132-V132)+Qh_SP*(AR132-AO132))/Exp_Flow_CFS))))","v":""},null,null,null,0.5,null,{"$f":"EXP((2.326*(LN(AY132^2/No_Samples+1))^0.5)-(0.5*LN(AY132^2/No_Samples+1)))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"AU132*BA132","v":{"$error":"#VALUE!"}},null,null,null,{"$f":"(R132*Disc_Flow_CFS+BD132*Exp_Flow_CFS)/(Disc_Flow_CFS+Exp_Flow_CFS)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J133=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J133,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J133,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J133,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J133=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J133,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J133,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J133=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J133,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J133,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$f":"AU133*BA133","v":{"$error":"#VALUE!"}},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J134=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J134,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J134,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J134,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J134=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J134,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J134,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J134=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J134,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J134,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J135=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J135,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J135,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J135,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J135=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J135,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J135,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J135=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J135,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J135,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J136=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J136,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J136,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J136,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J136=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J136,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J136,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J136=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J136,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J136,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J137=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J137,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J137,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J137,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J137=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J137,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J137,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J137=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J137,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J137,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$f":"AU137*BA137","v":{"$error":"#VALUE!"}},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J138=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J138,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J138,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J138,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J138=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J138,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J138,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J138=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J138,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J138,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J139=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J139,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J139,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J139,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J139=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J139,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J139,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J139=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J139,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J139,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J140=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J140,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J140,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J140,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J140=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J140,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J140,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J140=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J140,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J140,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J141=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J141,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J141,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J141,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J141=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J141,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J141,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J141=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J141,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J141,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J142=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J142,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J142,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J142,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J142=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J142,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J142,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J142=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J142,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J142,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J143=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J143,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J143,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J143,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J143=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J143,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J143,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J143=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J143,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J143,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J144=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J144,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J144,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J144,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J144=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J144,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J144,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J144=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J144,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J144,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,{"$f":"IF(Z144=\"\",0.5,Z144)","v":0.5},null,{"$f":"EXP((2.326*(LN(AY144^2/No_Samples+1))^0.5)-(0.5*LN(AY144^2/No_Samples+1)))","v":{"$error":"#DIV/0!"}},null,null,{"$f":"AU144*BA144","v":{"$error":"#VALUE!"}},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J145=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J145,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J145,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J145,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J145=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J145,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J145,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J145=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J145,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J145,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J146=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J146,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J146,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J146,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J146=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J146,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J146,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J146=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J146,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J146,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J147=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J147,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J147,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J147,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J147=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J147,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J147,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J147=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J147,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J147,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J148=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J148,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J148,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J148,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J148=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J148,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J148,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J148=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J148,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J148,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J149=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J149,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J149,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J149,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J149=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J149,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J149,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J149=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J149,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J149,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J150=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J150,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J150,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J150,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J150=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J150,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J150,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J150=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J150,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J150,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J151=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J151,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J151,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J151,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J151=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J151,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J151,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J151=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J151,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J151,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J152=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J152,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J152,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J152,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J152=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J152,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J152,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J152=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J152,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J152,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,{"$f":"IF(Z152=\"\",0.5,Z152)","v":0.5},null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J153=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J153,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J153,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J153,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J153=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J153,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J153,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J153=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J153,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J153,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J154=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J154,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J154,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J154,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J154=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J154,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J154,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J154=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J154,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J154,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J155=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J155,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J155,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J155,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J155=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J155,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J155,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J155=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J155,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J155,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J156=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J156,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J156,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J156,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J156=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J156,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J156,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J156=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J156,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J156,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J157=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J157,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J157,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J157,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J157=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J157,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J157,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J157=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J157,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J157,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J158=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J158,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J158,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J158,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J158=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J158,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J158,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J158=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J158,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J158,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J159=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J159,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J159,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J159,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J159=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J159,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J159,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J159=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J159,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J159,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$error":"#VALUE!"},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J160=\"\",\"\",IF($G$14=\"Site-Specific Data\",IF(VLOOKUP(J160,'Site-Specific Data'!$D$3:$G$39,4,FALSE)=\"\",\"\", VLOOKUP(J160,'Site-Specific Data'!$D$3:$G$39,4,FALSE)),(VLOOKUP(J160,(INDIRECT(\"'\"&$G$14&\"'!D2:E74\")),2,FALSE))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(J160=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J160,'Site-Specific Data'!D$3:G$39,2,FALSE),VLOOKUP(J160,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),9,FALSE))))","v":""},null,null,{"$f":"IF(J160=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(J160,'Site-Specific Data'!D$3:G$39,3,FALSE),VLOOKUP(J160,(INDIRECT(\"'\"&Data_Source&\"'!D2:M74\")),10,FALSE))))","v":""},null,null,"",null,null,null,0.5,null,{"$error":"#DIV/0!"},null,null,{"$f":"AU160*BA160","v":{"$error":"#VALUE!"}},null,null,null,{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(I161=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(I161,'Site-Specific Data'!D$3:G$30,2,FALSE),VLOOKUP(I161,(INDIRECT(\"'\"&Data_Source&\"'!C2:K74\")),6,FALSE))))","v":""},null,null,{"$f":"IF(I161=\"\",\"\",(IF(Data_Source=\"Site-Specific Data\",VLOOKUP(I161,'Site-Specific Data'!D$3:G$30,3,FALSE),VLOOKUP(I161,(INDIRECT(\"'\"&Data_Source&\"'!C2:K74\")),7,FALSE))))","v":""},null,null,{"$f":"IF(Qh_Stream=\"\",\"\",IF(Q_Total=\"\",\"\",IF(AN161=\"\",\"\",IF(#REF!=\"\",\"\",AN161+((Qh_Stream*(AN161-M161)+Qh_SP*(AN161-#REF!))/Disc_Flow_CFS)))))","v":""}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,"Site-Specific Data"]
[null,null,null,null,null,null,null,null,null,"WQN0100"]
[null,null,null,null,null,null,null,null,null,"WQN0178"]
[null,null,null,null,null,null,null,null,null,"WQN0181"]
[null,null,null,null,null,null,null,null,null,"WQN0183"]
[null,null,null,null,null,null,null,null,null,"WQN0191"]
[null,null,null,null,null,null,null,null,null,"WQN0195"]
[null,null,null,null,null,null,null,null,null,"WQN0196"]
[null,null,null,null,null,null,null,null,null,"WQN0197"]
[null,null,null,null,null,null,null,null,null,"WQN0199"]
[null,null,null,null,null,null,null,null,null,"WQN0275"]
[null,null,null,null,null,null,null,null,null,"WQN0276"]
[null,null,null,null,null,null,null,null,null,"WQN0279"]
[null,null,null,null,null,null,null,null,null,"WQN0290"]
[null,null,null,null,null,null,null,null,null,"WQN0291"]
[null,null,null,null,null,null,null,null,null,"WQN0292"]
[null,null,null,null,null,null,null,null,null,"WQN0294"]
[null,null,null,null,null,null,null,null,null,"WQN0296"]
[null,null,null,null,null,null,null,null,null,"WQN0297"]
[null,null,null,null,null,null,null,null,null,"WQN0409"]
[null,null,null,null,null,null,null,null,null,"WQN0411"]
[null,null,null,null,null,null,null,null,null,"WQN0428"]
[null,null,null,null,null,null,null,null,null,"WQN0443"]
[null,null,null,null,null,null,null,null,null,"WQN0452"]
[null,null,null,null,null,null,null,null,null,"WQN0453"]
[null,null,null,null,null,null,null,null,null,"WQN0454"]
[null,null,null,null,null,null,null,null,null,"WQN0455"]
[null,null,null,null,null,null,null,null,null,"WQN0456"]
[null,null,null,null,null,null,null,null,null,"WQN0457"]
[null,null,null,null,null,null,null,null,null,"WQN0458"]
[null,null,null,null,null,null,null,null,null,"WQN0459"]
[null,null,null,null,null,null,null,null,null,"WQN0463"]
[null,null,null,null,null,null,null,null,null,"WQN0464"]
[null,null,null,null,null,null,null,null,null,"WQN0465"]
[null,null,null,null,null,null,null,null,null,"WQN0466"]
[null,null,null,null,null,null,null,null,null,"WQN0500"]
[null,null,null,null,null,null,null,null,null,"WQN0514"]
[null,null,null,null,null,null,null,null,null,"WQN0626"]
[null,null,null,null,null,null,null,null,null,"WQN0627"]
[null,null,null,null,null,null,null,null,null,"WQN0628"]
[null,null,null,null,null,null,null,null,null,"WQN0629"]
[null,null,null,null,null,null,null,null,null,"WQN0630"]
[null,null,null,null,null,null,null,null,null,"WQN0634"]
[null,null,null,null,null,null,null,null,null,"WQN0723"]
[null,null,null,null,null,null,null,null,null,"WQN0724"]
[null,null,null,null,null,null,null,null,null,"WQN0733"]
[null,null,null,null,null,null,null,null,null,"WQN0734"]
[null,null,null,null,null,null,null,null,null,"WQN0735"]
[null,null,null,null,null,null,null,null,null,"WQN0870"]
[null,null,null,null,null,null,null,null,null,"WQN0873"]
[null,null,null,null,null,null,null,null,null,"WQN0877"]
[null,null,null,null,null,null,null,null,null,"WQN0879"]
[null,null,null,null,null,null,null,null,null,"WQN0885"]

{"sheet":"Results","index":2,"n_rows":79,"n_cols":43,"rows_kept":79,"cut":false,"hidden":true,"merged":[[76,18,76,20],[77,18,77,20],[78,18,78,20],[49,18,49,20],[47,18,48,20],[67,18,67,20],[68,18,68,20],[69,18,69,20],[70,18,70,20],[71,18,71,20],[72,18,72,20],[73,18,73,20],[74,18,74,20],[75,18,75,20],[58,18,58,20],[59,18,59,20],[60,18,60,20],[61,18,61,20],[62,18,62,20],[63,18,63,20],[64,18,64,20],[65,18,65,20],[66,18,66,20],[50,18,50,20],[51,18,51,20],[52,18,52,20],[53,18,53,20],[54,18,54,20],[55,18,55,20],[56,18,56,20],[57,18,57,20],[73,14,73,17],[1,21,1,27],[23,22,23,24],[24,22,24,24],[16,13,16,15],[17,13,17,15],[18,13,18,15],[19,13,19,15],[20,13,20,15],[21,13,21,15],[22,13,22,15],[23,13,23,15],[24,13,24,15],[16,16,16,18],[17,16,17,18],[18,16,18,18],[19,16,19,18],[18,25,18,27],[19,25,19,27],[20,25,20,27],[21,25,21,27],[22,25,22,27],[23,25,23,27],[24,25,24,27],[16,22,16,24],[17,22,17,24],[18,22,18,24],[19,22,19,24],[20,22,20,24],[21,22,21,24],[22,22,22,24],[78,14,78,17],[68,14,68,17],[69,14,69,17],[70,14,70,17],[71,14,71,17],[72,14,72,17],[74,14,74,17],[75,14,75,17],[76,14,76,17],[77,14,77,17],[50,14,50,17],[51,14,51,17],[52,14,52,17],[53,14,53,17],[54,14,54,17],[55,14,55,17],[66,14,66,17],[67,14,67,17],[56,14,56,17],[57,14,57,17],[58,14,58,17],[59,14,59,17],[60,14,60,17],[61,14,61,17],[62,14,62,17],[63,14,63,17],[64,14,64,17],[65,14,65,17],[74,10,74,13],[75,10,75,13],[76,10,76,13],[77,1,77,9],[78,1,78,9],[73,1,73,9],[74,1,74,9],[75,1,75,9],[76,1,76,9],[77,10,77,13],[78,10,78,13],[50,10,50,13],[51,10,51,13],[52,10,52,13],[53,10,53,13],[54,10,54,13],[70,10,70,13],[71,10,71,13],[72,10,72,13],[73,10,73,13],[68,10,68,13],[69,10,69,13],[55,10,55,13],[56,10,56,13],[57,10,57,13],[58,10,58,13],[59,10,59,13],[60,10,60,13],[61,10,61,13],[62,10,62,13],[63,10,63,13],[64,10,64,13],[65,10,65,13],[66,10,66,13],[67,10,67,13],[68,1,68,9],[69,1,69,9],[70,1,70,9],[71,1,71,9],[72,1,72,9],[59,1,59,9],[60,1,60,9],[61,1,61,9],[62,1,62,9],[63,1,63,9],[64,1,64,9],[65,1,65,9],[66,1,66,9],[67,1,67,9],[50,1,50,9],[51,1,51,9],[52,1,52,9],[53,1,53,9],[54,1,54,9],[55,1,55,9],[56,1,56,9],[57,1,57,9],[58,1,58,9],[42,1,42,9],[42,10,42,12],[42,13,42,15],[42,16,42,18],[42,22,42,24],[42,25,42,27],[42,19,42,21],[47,1,48,9],[49,1,49,9],[47,10,48,13],[47,14,48,17],[49,10,49,13],[49,14,49,17],[40,1,40,9],[40,10,40,12],[40,13,40,15],[40,16,40,18],[40,22,40,24],[40,25,40,27],[40,19,40,21],[41,1,41,9],[41,10,41,12],[41,13,41,15],[41,16,41,18],[41,22,41,24],[41,25,41,27],[41,19,41,21],[38,1,38,9],[38,10,38,12],[38,13,38,15],[38,16,38,18],[38,22,38,24],[38,25,38,27],[38,19,38,21],[39,1,39,9],[39,10,39,12],[39,13,39,15],[39,16,39,18],[39,22,39,24],[39,25,39,27],[39,19,39,21],[36,1,36,9],[36,10,36,12],[36,13,36,15],[36,16,36,18],[36,22,36,24],[36,25,36,27],[36,19,36,21],[37,1,37,9],[37,10,37,12],[37,13,37,15],[37,16,37,18],[37,22,37,24],[37,25,37,27],[37,19,37,21],[34,1,34,9],[34,10,34,12],[34,13,34,15],[34,16,34,18],[34,22,34,24],[34,25,34,27],[34,19,34,21],[35,1,35,9],[35,10,35,12],[35,13,35,15],[35,16,35,18],[35,22,35,24],[35,25,35,27],[35,19,35,21],[32,1,32,9],[32,10,32,12],[32,13,32,15],[32,16,32,18],[32,22,32,24],[32,25,32,27],[32,19,32,21],[33,1,33,9],[33,10,33,12],[33,13,33,15],[33,16,33,18],[33,22,33,24],[33,25,33,27],[33,19,33,21],[30,1,30,9],[30,10,30,12],[30,13,30,15],[30,16,30,18],[30,22,30,24],[30,25,30,27],[30,19,30,21],[31,1,31,9],[31,10,31,12],[31,13,31,15],[31,16,31,18],[31,22,31,24],[31,25,31,27],[31,19,31,21],[28,1,28,9],[28,10,28,12],[28,13,28,15],[28,16,28,18],[28,22,28,24],[28,25,28,27],[28,19,28,21],[29,1,29,9],[29,10,29,12],[29,13,29,15],[29,16,29,18],[29,22,29,24],[29,25,29,27],[29,19,29,21],[26,1,26,9],[26,10,26,12],[26,13,26,15],[26,16,26,18],[26,22,26,24],[26,25,26,27],[26,19,26,21],[25,19,25,21],[27,1,27,9],[27,10,27,12],[27,13,27,15],[27,16,27,18],[27,22,27,24],[27,25,27,27],[27,19,27,21],[25,1,25,9],[25,10,25,12],[25,13,25,15],[25,16,25,18],[22,16,22,18],[23,16,23,18],[24,16,24,18],[25,22,25,24],[25,25,25,27],[22,1,22,9],[23,1,23,9],[24,1,24,9],[19,10,19,12],[20,10,20,12],[21,10,21,12],[22,19,22,21],[23,19,23,21],[24,19,24,21],[22,10,22,12],[23,10,23,12],[24,10,24,12],[15,22,15,24],[14,25,14,27],[15,25,15,27],[14,19,14,21],[15,19,15,21],[14,10,14,12],[15,10,15,12],[16,10,16,12],[17,10,17,12],[16,19,16,21],[17,19,17,21],[14,22,14,24],[16,25,16,27],[17,25,17,27],[18,19,18,21],[19,19,19,21],[20,19,20,21],[21,19,21,21],[14,1,14,9],[15,1,15,9],[14,16,14,18],[15,16,15,18],[14,13,14,15],[15,13,15,15],[16,1,16,9],[17,1,17,9],[18,1,18,9],[20,16,20,18],[21,16,21,18],[18,10,18,12],[19,1,19,9],[20,1,20,9],[21,1,21,9],[13,1,13,9],[13,10,13,12],[13,13,13,15],[13,16,13,18],[13,19,13,21],[13,22,13,24],[13,25,13,27],[10,10,10,15],[10,16,10,27],[11,1,12,9],[11,10,12,12],[11,13,12,15],[11,16,12,18],[11,19,12,21],[11,22,12,24],[11,25,12,27]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Instructions!B1","v":"Anti-degradation Limits Spreadsheet"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Instructions!B2","v":"Version 1.0, April 2024"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,true]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Analysis Type ",null,null,null,{"$f":"Inputs!AA10","v":0}]
[]
[]
[]
[]
[]
[null,"Recommended Non-Degrading Limits"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($AP$3=\"New Direct to SP\",Inputs!AY29,IF($AP$3=\"New Upstream of SP\",Inputs!BC63,IF($AP$3=\"Expanding Direct to SP\",Inputs!AY97,IF($AP$3=\"Expanding Upstream of SP\",Inputs!AY131,\"\"))))","v":""}]
[null,null,null,null,null,null,null,null,null,null,"Mass Limits",null,null,null,null,null,"Concentration Limits"]
[null,"Pollutants",null,null,null,null,null,null,null,null,"AML (lbs/day)",null,null,"MDL (lbs/day)",null,null,"AML",null,null,"MDL",null,null,"IMAX",null,null,"Units"]
[]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N29<>\"\"),Inputs!N29,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L63<>\"\"),Inputs!L63,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L97<>\"\"),Inputs!L97,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J131<>\"\"),Inputs!J131,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND(Q14<>\"\",OR(Z14=\"mg/L\",Z14=\"ng/L\",Z14=\"ug/L\",Z14=\"µg/L\")),Total_Flow_MGD*8.34*Q14*IF(Z14=\"mg/L\",1,IF(Z14=\"ng/L\",0.000001,0.001)),\"XXX\")","v":"XXX"},null,null,{"$f":"IF(AND(T14<>\"\",OR(Z14=\"mg/L\",Z14=\"ng/L\",Z14=\"ug/L\",Z14=\"µg/L\")),Total_Flow_MGD*8.34*T14*IF(Z14=\"mg/L\",1,IF(Z14=\"ng/L\",0.000001,0.001)),\"XXX\")","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N29<>\"\"),Inputs!BD29,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L63<>\"\"),Inputs!BL63,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L97<>\"\"),Inputs!BH97,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J131<>\"\"),Inputs!BH131,\"\"))))","v":""},null,null,{"$f":"Q14*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY29,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC63,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY97,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY131,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY29,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC63,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY97,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY131,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY29,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC63,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY97,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY131,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY29,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC63,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY97,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY131,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$f":"Q14*2.5","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N29<>\"\"),Inputs!T29,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L63<>\"\"),Inputs!R63,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L97<>\"\"),Inputs!Q97,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J131<>\"\"),Inputs!O131,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N30<>\"\"),Inputs!N30,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L64<>\"\"),Inputs!L64,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L98<>\"\"),Inputs!L98,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J132<>\"\"),Inputs!J132,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N30<>\"\"),Inputs!BD30,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L64<>\"\"),Inputs!BL64,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L98<>\"\"),Inputs!BH98,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J132<>\"\"),Inputs!BH132,\"\"))))","v":""},null,null,{"$f":"Q15*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY30,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC64,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY98,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY132,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY30,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC64,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY98,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY132,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY30,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC64,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY98,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY132,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY30,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC64,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY98,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY132,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$f":"Q15*2.5","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N30<>\"\"),Inputs!T30,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L64<>\"\"),Inputs!R64,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L98<>\"\"),Inputs!Q98,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J132<>\"\"),Inputs!O132,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N31<>\"\"),Inputs!N31,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L65<>\"\"),Inputs!L65,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L99<>\"\"),Inputs!L99,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J133<>\"\"),Inputs!J133,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N31<>\"\"),Inputs!BD31,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L65<>\"\"),Inputs!BL65,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L99<>\"\"),Inputs!BH99,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J133<>\"\"),Inputs!BH133,\"\"))))","v":""},null,null,{"$f":"Q16*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY31,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC65,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY99,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY133,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY31,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC65,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY99,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY133,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY31,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC65,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY99,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY133,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY31,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC65,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY99,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY133,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N31<>\"\"),Inputs!T31,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L65<>\"\"),Inputs!R65,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L99<>\"\"),Inputs!Q99,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J133<>\"\"),Inputs!O133,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N32<>\"\"),Inputs!N32,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L66<>\"\"),Inputs!L66,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L100<>\"\"),Inputs!L100,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J134<>\"\"),Inputs!J134,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N32<>\"\"),Inputs!BD32,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L66<>\"\"),Inputs!BL66,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L100<>\"\"),Inputs!BH100,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J134<>\"\"),Inputs!BH134,\"\"))))","v":""},null,null,{"$f":"Q17*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY32,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC66,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY100,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY134,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY32,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC66,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY100,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY134,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY32,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC66,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY100,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY134,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY32,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC66,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY100,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY134,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N32<>\"\"),Inputs!T32,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L66<>\"\"),Inputs!R66,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L100<>\"\"),Inputs!Q100,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J134<>\"\"),Inputs!O134,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N33<>\"\"),Inputs!N33,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L67<>\"\"),Inputs!L67,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L101<>\"\"),Inputs!L101,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J135<>\"\"),Inputs!J135,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N33<>\"\"),Inputs!BD33,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L67<>\"\"),Inputs!BL67,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L101<>\"\"),Inputs!BH101,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J135<>\"\"),Inputs!BH135,\"\"))))","v":""},null,null,{"$f":"Q18*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY33,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC67,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY101,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY135,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY33,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC67,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY101,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY135,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY33,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC67,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY101,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY135,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY33,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC67,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY101,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY135,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N33<>\"\"),Inputs!T33,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L67<>\"\"),Inputs!R67,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L101<>\"\"),Inputs!Q101,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J135<>\"\"),Inputs!O135,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N34<>\"\"),Inputs!N34,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L68<>\"\"),Inputs!L68,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L102<>\"\"),Inputs!L102,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J136<>\"\"),Inputs!J136,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N34<>\"\"),Inputs!BD34,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L68<>\"\"),Inputs!BL68,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L102<>\"\"),Inputs!BH102,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J136<>\"\"),Inputs!BH136,\"\"))))","v":""},null,null,{"$f":"Q19*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY34,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC68,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY102,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY136,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY34,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC68,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY102,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY136,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY34,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC68,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY102,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY136,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY34,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC68,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY102,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY136,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N34<>\"\"),Inputs!T34,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L68<>\"\"),Inputs!R68,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L102<>\"\"),Inputs!Q102,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J136<>\"\"),Inputs!O136,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N35<>\"\"),Inputs!N35,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L69<>\"\"),Inputs!L69,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L103<>\"\"),Inputs!L103,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J137<>\"\"),Inputs!J137,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N35<>\"\"),Inputs!BD35,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L69<>\"\"),Inputs!BL69,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L103<>\"\"),Inputs!BH103,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J137<>\"\"),Inputs!BH137,\"\"))))","v":""},null,null,{"$f":"Q20*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY35,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC69,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY103,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY137,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY35,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC69,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY103,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY137,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY35,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC69,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY103,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY137,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY35,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC69,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY103,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY137,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N35<>\"\"),Inputs!T35,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L69<>\"\"),Inputs!R69,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L103<>\"\"),Inputs!Q103,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J137<>\"\"),Inputs!O137,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N36<>\"\"),Inputs!N36,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L70<>\"\"),Inputs!L70,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L104<>\"\"),Inputs!L104,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J138<>\"\"),Inputs!J138,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N36<>\"\"),Inputs!BD36,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L70<>\"\"),Inputs!BL70,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L104<>\"\"),Inputs!BH104,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J138<>\"\"),Inputs!BH138,\"\"))))","v":""},null,null,{"$f":"Q21*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY36,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC70,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY104,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY138,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY36,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC70,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY104,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY138,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY36,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC70,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY104,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY138,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY36,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC70,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY104,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY138,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N36<>\"\"),Inputs!T36,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L70<>\"\"),Inputs!R70,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L104<>\"\"),Inputs!Q104,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J138<>\"\"),Inputs!O138,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N37<>\"\"),Inputs!N37,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L71<>\"\"),Inputs!L71,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L105<>\"\"),Inputs!L105,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J139<>\"\"),Inputs!J139,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N37<>\"\"),Inputs!BD37,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L71<>\"\"),Inputs!BL71,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L105<>\"\"),Inputs!BH105,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J139<>\"\"),Inputs!BH139,\"\"))))","v":""},null,null,{"$f":"Q22*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY37,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC71,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY105,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY139,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY37,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC71,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY105,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY139,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY37,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC71,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY105,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY139,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY37,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC71,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY105,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY139,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N37<>\"\"),Inputs!T37,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L71<>\"\"),Inputs!R71,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L105<>\"\"),Inputs!Q105,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J139<>\"\"),Inputs!O139,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N38<>\"\"),Inputs!N38,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L72<>\"\"),Inputs!L72,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L106<>\"\"),Inputs!L106,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J140<>\"\"),Inputs!J140,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N38<>\"\"),Inputs!BD38,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L72<>\"\"),Inputs!BL72,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L106<>\"\"),Inputs!BH106,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J140<>\"\"),Inputs!BH140,\"\"))))","v":""},null,null,{"$f":"Q23*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY38,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC72,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY106,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY140,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY38,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC72,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY106,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY140,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY38,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC72,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY106,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY140,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY38,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC72,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY106,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY140,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N38<>\"\"),Inputs!T38,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L72<>\"\"),Inputs!R72,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L106<>\"\"),Inputs!Q106,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J140<>\"\"),Inputs!O140,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N39<>\"\"),Inputs!N39,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L73<>\"\"),Inputs!L73,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L107<>\"\"),Inputs!L107,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J141<>\"\"),Inputs!J141,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N39<>\"\"),Inputs!BD39,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L73<>\"\"),Inputs!BL73,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L107<>\"\"),Inputs!BH107,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J141<>\"\"),Inputs!BH141,\"\"))))","v":""},null,null,{"$f":"Q24*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY39,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC73,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY107,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY141,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY39,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC73,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY107,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY141,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY39,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC73,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY107,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY141,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY39,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC73,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY107,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY141,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N39<>\"\"),Inputs!T39,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L73<>\"\"),Inputs!R73,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L107<>\"\"),Inputs!Q107,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J141<>\"\"),Inputs!O141,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N40<>\"\"),Inputs!N40,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L74<>\"\"),Inputs!L74,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L108<>\"\"),Inputs!L108,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J142<>\"\"),Inputs!J142,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N40<>\"\"),Inputs!BD40,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L74<>\"\"),Inputs!BL74,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L108<>\"\"),Inputs!BH108,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J142<>\"\"),Inputs!BH142,\"\"))))","v":""},null,null,{"$f":"Q25*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY40,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC74,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY108,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY142,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY40,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC74,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY108,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY142,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY40,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC74,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY108,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY142,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY40,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC74,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY108,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY142,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N40<>\"\"),Inputs!T40,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L74<>\"\"),Inputs!R74,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L108<>\"\"),Inputs!Q108,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J142<>\"\"),Inputs!O142,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N41<>\"\"),Inputs!N41,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L75<>\"\"),Inputs!L75,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L109<>\"\"),Inputs!L109,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J143<>\"\"),Inputs!J143,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N41<>\"\"),Inputs!BD41,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L75<>\"\"),Inputs!BL75,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L109<>\"\"),Inputs!BH109,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J143<>\"\"),Inputs!BH143,\"\"))))","v":""},null,null,{"$f":"Q26*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY41,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC75,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY109,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY143,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY41,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC75,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY109,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY143,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY41,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC75,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY109,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY143,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY41,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC75,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY109,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY143,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$f":"Q26*2.5","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N41<>\"\"),Inputs!T41,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L75<>\"\"),Inputs!R75,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L109<>\"\"),Inputs!Q109,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J143<>\"\"),Inputs!O143,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N42<>\"\"),Inputs!N42,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L76<>\"\"),Inputs!L76,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L110<>\"\"),Inputs!L110,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J144<>\"\"),Inputs!J144,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N42<>\"\"),Inputs!BD42,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L76<>\"\"),Inputs!BL76,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L110<>\"\"),Inputs!BH110,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J144<>\"\"),Inputs!BH144,\"\"))))","v":""},null,null,{"$f":"Q27*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY42,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC76,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY110,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY144,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY42,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC76,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY110,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY144,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY42,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC76,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY110,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY144,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY42,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC76,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY110,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY144,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N42<>\"\"),Inputs!T42,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L76<>\"\"),Inputs!R76,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L110<>\"\"),Inputs!Q110,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J144<>\"\"),Inputs!O144,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N43<>\"\"),Inputs!N43,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L77<>\"\"),Inputs!L77,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L111<>\"\"),Inputs!L111,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J145<>\"\"),Inputs!J145,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N43<>\"\"),Inputs!BD43,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L77<>\"\"),Inputs!BL77,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L111<>\"\"),Inputs!BH111,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J145<>\"\"),Inputs!BH145,\"\"))))","v":""},null,null,{"$f":"Q28*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY43,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC77,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY111,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY145,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY43,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC77,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY111,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY145,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY43,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC77,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY111,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY145,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY43,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC77,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY111,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY145,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N43<>\"\"),Inputs!T43,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L77<>\"\"),Inputs!R77,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L111<>\"\"),Inputs!Q111,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J145<>\"\"),Inputs!O145,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N44<>\"\"),Inputs!N44,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L78<>\"\"),Inputs!L78,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L112<>\"\"),Inputs!L112,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J146<>\"\"),Inputs!J146,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N44<>\"\"),Inputs!BD44,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L78<>\"\"),Inputs!BL78,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L112<>\"\"),Inputs!BH112,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J146<>\"\"),Inputs!BH146,\"\"))))","v":""},null,null,{"$f":"Q29*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY44,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC78,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY112,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY146,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY44,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC78,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY112,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY146,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY44,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC78,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY112,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY146,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY44,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC78,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY112,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY146,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N44<>\"\"),Inputs!T44,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L78<>\"\"),Inputs!R78,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L112<>\"\"),Inputs!Q112,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J146<>\"\"),Inputs!O146,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N45<>\"\"),Inputs!N45,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L79<>\"\"),Inputs!L79,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L113<>\"\"),Inputs!L113,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J147<>\"\"),Inputs!J147,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N45<>\"\"),Inputs!BD45,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L79<>\"\"),Inputs!BL79,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L113<>\"\"),Inputs!BH113,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J147<>\"\"),Inputs!BH147,\"\"))))","v":""},null,null,{"$f":"Q30*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY45,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC79,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY113,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY147,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY45,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC79,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY113,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY147,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY45,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC79,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY113,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY147,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY45,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC79,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY113,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY147,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N45<>\"\"),Inputs!T45,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L79<>\"\"),Inputs!R79,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L113<>\"\"),Inputs!Q113,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J147<>\"\"),Inputs!O147,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N46<>\"\"),Inputs!N46,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L80<>\"\"),Inputs!L80,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L114<>\"\"),Inputs!L114,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J148<>\"\"),Inputs!J148,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N46<>\"\"),Inputs!BD46,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L80<>\"\"),Inputs!BL80,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L114<>\"\"),Inputs!BH114,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J148<>\"\"),Inputs!BH148,\"\"))))","v":""},null,null,{"$f":"Q31*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY46,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC80,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY114,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY148,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY46,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC80,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY114,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY148,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY46,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC80,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY114,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY148,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY46,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC80,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY114,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY148,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N46<>\"\"),Inputs!T46,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L80<>\"\"),Inputs!R80,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L114<>\"\"),Inputs!Q114,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J148<>\"\"),Inputs!O148,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N47<>\"\"),Inputs!N47,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L81<>\"\"),Inputs!L81,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L115<>\"\"),Inputs!L115,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J149<>\"\"),Inputs!J149,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N47<>\"\"),Inputs!BD47,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L81<>\"\"),Inputs!BL81,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L115<>\"\"),Inputs!BH115,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J149<>\"\"),Inputs!BH149,\"\"))))","v":""},null,null,{"$f":"Q32*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY47,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC81,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY115,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY149,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY47,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC81,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY115,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY149,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY47,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC81,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY115,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY149,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY47,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC81,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY115,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY149,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N47<>\"\"),Inputs!T47,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L81<>\"\"),Inputs!R81,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L115<>\"\"),Inputs!Q115,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J149<>\"\"),Inputs!O149,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N48<>\"\"),Inputs!N48,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L82<>\"\"),Inputs!L82,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L116<>\"\"),Inputs!L116,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J150<>\"\"),Inputs!J150,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N48<>\"\"),Inputs!BD48,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L82<>\"\"),Inputs!BL82,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L116<>\"\"),Inputs!BH116,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J150<>\"\"),Inputs!BH150,\"\"))))","v":""},null,null,{"$f":"Q33*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY48,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC82,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY116,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY150,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY48,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC82,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY116,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY150,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY48,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC82,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY116,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY150,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY48,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC82,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY116,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY150,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N48<>\"\"),Inputs!T48,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L82<>\"\"),Inputs!R82,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L116<>\"\"),Inputs!Q116,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J150<>\"\"),Inputs!O150,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N49<>\"\"),Inputs!N49,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L83<>\"\"),Inputs!L83,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L117<>\"\"),Inputs!L117,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J151<>\"\"),Inputs!J151,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N49<>\"\"),Inputs!BD49,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L83<>\"\"),Inputs!BL83,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L117<>\"\"),Inputs!BH117,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J151<>\"\"),Inputs!BH151,\"\"))))","v":""},null,null,{"$f":"Q34*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY49,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC83,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY117,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY151,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY49,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC83,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY117,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY151,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY49,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC83,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY117,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY151,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY49,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC83,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY117,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY151,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N49<>\"\"),Inputs!T49,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L83<>\"\"),Inputs!R83,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L117<>\"\"),Inputs!Q117,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J151<>\"\"),Inputs!O151,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N50<>\"\"),Inputs!N50,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L84<>\"\"),Inputs!L84,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L118<>\"\"),Inputs!L118,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J152<>\"\"),Inputs!J152,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N50<>\"\"),Inputs!BD50,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L84<>\"\"),Inputs!BL84,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L118<>\"\"),Inputs!BH118,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J152<>\"\"),Inputs!BH152,\"\"))))","v":""},null,null,{"$f":"Q35*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY50,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC84,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY118,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY152,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY50,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC84,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY118,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY152,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY50,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC84,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY118,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY152,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY50,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC84,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY118,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY152,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N50<>\"\"),Inputs!T50,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L84<>\"\"),Inputs!R84,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L118<>\"\"),Inputs!Q118,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J152<>\"\"),Inputs!O152,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N51<>\"\"),Inputs!N51,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L85<>\"\"),Inputs!L85,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L119<>\"\"),Inputs!L119,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J153<>\"\"),Inputs!J153,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N51<>\"\"),Inputs!BD51,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L85<>\"\"),Inputs!BL85,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L119<>\"\"),Inputs!BH119,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J153<>\"\"),Inputs!BH153,\"\"))))","v":""},null,null,{"$f":"Q36*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY51,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC85,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY119,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY153,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY51,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC85,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY119,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY153,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY51,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC85,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY119,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY153,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY51,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC85,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY119,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY153,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N51<>\"\"),Inputs!T51,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L85<>\"\"),Inputs!R85,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L119<>\"\"),Inputs!Q119,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J153<>\"\"),Inputs!O153,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N52<>\"\"),Inputs!N52,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L86<>\"\"),Inputs!L86,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L120<>\"\"),Inputs!L120,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J154<>\"\"),Inputs!J154,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N52<>\"\"),Inputs!BD52,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L86<>\"\"),Inputs!BL86,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L120<>\"\"),Inputs!BH120,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J154<>\"\"),Inputs!BH154,\"\"))))","v":""},null,null,{"$f":"Q37*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY52,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC86,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY120,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY154,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY52,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC86,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY120,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY154,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY52,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC86,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY120,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY154,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY52,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC86,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY120,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY154,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N52<>\"\"),Inputs!T52,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L86<>\"\"),Inputs!R86,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L120<>\"\"),Inputs!Q120,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J154<>\"\"),Inputs!O154,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N53<>\"\"),Inputs!N53,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L87<>\"\"),Inputs!L87,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L121<>\"\"),Inputs!L121,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J155<>\"\"),Inputs!J155,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N53<>\"\"),Inputs!BD53,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L87<>\"\"),Inputs!BL87,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L121<>\"\"),Inputs!BH121,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J155<>\"\"),Inputs!BH155,\"\"))))","v":""},null,null,{"$f":"Q38*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY53,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC87,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY121,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY155,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY53,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC87,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY121,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY155,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY53,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC87,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY121,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY155,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY53,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC87,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY121,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY155,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N53<>\"\"),Inputs!T53,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L87<>\"\"),Inputs!R87,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L121<>\"\"),Inputs!Q121,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J155<>\"\"),Inputs!O155,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N54<>\"\"),Inputs!N54,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L88<>\"\"),Inputs!L88,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L122<>\"\"),Inputs!L122,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J156<>\"\"),Inputs!J156,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N54<>\"\"),Inputs!BD54,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L88<>\"\"),Inputs!BL88,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L122<>\"\"),Inputs!BH122,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J156<>\"\"),Inputs!BH156,\"\"))))","v":""},null,null,{"$f":"Q39*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY54,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC88,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY122,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY156,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY54,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC88,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY122,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY156,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY54,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC88,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY122,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY156,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY54,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC88,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY122,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY156,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N54<>\"\"),Inputs!T54,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L88<>\"\"),Inputs!R88,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L122<>\"\"),Inputs!Q122,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J156<>\"\"),Inputs!O156,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N55<>\"\"),Inputs!N55,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L89<>\"\"),Inputs!L89,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L123<>\"\"),Inputs!L123,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J157<>\"\"),Inputs!J157,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N55<>\"\"),Inputs!BD55,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L89<>\"\"),Inputs!BL89,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L123<>\"\"),Inputs!BH123,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J157<>\"\"),Inputs!BH157,\"\"))))","v":""},null,null,{"$f":"Q40*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY55,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC89,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY123,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY157,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY55,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC89,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY123,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY157,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY55,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC89,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY123,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY157,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY55,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC89,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY123,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY157,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N55<>\"\"),Inputs!T55,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L89<>\"\"),Inputs!R89,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L123<>\"\"),Inputs!Q123,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J157<>\"\"),Inputs!O157,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N56<>\"\"),Inputs!N56,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L90<>\"\"),Inputs!L90,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L124<>\"\"),Inputs!L124,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J158<>\"\"),Inputs!J158,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N56<>\"\"),Inputs!BD56,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L90<>\"\"),Inputs!BL90,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L124<>\"\"),Inputs!BH124,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J158<>\"\"),Inputs!BH158,\"\"))))","v":""},null,null,{"$f":"Q41*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY56,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC90,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY124,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY158,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY56,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC90,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY124,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY158,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY56,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC90,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY124,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY158,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY56,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC90,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY124,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY158,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N56<>\"\"),Inputs!T56,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L90<>\"\"),Inputs!R90,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L124<>\"\"),Inputs!Q124,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J158<>\"\"),Inputs!O158,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N57<>\"\"),Inputs!N57,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L91<>\"\"),Inputs!L91,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L125<>\"\"),Inputs!L125,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J159<>\"\"),Inputs!J159,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N57<>\"\"),Inputs!BD57,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L91<>\"\"),Inputs!BL91,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L125<>\"\"),Inputs!BH125,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J159<>\"\"),Inputs!BH159,\"\"))))","v":""},null,null,{"$f":"Q42*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY57,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC91,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY125,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY159,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY57,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC91,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY125,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY159,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY57,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC91,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY125,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY159,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY57,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC91,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY125,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY159,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N57<>\"\"),Inputs!T57,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L91<>\"\"),Inputs!R91,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L125<>\"\"),Inputs!Q125,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J159<>\"\"),Inputs!O159,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N58<>\"\"),Inputs!N58,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L92<>\"\"),Inputs!L92,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L126<>\"\"),Inputs!L126,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J160<>\"\"),Inputs!J160,\"\"))))","v":""},null,null,null,null,null,null,null,null,"XXX",null,null,{"$error":"#VALUE!"},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N58<>\"\"),Inputs!BD58,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L92<>\"\"),Inputs!BL92,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L126<>\"\"),Inputs!BH126,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J160<>\"\"),Inputs!BH160,\"\"))))","v":""},null,null,{"$f":"Q43*(EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY58,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC92,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY126,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY160,\"\")))))^2+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY58,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC92,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY126,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY160,\"\")))))^2+1))/EXP(2.326*(LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY58,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC92,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY126,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY160,\"\")))))^2/No_Samples+1))^0.5-0.5*LN((IF($AP$3=\"New Direct to SP Waters\",Inputs!AY58,IF($AP$3=\"New Upstream of SP Waters\",Inputs!BC92,IF($AP$3=\"Expanding Direct to SP Waters\",Inputs!AY126,IF($AP$3=\"Expanding Upstream of SP Waters\",Inputs!AY160,\"\")))))^2/No_Samples+1)))","v":{"$error":"#VALUE!"}},null,null,{"$f":"Q43*2.5","v":{"$error":"#VALUE!"}},null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N58<>\"\"),Inputs!T58,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L92<>\"\"),Inputs!R92,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L126<>\"\"),Inputs!Q126,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J160<>\"\"),Inputs!O160,\"\"))))","v":""}]
[]
[]
[null,null,"Special Protection Summary Data"]
[]
[null,"Pollutants",null,null,null,null,null,null,null,null,"Median of Upstream",null,null,null,"WQ Objective",null,null,null,"Units"]
[]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N29<>\"\"),Inputs!N29,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L63<>\"\"),Inputs!L63,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L97<>\"\"),Inputs!L97,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J131<>\"\"),Inputs!J131,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N29<>\"\"),Inputs!AO29,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L63<>\"\"),Inputs!AO63,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L97<>\"\"),Inputs!AO97,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J131<>\"\"),Inputs!AO131,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N29<>\"\"),Inputs!AR29,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L63<>\"\"),Inputs!AR63,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L97<>\"\"),Inputs!AR97,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J131<>\"\"),Inputs!AR131,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N29<>\"\"),Inputs!T29,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L63<>\"\"),Inputs!R63,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L97<>\"\"),Inputs!Q97,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J131<>\"\"),Inputs!O131,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N30<>\"\"),Inputs!N30,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L64<>\"\"),Inputs!L64,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L98<>\"\"),Inputs!L98,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J132<>\"\"),Inputs!J132,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N30<>\"\"),Inputs!AO30,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L64<>\"\"),Inputs!AO64,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L98<>\"\"),Inputs!AO98,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J132<>\"\"),Inputs!AO132,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N30<>\"\"),Inputs!AR30,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L64<>\"\"),Inputs!AR64,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L98<>\"\"),Inputs!AR98,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J132<>\"\"),Inputs!AR132,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N30<>\"\"),Inputs!T30,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L64<>\"\"),Inputs!R64,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L98<>\"\"),Inputs!Q98,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J132<>\"\"),Inputs!O132,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N31<>\"\"),Inputs!N31,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L65<>\"\"),Inputs!L65,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L99<>\"\"),Inputs!L99,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J133<>\"\"),Inputs!J133,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N31<>\"\"),Inputs!AO31,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L65<>\"\"),Inputs!AO65,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L99<>\"\"),Inputs!AO99,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J133<>\"\"),Inputs!AO133,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N31<>\"\"),Inputs!AR31,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L65<>\"\"),Inputs!AR65,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L99<>\"\"),Inputs!AR99,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J133<>\"\"),Inputs!AR133,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N31<>\"\"),Inputs!T31,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L65<>\"\"),Inputs!R65,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L99<>\"\"),Inputs!Q99,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J133<>\"\"),Inputs!O133,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N32<>\"\"),Inputs!N32,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L66<>\"\"),Inputs!L66,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L100<>\"\"),Inputs!L100,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J134<>\"\"),Inputs!J134,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N32<>\"\"),Inputs!AO32,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L66<>\"\"),Inputs!AO66,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L100<>\"\"),Inputs!AO100,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J134<>\"\"),Inputs!AO134,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N32<>\"\"),Inputs!AR32,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L66<>\"\"),Inputs!AR66,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L100<>\"\"),Inputs!AR100,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J134<>\"\"),Inputs!AR134,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N32<>\"\"),Inputs!T32,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L66<>\"\"),Inputs!R66,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L100<>\"\"),Inputs!Q100,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J134<>\"\"),Inputs!O134,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N33<>\"\"),Inputs!N33,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L67<>\"\"),Inputs!L67,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L101<>\"\"),Inputs!L101,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J135<>\"\"),Inputs!J135,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N33<>\"\"),Inputs!AO33,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L67<>\"\"),Inputs!AO67,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L101<>\"\"),Inputs!AO101,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J135<>\"\"),Inputs!AO135,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N33<>\"\"),Inputs!AR33,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L67<>\"\"),Inputs!AR67,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L101<>\"\"),Inputs!AR101,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J135<>\"\"),Inputs!AR135,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N33<>\"\"),Inputs!T33,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L67<>\"\"),Inputs!R67,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L101<>\"\"),Inputs!Q101,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J135<>\"\"),Inputs!O135,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N34<>\"\"),Inputs!N34,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L68<>\"\"),Inputs!L68,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L102<>\"\"),Inputs!L102,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J136<>\"\"),Inputs!J136,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N34<>\"\"),Inputs!AO34,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L68<>\"\"),Inputs!AO68,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L102<>\"\"),Inputs!AO102,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J136<>\"\"),Inputs!AO136,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N34<>\"\"),Inputs!AR34,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L68<>\"\"),Inputs!AR68,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L102<>\"\"),Inputs!AR102,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J136<>\"\"),Inputs!AR136,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N34<>\"\"),Inputs!T34,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L68<>\"\"),Inputs!R68,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L102<>\"\"),Inputs!Q102,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J136<>\"\"),Inputs!O136,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N35<>\"\"),Inputs!N35,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L69<>\"\"),Inputs!L69,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L103<>\"\"),Inputs!L103,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J137<>\"\"),Inputs!J137,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N35<>\"\"),Inputs!AO35,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L69<>\"\"),Inputs!AO69,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L103<>\"\"),Inputs!AO103,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J137<>\"\"),Inputs!AO137,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N35<>\"\"),Inputs!AR35,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L69<>\"\"),Inputs!AR69,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L103<>\"\"),Inputs!AR103,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J137<>\"\"),Inputs!AR137,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N35<>\"\"),Inputs!T35,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L69<>\"\"),Inputs!R69,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L103<>\"\"),Inputs!Q103,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J137<>\"\"),Inputs!O137,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N36<>\"\"),Inputs!N36,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L70<>\"\"),Inputs!L70,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L104<>\"\"),Inputs!L104,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J138<>\"\"),Inputs!J138,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N36<>\"\"),Inputs!AO36,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L70<>\"\"),Inputs!AO70,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L104<>\"\"),Inputs!AO104,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J138<>\"\"),Inputs!AO138,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N36<>\"\"),Inputs!AR36,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L70<>\"\"),Inputs!AR70,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L104<>\"\"),Inputs!AR104,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J138<>\"\"),Inputs!AR138,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N36<>\"\"),Inputs!T36,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L70<>\"\"),Inputs!R70,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L104<>\"\"),Inputs!Q104,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J138<>\"\"),Inputs!O138,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N37<>\"\"),Inputs!N37,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L71<>\"\"),Inputs!L71,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L105<>\"\"),Inputs!L105,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J139<>\"\"),Inputs!J139,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N37<>\"\"),Inputs!AO37,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L71<>\"\"),Inputs!AO71,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L105<>\"\"),Inputs!AO105,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J139<>\"\"),Inputs!AO139,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N37<>\"\"),Inputs!AR37,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L71<>\"\"),Inputs!AR71,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L105<>\"\"),Inputs!AR105,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J139<>\"\"),Inputs!AR139,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N37<>\"\"),Inputs!T37,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L71<>\"\"),Inputs!R71,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L105<>\"\"),Inputs!Q105,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J139<>\"\"),Inputs!O139,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N38<>\"\"),Inputs!N38,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L72<>\"\"),Inputs!L72,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L106<>\"\"),Inputs!L106,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J140<>\"\"),Inputs!J140,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N38<>\"\"),Inputs!AO38,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L72<>\"\"),Inputs!AO72,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L106<>\"\"),Inputs!AO106,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J140<>\"\"),Inputs!AO140,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N38<>\"\"),Inputs!AR38,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L72<>\"\"),Inputs!AR72,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L106<>\"\"),Inputs!AR106,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J140<>\"\"),Inputs!AR140,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N38<>\"\"),Inputs!T38,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L72<>\"\"),Inputs!R72,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L106<>\"\"),Inputs!Q106,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J140<>\"\"),Inputs!O140,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N39<>\"\"),Inputs!N39,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L73<>\"\"),Inputs!L73,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L107<>\"\"),Inputs!L107,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J141<>\"\"),Inputs!J141,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N39<>\"\"),Inputs!AO39,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L73<>\"\"),Inputs!AO73,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L107<>\"\"),Inputs!AO107,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J141<>\"\"),Inputs!AO141,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N39<>\"\"),Inputs!AR39,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L73<>\"\"),Inputs!AR73,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L107<>\"\"),Inputs!AR107,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J141<>\"\"),Inputs!AR141,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N39<>\"\"),Inputs!T39,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L73<>\"\"),Inputs!R73,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L107<>\"\"),Inputs!Q107,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J141<>\"\"),Inputs!O141,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N40<>\"\"),Inputs!N40,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L74<>\"\"),Inputs!L74,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L108<>\"\"),Inputs!L108,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J142<>\"\"),Inputs!J142,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N40<>\"\"),Inputs!AO40,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L74<>\"\"),Inputs!AO74,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L108<>\"\"),Inputs!AO108,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J142<>\"\"),Inputs!AO142,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N40<>\"\"),Inputs!AR40,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L74<>\"\"),Inputs!AR74,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L108<>\"\"),Inputs!AR108,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J142<>\"\"),Inputs!AR142,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N40<>\"\"),Inputs!T40,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L74<>\"\"),Inputs!R74,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L108<>\"\"),Inputs!Q108,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J142<>\"\"),Inputs!O142,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N41<>\"\"),Inputs!N41,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L75<>\"\"),Inputs!L75,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L109<>\"\"),Inputs!L109,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J143<>\"\"),Inputs!J143,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N41<>\"\"),Inputs!AO41,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L75<>\"\"),Inputs!AO75,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L109<>\"\"),Inputs!AO109,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J143<>\"\"),Inputs!AO143,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N41<>\"\"),Inputs!AR41,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L75<>\"\"),Inputs!AR75,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L109<>\"\"),Inputs!AR109,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J143<>\"\"),Inputs!AR143,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N41<>\"\"),Inputs!T41,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L75<>\"\"),Inputs!R75,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L109<>\"\"),Inputs!Q109,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J143<>\"\"),Inputs!O143,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N42<>\"\"),Inputs!N42,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L76<>\"\"),Inputs!L76,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L110<>\"\"),Inputs!L110,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J144<>\"\"),Inputs!J144,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N42<>\"\"),Inputs!AO42,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L76<>\"\"),Inputs!AO76,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L110<>\"\"),Inputs!AO110,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J144<>\"\"),Inputs!AO144,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N42<>\"\"),Inputs!AR42,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L76<>\"\"),Inputs!AR76,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L110<>\"\"),Inputs!AR110,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J144<>\"\"),Inputs!AR144,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N42<>\"\"),Inputs!T42,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L76<>\"\"),Inputs!R76,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L110<>\"\"),Inputs!Q110,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J144<>\"\"),Inputs!O144,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N43<>\"\"),Inputs!N43,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L77<>\"\"),Inputs!L77,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L111<>\"\"),Inputs!L111,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J145<>\"\"),Inputs!J145,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N43<>\"\"),Inputs!AO43,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L77<>\"\"),Inputs!AO77,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L111<>\"\"),Inputs!AO111,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J145<>\"\"),Inputs!AO145,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N43<>\"\"),Inputs!AR43,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L77<>\"\"),Inputs!AR77,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L111<>\"\"),Inputs!AR111,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J145<>\"\"),Inputs!AR145,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N43<>\"\"),Inputs!T43,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L77<>\"\"),Inputs!R77,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L111<>\"\"),Inputs!Q111,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J145<>\"\"),Inputs!O145,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N44<>\"\"),Inputs!N44,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L78<>\"\"),Inputs!L78,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L112<>\"\"),Inputs!L112,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J146<>\"\"),Inputs!J146,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N44<>\"\"),Inputs!AO44,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L78<>\"\"),Inputs!AO78,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L112<>\"\"),Inputs!AO112,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J146<>\"\"),Inputs!AO146,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N44<>\"\"),Inputs!AR44,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L78<>\"\"),Inputs!AR78,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L112<>\"\"),Inputs!AR112,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J146<>\"\"),Inputs!AR146,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N44<>\"\"),Inputs!T44,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L78<>\"\"),Inputs!R78,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L112<>\"\"),Inputs!Q112,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J146<>\"\"),Inputs!O146,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N45<>\"\"),Inputs!N45,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L79<>\"\"),Inputs!L79,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L113<>\"\"),Inputs!L113,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J147<>\"\"),Inputs!J147,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N45<>\"\"),Inputs!AO45,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L79<>\"\"),Inputs!AO79,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L113<>\"\"),Inputs!AO113,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J147<>\"\"),Inputs!AO147,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N45<>\"\"),Inputs!AR45,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L79<>\"\"),Inputs!AR79,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L113<>\"\"),Inputs!AR113,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J147<>\"\"),Inputs!AR147,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N45<>\"\"),Inputs!T45,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L79<>\"\"),Inputs!R79,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L113<>\"\"),Inputs!Q113,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J147<>\"\"),Inputs!O147,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N46<>\"\"),Inputs!N46,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L80<>\"\"),Inputs!L80,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L114<>\"\"),Inputs!L114,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J148<>\"\"),Inputs!J148,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N46<>\"\"),Inputs!AO46,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L80<>\"\"),Inputs!AO80,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L114<>\"\"),Inputs!AO114,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J148<>\"\"),Inputs!AO148,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N46<>\"\"),Inputs!AR46,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L80<>\"\"),Inputs!AR80,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L114<>\"\"),Inputs!AR114,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J148<>\"\"),Inputs!AR148,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N46<>\"\"),Inputs!T46,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L80<>\"\"),Inputs!R80,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L114<>\"\"),Inputs!Q114,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J148<>\"\"),Inputs!O148,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N47<>\"\"),Inputs!N47,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L81<>\"\"),Inputs!L81,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L115<>\"\"),Inputs!L115,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J149<>\"\"),Inputs!J149,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N47<>\"\"),Inputs!AO47,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L81<>\"\"),Inputs!AO81,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L115<>\"\"),Inputs!AO115,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J149<>\"\"),Inputs!AO149,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N47<>\"\"),Inputs!AR47,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L81<>\"\"),Inputs!AR81,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L115<>\"\"),Inputs!AR115,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J149<>\"\"),Inputs!AR149,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N47<>\"\"),Inputs!T47,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L81<>\"\"),Inputs!R81,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L115<>\"\"),Inputs!Q115,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J149<>\"\"),Inputs!O149,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N48<>\"\"),Inputs!N48,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L82<>\"\"),Inputs!L82,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L116<>\"\"),Inputs!L116,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J150<>\"\"),Inputs!J150,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N48<>\"\"),Inputs!AO48,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L82<>\"\"),Inputs!AO82,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L116<>\"\"),Inputs!AO116,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J150<>\"\"),Inputs!AO150,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N48<>\"\"),Inputs!AR48,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L82<>\"\"),Inputs!AR82,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L116<>\"\"),Inputs!AR116,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J150<>\"\"),Inputs!AR150,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N48<>\"\"),Inputs!T48,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L82<>\"\"),Inputs!R82,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L116<>\"\"),Inputs!Q116,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J150<>\"\"),Inputs!O150,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N49<>\"\"),Inputs!N49,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L83<>\"\"),Inputs!L83,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L117<>\"\"),Inputs!L117,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J151<>\"\"),Inputs!J151,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N49<>\"\"),Inputs!AO49,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L83<>\"\"),Inputs!AO83,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L117<>\"\"),Inputs!AO117,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J151<>\"\"),Inputs!AO151,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N49<>\"\"),Inputs!AR49,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L83<>\"\"),Inputs!AR83,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L117<>\"\"),Inputs!AR117,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J151<>\"\"),Inputs!AR151,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N49<>\"\"),Inputs!T49,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L83<>\"\"),Inputs!R83,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L117<>\"\"),Inputs!Q117,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J151<>\"\"),Inputs!O151,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N50<>\"\"),Inputs!N50,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L84<>\"\"),Inputs!L84,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L118<>\"\"),Inputs!L118,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J152<>\"\"),Inputs!J152,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N50<>\"\"),Inputs!AO50,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L84<>\"\"),Inputs!AO84,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L118<>\"\"),Inputs!AO118,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J152<>\"\"),Inputs!AO152,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N50<>\"\"),Inputs!AR50,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L84<>\"\"),Inputs!AR84,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L118<>\"\"),Inputs!AR118,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J152<>\"\"),Inputs!AR152,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N50<>\"\"),Inputs!T50,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L84<>\"\"),Inputs!R84,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L118<>\"\"),Inputs!Q118,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J152<>\"\"),Inputs!O152,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N51<>\"\"),Inputs!N51,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L85<>\"\"),Inputs!L85,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L119<>\"\"),Inputs!L119,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J153<>\"\"),Inputs!J153,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N51<>\"\"),Inputs!AO51,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L85<>\"\"),Inputs!AO85,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L119<>\"\"),Inputs!AO119,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J153<>\"\"),Inputs!AO153,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N51<>\"\"),Inputs!AR51,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L85<>\"\"),Inputs!AR85,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L119<>\"\"),Inputs!AR119,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J153<>\"\"),Inputs!AR153,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N51<>\"\"),Inputs!T51,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L85<>\"\"),Inputs!R85,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L119<>\"\"),Inputs!Q119,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J153<>\"\"),Inputs!O153,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N52<>\"\"),Inputs!N52,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L86<>\"\"),Inputs!L86,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L120<>\"\"),Inputs!L120,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J154<>\"\"),Inputs!J154,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N52<>\"\"),Inputs!AO52,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L86<>\"\"),Inputs!AO86,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L120<>\"\"),Inputs!AO120,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J154<>\"\"),Inputs!AO154,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N52<>\"\"),Inputs!AR52,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L86<>\"\"),Inputs!AR86,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L120<>\"\"),Inputs!AR120,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J154<>\"\"),Inputs!AR154,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N52<>\"\"),Inputs!T52,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L86<>\"\"),Inputs!R86,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L120<>\"\"),Inputs!Q120,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J154<>\"\"),Inputs!O154,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N53<>\"\"),Inputs!N53,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L87<>\"\"),Inputs!L87,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L121<>\"\"),Inputs!L121,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J155<>\"\"),Inputs!J155,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N53<>\"\"),Inputs!AO53,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L87<>\"\"),Inputs!AO87,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L121<>\"\"),Inputs!AO121,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J155<>\"\"),Inputs!AO155,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N53<>\"\"),Inputs!AR53,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L87<>\"\"),Inputs!AR87,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L121<>\"\"),Inputs!AR121,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J155<>\"\"),Inputs!AR155,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N53<>\"\"),Inputs!T53,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L87<>\"\"),Inputs!R87,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L121<>\"\"),Inputs!Q121,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J155<>\"\"),Inputs!O155,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N54<>\"\"),Inputs!N54,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L88<>\"\"),Inputs!L88,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L122<>\"\"),Inputs!L122,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J156<>\"\"),Inputs!J156,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N54<>\"\"),Inputs!AO54,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L88<>\"\"),Inputs!AO88,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L122<>\"\"),Inputs!AO122,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J156<>\"\"),Inputs!AO156,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N54<>\"\"),Inputs!AR54,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L88<>\"\"),Inputs!AR88,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L122<>\"\"),Inputs!AR122,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J156<>\"\"),Inputs!AR156,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N54<>\"\"),Inputs!T54,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L88<>\"\"),Inputs!R88,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L122<>\"\"),Inputs!Q122,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J156<>\"\"),Inputs!O156,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N55<>\"\"),Inputs!N55,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L89<>\"\"),Inputs!L89,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L123<>\"\"),Inputs!L123,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J157<>\"\"),Inputs!J157,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N55<>\"\"),Inputs!AO55,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L89<>\"\"),Inputs!AO89,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L123<>\"\"),Inputs!AO123,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J157<>\"\"),Inputs!AO157,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N55<>\"\"),Inputs!AR55,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L89<>\"\"),Inputs!AR89,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L123<>\"\"),Inputs!AR123,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J157<>\"\"),Inputs!AR157,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N55<>\"\"),Inputs!T55,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L89<>\"\"),Inputs!R89,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L123<>\"\"),Inputs!Q123,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J157<>\"\"),Inputs!O157,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N56<>\"\"),Inputs!N56,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L90<>\"\"),Inputs!L90,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L124<>\"\"),Inputs!L124,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J158<>\"\"),Inputs!J158,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N56<>\"\"),Inputs!AO56,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L90<>\"\"),Inputs!AO90,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L124<>\"\"),Inputs!AO124,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J158<>\"\"),Inputs!AO158,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N56<>\"\"),Inputs!AR56,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L90<>\"\"),Inputs!AR90,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L124<>\"\"),Inputs!AR124,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J158<>\"\"),Inputs!AR158,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N56<>\"\"),Inputs!T56,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L90<>\"\"),Inputs!R90,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L124<>\"\"),Inputs!Q124,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J158<>\"\"),Inputs!O158,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N57<>\"\"),Inputs!N57,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L91<>\"\"),Inputs!L91,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L125<>\"\"),Inputs!L125,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J159<>\"\"),Inputs!J159,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N57<>\"\"),Inputs!AO57,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L91<>\"\"),Inputs!AO91,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L125<>\"\"),Inputs!AO125,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J159<>\"\"),Inputs!AO159,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N57<>\"\"),Inputs!AR57,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L91<>\"\"),Inputs!AR91,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L125<>\"\"),Inputs!AR125,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J159<>\"\"),Inputs!AR159,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N57<>\"\"),Inputs!T57,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L91<>\"\"),Inputs!R91,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L125<>\"\"),Inputs!Q125,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J159<>\"\"),Inputs!O159,\"\"))))","v":""}]
[null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N58<>\"\"),Inputs!N58,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L92<>\"\"),Inputs!L92,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L126<>\"\"),Inputs!L126,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J160<>\"\"),Inputs!J160,\"\"))))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N58<>\"\"),Inputs!AO58,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L92<>\"\"),Inputs!AO92,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L126<>\"\"),Inputs!AO126,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J160<>\"\"),Inputs!AO160,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N58<>\"\"),Inputs!AR58,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L92<>\"\"),Inputs!AR92,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L126<>\"\"),Inputs!AR126,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J160<>\"\"),Inputs!AR160,\"\"))))","v":""},null,null,null,{"$f":"IF(AND($AP$3=\"New Direct to SP Waters\",Inputs!N58<>\"\"),Inputs!T58,IF(AND($AP$3=\"New Upstream of SP Waters\",Inputs!L92<>\"\"),Inputs!R92,IF(AND($AP$3=\"Expanding Direct to SP Waters\",Inputs!L126<>\"\"),Inputs!Q126,IF(AND($AP$3=\"Expanding Upstream of SP Waters\",Inputs!J160<>\"\"),Inputs!O160,\"\"))))","v":""}]

{"sheet":"Site-Specific Data","index":3,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[]}
[null,null,null,"Parameter","Median","95% Upper Confidence Limit","Units","ND or <"]
[]
[null,null,null,"Total Dissolved Solids"]
[null,null,null,"Chloride"]
[null,null,null,"Bromide"]
[null,null,null,"Sulfate"]
[null,null,null,"Total Aluminum"]
[null,null,null,"Total Antimony"]
[null,null,null,"Total Arsenic"]
[null,null,null,"Total Barium"]
[null,null,null,"Total Beryllium"]
[null,null,null,"Total Boron"]
[null,null,null,"Total Cadmium"]
[null,null,null,"Total Chromium"]
[null,null,null,"Hexavalent Chromium"]
[null,null,null,"Total Cobalt"]
[null,null,null,"Total Copper"]
[null,null,null,"Free Available Cyanide"]
[null,null,null,"Total Cyanide"]
[null,null,null,"Dissolved Iron"]
[null,null,null,"Total Iron"]
[null,null,null,"Total Lead"]
[null,null,null,"Total Manganese"]
[null,null,null,"Total Mercury"]
[null,null,null,"Total Nickel"]
[null,null,null,"Total Phenols (Phenolics)"]
[null,null,null,"Total Selenium"]
[null,null,null,"Total Silver"]
[null,null,null,"Total Thallium"]
[null,null,null,"Total Zinc"]

{"sheet":"Versions","index":4,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Date","Version","Change(s)"]
["2024-04-03",1,"Original"]

{"sheet":"WQN0100","index":5,"n_rows":57,"n_cols":15,"rows_kept":57,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Alkalinity (Lab)","mg/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,15,16.600000000000001,18,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Aluminum Dissolved","ug/l","2019-04-25","2024-03-25",4.915300546448087,58,0.91305110027008896,null,15,15,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Aluminum Total","ug/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,61.7,85.2,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Ammonia as N Dissolved","mg/l","2020-10-21","2024-03-25",3.4262295081967209,42,0.9115704530122456,null,0.02,0.02,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Ammonia as N Total","mg/l","2019-04-25","2024-03-25",4.915300546448087,57,0.93726331964417142,null,0.02,0.02,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Barium Total","ug/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,33.6,35.200000000000003]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Boron Total","ug/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,200,200,"<"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Bromide Total","ug/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,25,25,"<"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Cadmium Dissolved","ug/l","2019-04-25","2024-03-25",4.915300546448087,58,0.91305110027008896,null,0.2,0.2,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Calcium Dissolved","mg/l","2020-10-21","2024-03-25",3.4262295081967209,42,0.9115704530122456,null,5.8449999999999998,6.21]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Calcium Total","mg/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,5.9,6.2789999999999999,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Carbon Dioxide Total","mg/l","2020-10-21","2024-01-24",3.2595628415300548,38,0.92704861148376938,null,22.6,25]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Carbon Dissolved Organic","mg/l","2020-10-21","2024-02-28",3.3551912568306008,41,0.94041611198190356,null,1.35,1.53]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Carbon Total Organic","mg/l","2020-10-21","2024-02-28",3.3551912568306008,41,0.94041611198190356,null,1.29,1.43]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2019-04-25","2024-03-25",4.915300546448087,56,0.91857318539049337,null,1.1000000000000001,1.4,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Chloride Total","mg/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,11,11.21,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Coliform Fecal","cf/100ml","2019-05-28","2024-03-25",4.8251366120218577,53,0.90162935155950785,null,25,25,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Copper Dissolved","ug/l","2019-04-25","2024-03-25",4.915300546448087,58,0.91305110027008896,null,4,4,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Copper Total","ug/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Dissolved Oxygen (Field)","mg/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,9.6999999999999993,10.36]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Dissolved Solids Total","mg/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,66,68,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","E. Coli","cf/100ml","2019-05-28","2024-03-25",4.8251366120218577,52,0.9296057789329375,null,25,25,"<"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Hardness Total","mg/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,25,26,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Iron Dissolved","ug/l","2019-04-25","2024-03-25",4.915300546448087,58,0.91305110027008896,null,100,100,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Iron Total","ug/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,107,153,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Lead Dissolved","ug/l","2019-04-25","2024-03-25",4.915300546448087,58,0.91305110027008896,null,1,1,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Lead Total","ug/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,1,1,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Lithium Dissolved","ug/l","2019-04-25","2024-03-25",4.915300546448087,58,0.91305110027008896,null,25,25,"<"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Lithium Total","ug/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,25,25,"<"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Magnesium Dissolved","mg/l","2020-10-21","2024-03-25",3.4262295081967209,42,0.9115704530122456,null,2.54,2.63]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Magnesium Total","mg/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,2.5299999999999998,2.59]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Manganese Dissolved","ug/l","2019-04-25","2024-03-25",4.915300546448087,58,0.91305110027008896,null,3.11,3.73,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Manganese Total","ug/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,13.9,20.3,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Nickel Dissolved","ug/l","2019-04-25","2024-03-25",4.915300546448087,58,0.91305110027008896,null,8,8,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Nickel Total","ug/l","2019-04-25","2024-03-25",4.915300546448087,58,0.91305110027008896,null,8,8,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Nitrate + Nitrite as N Dissolved","mg/l","2020-10-21","2024-03-25",3.4262295081967209,41,0.94041611198190356,null,0.09,0.11,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Nitrate + Nitrite as N Total","mg/l","2020-10-21","2024-03-25",3.4262295081967209,42,0.9115704530122456,null,0.08,0.1,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Nitrate as N Total","mg/l","2019-04-25","2023-10-17",4.4781420765027322,17,0.950958251953125,null,0.12,0.16,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Nitrite as N Total","mg/l","2019-04-25","2023-10-17",4.4781420765027322,17,0.950958251953125,null,0.04,0.04,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Nitrogen Total","mg/l","2019-04-25","2024-03-25",4.915300546448087,58,0.91305110027008896,null,0.25,0.27,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Orthophosphate Dissolved","mg/l","2020-10-21","2024-03-25",3.4262295081967209,41,0.94041611198190356,null,0.01,1.2E-2,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Orthophosphate Total","mg/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,1.2E-2,1.2999999999999999E-2,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Osmotic Pressure","mosm/kg","2020-10-21","2024-03-25",3.4262295081967209,35,0.91046892106533028,null,1,1,"<"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","pH","ph units","2019-04-25","2024-03-25",4.915300546448087,59,0.96365682004294606,6.9849999999999994,7.0350000000000001,7.11]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Phosphorus Dissolved","mg/l","2020-10-21","2024-03-25",3.4262295081967209,42,0.9115704530122456,null,1.2999999999999999E-2,1.4E-2,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Phosphorus Total","mg/l","2019-04-25","2024-03-25",4.915300546448087,58,0.91305110027008896,null,1.7999999999999999E-2,2.1000000000000001E-2,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Potassium Total","mg/l","2019-04-25","2024-03-25",4.915300546448087,56,0.91857318539049337,null,1,1,"<"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Selenium Total","ug/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,7,7,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Sodium Total","mg/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,6.03,6.17]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Specific Conductance","umhos/cm","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,84.5,89.2]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Strontium Total","ug/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,24,24]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Sulfate Total","mg/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,6.76,6.99,null,"Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Suspended Solids Total","mg/l","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,20,20,"<","Y"]
["WQN0100","UNT Sixpenny","Upstr of Old Railroad Grade Tunnel","Temperature Water (Field)","c","2019-04-25","2024-03-25",4.915300546448087,59,0.93255538809921068,null,12.85,15.17]
["WQN0100","UNT Sixpenny","Dwnstr of Lobachsville Rd (SR1023) Br","Zinc Dissolved","ug/l","2019-04-25","2024-03-25",4.915300546448087,58,0.91305110027008896,null,5.98,6.44,null,"Y"]
["WQN0100","UNT Sixpenny","Dwnstr of Lobachsville Rd (SR1023) Br","Zinc Total","ug/l","2019-04-25","2024-03-25",4.915300546448087,58,0.91305110027008896,null,8.1,8.8699999999999992,null,"Y"]

{"sheet":"WQN0178","index":6,"n_rows":55,"n_cols":15,"rows_kept":55,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Alkalinity (Lab)","mg/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,33.200000000000003,35.799999999999997,37.200000000000003,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Aluminum Dissolved","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,15,15,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Aluminum Total","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,31.65,41.2,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Ammonia as N Dissolved","mg/l","2020-10-27","2024-03-18",3.3907103825136611,41,0.94041611198190356,null,0.02,0.02,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Ammonia as N Total","mg/l","2019-04-25","2024-03-18",4.8961748633879782,57,0.93726331964417142,null,0.02,0.02,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Barium Total","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,23.3,25.1]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Boron Total","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,200,200,"<"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Bromide Total","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,25,25,"<"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Cadmium Dissolved","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,0.2,0.2,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Calcium Dissolved","mg/l","2020-10-27","2024-03-18",3.3907103825136611,41,0.94041611198190356,null,11.2,12.28]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Calcium Total","mg/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,11.585000000000001,12.13,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Carbon Dioxide Total","mg/l","2020-10-27","2024-01-24",3.2431693989071042,38,0.92704861148376938,null,39.549999999999997,42.8]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Carbon Dissolved Organic","mg/l","2020-10-27","2024-03-18",3.3907103825136611,39,0.94674808590207227,null,1.91,2.34]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Carbon Total Organic","mg/l","2020-10-27","2024-03-18",3.3907103825136611,40,0.91930953224800727,null,1.94,2.2599999999999998]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2019-04-25","2024-03-18",4.8961748633879782,57,0.93726331964417142,null,0.84,1.1000000000000001,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Chloride Total","mg/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,12.065,12.71,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Coliform Fecal","cf/100ml","2019-05-29","2024-03-18",4.8032786885245899,54,0.92409527051089835,null,73.5,100,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Copper Dissolved","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,4,4,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Copper Total","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,4,4,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Dissolved Oxygen (Field)","mg/l","2019-04-25","2024-03-18",4.8961748633879782,57,0.93726331964417142,10.11,10.62]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Dissolved Solids Total","mg/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,98,102,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","E. Coli","cf/100ml","2019-05-29","2024-03-18",4.8032786885245899,53,0.90162935155950785,null,75,100]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Hardness Total","mg/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,46,48,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Iron Dissolved","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,100,100,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Iron Total","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,100,100,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Lead Dissolved","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,1,1,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Lead Total","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,1,1,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Lithium Dissolved","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,25,25,"<"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Lithium Total","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,25,25,"<"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Magnesium Dissolved","mg/l","2020-10-27","2024-03-18",3.3907103825136611,41,0.94041611198190356,null,4.2,4.5]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Magnesium Total","mg/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,4.1449999999999996,4.3600000000000003]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Manganese Dissolved","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,3.7450000000000001,4.0999999999999996,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Manganese Total","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,5.09,5.91,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Nickel Dissolved","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,8,8,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Nickel Total","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,8,8,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Nitrate + Nitrite as N Dissolved","mg/l","2020-10-27","2024-03-18",3.3907103825136611,41,0.94041611198190356,null,0.6,0.72,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Nitrate + Nitrite as N Total","mg/l","2020-10-27","2024-03-18",3.3907103825136611,41,0.94041611198190356,null,0.61,0.72,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Nitrogen Total","mg/l","2019-04-25","2024-03-18",4.8961748633879782,57,0.93726331964417142,null,0.76,0.84,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Orthophosphate Dissolved","mg/l","2020-10-27","2024-03-18",3.3907103825136611,41,0.94041611198190356,null,0.01,1.2999999999999999E-2,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Orthophosphate Total","mg/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,1.2E-2,1.2999999999999999E-2,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Osmotic Pressure","mosm/kg","2020-10-27","2024-03-18",3.3907103825136611,34,0.94238732708618034,null,1,1]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","pH","ph units","2019-04-25","2024-03-18",4.8961748633879782,58,0.95205967592833274,7.415,7.4849999999999994,7.6099999999999994]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Phosphorus Dissolved","mg/l","2020-10-27","2024-03-18",3.3907103825136611,41,0.94041611198190356,null,1.2E-2,1.4E-2,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Phosphorus Total","mg/l","2019-04-25","2024-03-18",4.8961748633879782,57,0.93726331964417142,null,1.4999999999999999E-2,1.7999999999999999E-2,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Potassium Total","mg/l","2019-04-25","2024-03-18",4.8961748633879782,55,0.94193585320759066,null,1.19,1.29]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Selenium Total","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,7,7,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Sodium Total","mg/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,7.84,8.0299999999999994]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Specific Conductance","umhos/cm","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,135.77500000000001,139.85]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Strontium Total","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,67.5,70]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Sulfate Total","mg/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,10.055,10.24,null,"Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Suspended Solids Total","mg/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,20,20,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Temperature Water (Field)","c","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,13,15.4]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Zinc Dissolved","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,5,5.79,"<","Y"]
["WQN0178","PINE CREEK","Dwnstr of Lobachsville Rd (SR1023) Br","Zinc Total","ug/l","2019-04-25","2024-03-18",4.8961748633879782,58,0.91305110027008896,null,5.5350000000000001,5.92,null,"Y"]

{"sheet":"WQN0181","index":7,"n_rows":54,"n_cols":15,"rows_kept":54,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Alkalinity (Lab)","mg/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,6,6.9,7.6,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Aluminum Dissolved","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,53.95,57.5,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Aluminum Total","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,75.55,89.2,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Ammonia as N Dissolved","mg/l","2020-11-17","2024-03-11",3.3142076502732238,40,0.91930953224800727,null,0.02,0.02,"<","Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Ammonia as N Total","mg/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,0.02,0.02,"<","Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Barium Total","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,10.85,11.7]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Boron Total","ug/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,200,200,"<"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Bromide Total","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,25,25,"<"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Cadmium Dissolved","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,0.2,0.2,"<","Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Calcium Dissolved","mg/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,3.32,3.57]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Calcium Total","mg/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,3.2909999999999999,3.5739999999999998,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Carbon Dissolved Organic","mg/l","2020-12-08","2024-03-11",3.2568306010928958,40,0.91930953224800727,null,5.45,7.3]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Carbon Total Organic","mg/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,5.32,6.78]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,1.21,1.4,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Chloride Total","mg/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,6.4050000000000002,6.86,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Coliform Fecal","cf/100ml","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,25,25,"<","Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Copper Dissolved","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,4,4,"<","Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Copper Total","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,4,4,"<","Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Dissolved Oxygen (Field)","mg/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,10.18,10.84]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Dissolved Solids Total","mg/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,44,50,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","E. Coli","cf/100ml","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,25,25,"<"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Hardness Total","mg/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,13,14,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Iron Dissolved","ug/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,103,131,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Iron Total","ug/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,172,194,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Lead Dissolved","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,1,1,"<","Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Lead Total","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,1,1,"<","Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Lithium Dissolved","ug/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,25,25,"<"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Lithium Total","ug/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,25,25,"<"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Magnesium Dissolved","mg/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,1.18,1.25]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Magnesium Total","mg/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,1.18,1.25]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Manganese Dissolved","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,8.17,10,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Manganese Total","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,33.950000000000003,42,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Nickel Dissolved","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,8,8,"<","Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Nickel Total","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,8,8,"<","Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Nitrate + Nitrite as N Dissolved","mg/l","2020-11-17","2024-03-11",3.3142076502732238,40,0.91930953224800727,null,7.0000000000000007E-2,0.08,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Nitrate + Nitrite as N Total","mg/l","2020-10-05","2024-03-11",3.4316939890710381,42,0.9115704530122456,null,7.0000000000000007E-2,0.08,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Nitrogen Total","mg/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,0.36,0.38,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Orthophosphate Dissolved","mg/l","2020-11-17","2024-03-11",3.3142076502732238,40,0.91930953224800727,null,0.01,0.01,"<","Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Orthophosphate Total","mg/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,0.01,0.01,"<","Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Osmotic Pressure","mosm/kg","2020-11-17","2024-03-11",3.3142076502732238,32,0.94989754026755691,null,1,1,"<"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","pH","ph units","2019-03-26","2024-03-11",4.9590163934426226,60,0.9726598661319219,6.5549999999999997,6.5774999999999997,6.6349999999999998]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Phosphorus Dissolved","mg/l","2020-11-17","2024-03-11",3.3142076502732238,40,0.91930953224800727,null,1.2E-2,1.4999999999999999E-2,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Phosphorus Total","mg/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,1.9E-2,2.1000000000000001E-2,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Potassium Total","mg/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,1,1,"<"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Selenium Total","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,7,7,"<","Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Sodium Total","mg/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,4.2,4.37]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Specific Conductance","umhos/cm","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,48.7,50.75]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Strontium Total","ug/l","2019-03-26","2024-03-11",4.9590163934426226,59,0.93255538809921068,null,14,15]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Sulfate Total","mg/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,4.4800000000000004,4.68,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Suspended Solids Total","mg/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,20,20,"<","Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Temperature Water (Field)","c","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,10.84,14.06]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Zinc Dissolved","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,5.3150000000000004,5.93,null,"Y"]
["WQN0181","Little Bushkill","Dwnstr of Sugar Mountain Rd (SR 2003) Br","Zinc Total","ug/l","2019-03-26","2024-03-11",4.9590163934426226,60,0.90753901892707578,null,6.8250000000000002,7.27,null,"Y"]

{"sheet":"WQN0183","index":8,"n_rows":55,"n_cols":15,"rows_kept":55,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Alkalinity (Lab)","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,17,20.2,22.4,null,"Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Aluminum Dissolved","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,15,15,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Aluminum Total","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,30.5,33.799999999999997,null,"Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Ammonia as N Dissolved","mg/l","2020-11-03","2024-03-12",3.3551912568306008,39,0.94674808590207227,null,0.02,0.02,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Ammonia as N Total","mg/l","2019-04-17","2024-03-12",4.9016393442622954,56,0.91857318539049337,null,0.02,0.02,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Barium Total","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,22.5,23.7]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Boron Total","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,200,200,"<"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Bromide Total","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,25,25,"<"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Cadmium Dissolved","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,0.2,0.2,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Calcium Dissolved","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,7.48,7.99]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Calcium Total","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,7.5039999999999996,8.0399999999999991,null,"Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Carbon Dioxide Total","mg/l","2020-11-03","2023-12-05",3.0874316939890711,34,0.94238732708618034,null,25.5,29]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Carbon Dissolved Organic","mg/l","2020-11-03","2024-03-12",3.3551912568306008,39,0.94674808590207227,null,2.0299999999999998,2.62]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Carbon Total Organic","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,2.08,2.35]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2019-04-17","2024-03-12",4.9016393442622954,56,0.91857318539049337,null,0.94,1.1000000000000001,null,"Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Chloride Total","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,3.5,3.73,null,"Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Coliform Fecal","cf/100ml","2019-04-17","2024-03-12",4.9016393442622954,54,0.92409527051089835,null,25,40,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Copper Dissolved","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,4,4,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Copper Total","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,4,4,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Dissolved Oxygen (Field)","mg/l","2019-04-17","2024-03-12",4.9016393442622954,58,0.91305110027008896,10.58,11.63]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Dissolved Solids Total","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,42,46,null,"Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","E. Coli","cf/100ml","2019-04-17","2024-03-12",4.9016393442622954,53,0.90162935155950785,null,25,40]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Hardness Total","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,21,23,null,"Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Iron Dissolved","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,100,100,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Iron Total","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,100,100,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Lead Dissolved","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,1,1,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Lead Total","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,1,1,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Lithium Dissolved","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,25,25,"<"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Lithium Total","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,25,25,"<"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Magnesium Dissolved","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,0.62,0.64]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Magnesium Total","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,0.63,0.65]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Manganese Dissolved","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,8,8.67,null,"Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Manganese Total","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,14.3,16.3,null,"Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Nickel Dissolved","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,8,8,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Nickel Total","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,8,8,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Nitrate + Nitrite as N Dissolved","mg/l","2020-11-03","2024-03-12",3.3551912568306008,39,0.94674808590207227,null,0.28000000000000003,0.34,null,"Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Nitrate + Nitrite as N Total","mg/l","2020-10-07","2024-03-12",3.4289617486338799,41,0.94041611198190356,null,0.27,0.34,null,"Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Nitrogen Total","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,0.4,0.44,null,"Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Orthophosphate Dissolved","mg/l","2020-11-03","2024-03-12",3.3551912568306008,40,0.91930953224800727,null,0.01,0.01,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Orthophosphate Total","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,0.01,0.01,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Osmotic Pressure","mosm/kg","2020-10-07","2024-03-12",3.4289617486338799,33,0.91985668754205108,null,1,1,"<"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","pH","ph units","2019-04-17","2024-03-12",4.9016393442622954,58,0.95205967592833274,6.8650000000000002,6.9674999999999994,7.02]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Phosphorus Dissolved","mg/l","2020-11-03","2024-03-12",3.3551912568306008,39,0.94674808590207227,null,0.01,0.01,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Phosphorus Total","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,1.0999999999999999E-2,1.2999999999999999E-2,null,"Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Potassium Total","mg/l","2019-04-17","2024-03-12",4.9016393442622954,55,0.94193585320759066,null,1,1,"<"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Selenium Total","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,7,7,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Sodium Total","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,2.62,2.86]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Specific Conductance","umhos/cm","2019-04-17","2024-03-12",4.9016393442622954,58,0.91305110027008896,null,58.25,62.3]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Strontium Total","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,18,20]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Sulfate Total","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,3.48,3.65,null,"Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Suspended Solids Total","mg/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,20,20,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Temperature Water (Field)","c","2019-04-17","2024-03-12",4.9016393442622954,58,0.91305110027008896,null,7.7900000000000009,9.65]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Zinc Dissolved","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,5,5,"<","Y"]
["WQN0183","East Branch Dyberry Creek","Upstr of Rt 4007 (Dug Rd) Br; above confl with W Br Dyberry Crk","Zinc Total","ug/l","2019-04-17","2024-03-12",4.9016393442622954,57,0.93726331964417142,null,5,5.25,"<","Y"]

{"sheet":"WQN0191","index":9,"n_rows":55,"n_cols":15,"rows_kept":55,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Alkalinity (Lab)","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,3.6,4,4.2,null,"Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Aluminum Dissolved","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,26.5,32.1,null,"Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Aluminum Total","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,41.8,50.2,null,"Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Ammonia as N Dissolved","mg/l","2020-11-16","2024-03-11",3.316939890710382,41,0.94041611198190356,null,0.02,0.02,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Ammonia as N Total","mg/l","2019-04-16","2024-03-11",4.9016393442622954,58,0.91305110027008896,null,0.02,0.02,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Barium Total","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,12.7,12.9]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Boron Total","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,200,200,"<"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Bromide Total","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,25,25,"<"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Cadmium Dissolved","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,0.2,0.2,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Calcium Dissolved","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,2.1800000000000002,2.23]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Calcium Total","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,2.1880000000000002,2.27,null,"Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Carbon Dioxide Total","mg/l","2020-11-16","2023-11-14",2.9945205479452048,35,0.91046892106533028,null,9.4,13]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Carbon Dissolved Organic","mg/l","2020-12-07","2024-03-11",3.2595628415300548,40,0.91930953224800727,null,0.94500000000000006,1.1299999999999999]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Carbon Total Organic","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,0.96,1.18]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,1.01,1.28,null,"Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Chloride Total","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,19.18,19.809999999999999,null,"Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Coliform Fecal","cf/100ml","2019-04-16","2024-03-11",4.9016393442622954,58,0.91305110027008896,null,25,25,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Copper Dissolved","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Copper Total","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Dissolved Oxygen (Field)","mg/l","2019-03-27","2024-03-11",4.9562841530054644,59,0.93255538809921068,10.32,11.15]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Dissolved Solids Total","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,48,50,null,"Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","E. Coli","cf/100ml","2019-04-16","2024-03-11",4.9016393442622954,57,0.93726331964417142,null,25,25,"<"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Hardness Total","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,9,9,null,"Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Iron Dissolved","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,100,100,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Iron Total","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,100,100,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Lead Dissolved","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,1,1,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Lead Total","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,1,1,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Lithium Dissolved","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,25,25,"<"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Lithium Total","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,25,25,"<"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Magnesium Dissolved","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,0.81,0.85]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Magnesium Total","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,0.82,0.85]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Manganese Dissolved","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,2.66,3.04,null,"Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Manganese Total","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,7.22,9.68,null,"Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Nickel Dissolved","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,8,8,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Nickel Total","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,8,8,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Nitrate + Nitrite as N Dissolved","mg/l","2020-11-16","2024-03-11",3.316939890710382,40,0.91930953224800727,null,0.05,0.05,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Nitrate + Nitrite as N Total","mg/l","2020-10-05","2024-03-11",3.4316939890710381,42,0.9115704530122456,null,0.05,0.05,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Nitrogen Total","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,0.25,0.25,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Orthophosphate Dissolved","mg/l","2020-11-16","2024-03-11",3.316939890710382,40,0.91930953224800727,null,0.01,0.01,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Orthophosphate Total","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,0.01,0.01,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Osmotic Pressure","mosm/kg","2020-12-07","2024-03-11",3.2595628415300548,33,0.91985668754205108,null,1,1,"<"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","pH","ph units","2019-03-27","2024-03-11",4.9562841530054644,60,0.9726598661319219,6.3450000000000006,6.4149999999999991,6.5250000000000004]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Phosphorus Dissolved","mg/l","2020-11-16","2024-03-11",3.316939890710382,41,0.94041611198190356,null,0.01,0.01,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Phosphorus Total","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,0.01,0.01,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Potassium Total","mg/l","2019-04-16","2024-03-11",4.9016393442622954,57,0.93726331964417142,null,1,1,"<"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Selenium Total","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,7,7,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Sodium Total","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,10.3,10.49]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Specific Conductance","umhos/cm","2019-03-27","2024-03-11",4.9562841530054644,60,0.90753901892707578,null,76.825000000000003,78.55]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Strontium Total","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,10,10,"<"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Sulfate Total","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,1.75,1.83,null,"Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Suspended Solids Total","mg/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,20,20,"<","Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Temperature Water (Field)","c","2019-03-27","2024-03-11",4.9562841530054644,59,0.93255538809921068,null,8.36,11.9]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Zinc Dissolved","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,12.3,13.7,null,"Y"]
["WQN0191","WILD CREEK","1st Br Upstr of Penn Forest Res T482","Zinc Total","ug/l","2019-04-16","2024-03-11",4.9016393442622954,59,0.93255538809921068,null,13.4,14.7,null,"Y"]

{"sheet":"WQN0195","index":10,"n_rows":41,"n_cols":15,"rows_kept":41,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0195","Rock Run","Old SR23 Br","Alkalinity (Lab)","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,27,28.2,29.6,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Aluminum Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,10,10,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Aluminum Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,67,83.9,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Ammonia as N Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,0.02,0.02,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Arsenic Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Barium Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,26.6,27.1]
["WQN0195","Rock Run","Old SR23 Br","Cadmium Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,0.2,0.2,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Calcium Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,9.3699999999999992,9.8000000000000007,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2005-09-26","2010-09-20",4.9835616438356167,60,0.90753901892707578,null,0.91999999999999993,1.1000000000000001,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Chloride Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,9.4,9.83,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Coliform Fecal","cf/100ml","2005-09-26","2010-09-20",4.9835616438356167,59,0.93255538809921068,null,120,220,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Copper Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Copper Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Dissolved Oxygen (Field)","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,10.6,11.32]
["WQN0195","Rock Run","Old SR23 Br","Dissolved Solids Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,104,108,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Fluoride Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,0.2,0.2,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Hardness Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,41,43,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Iron Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,32,35,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Iron Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,155,174,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Lead Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,1,1,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Lead Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,1,1,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Magnesium Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,4.28,4.4349999999999996]
["WQN0195","Rock Run","Old SR23 Br","Manganese Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,6.6,7.4,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Manganese Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,10.9,12.7,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Nickel Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Nickel Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Nitrate as N Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,60,0.90753901892707578,null,1.175,1.3049999999999999,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Nitrite as N Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,60,0.90753901892707578,null,0.04,0.04,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Nitrogen Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,60,0.90753901892707578,null,1.2875000000000001,1.37,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Orthophosphate Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,60,0.90753901892707578,null,1.35E-2,1.4999999999999999E-2,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Osmotic Pressure","mosm/kg","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,2,2]
["WQN0195","Rock Run","Old SR23 Br","pH","ph units","2005-09-26","2010-09-20",4.9835616438356167,61,0.96038298510150011,7.4700000000000006,7.5449999999999999,7.6050000000000004]
["WQN0195","Rock Run","Old SR23 Br","Phenols Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,5,5,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Phosphorus Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,1.7999999999999999E-2,2.3E-2,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Specific Conductance","umhos/cm","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,124.15,129.44999999999999]
["WQN0195","Rock Run","Old SR23 Br","Sulfate Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,10.9,11.4,null,"Y"]
["WQN0195","Rock Run","Old SR23 Br","Suspended Solids Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,5,5,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Temperature Water (Field)","c","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,11.13,14.67]
["WQN0195","Rock Run","Old SR23 Br","Zinc Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,5,5,"<","Y"]
["WQN0195","Rock Run","Old SR23 Br","Zinc Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,5,5,"<","Y"]

{"sheet":"WQN0196","index":11,"n_rows":41,"n_cols":15,"rows_kept":41,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Alkalinity (Lab)","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,45.6,48,51,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Aluminum Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,10,10,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Aluminum Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,39.4,54.7,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Ammonia as N Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,0.02,0.02,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Arsenic Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Barium Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,23.1,24.7]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Cadmium Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,0.2,0.2,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Calcium Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,14.8,15.9,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2005-09-26","2010-09-20",4.9835616438356167,58,0.91305110027008896,null,0.9,1,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Chloride Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,10.8,12,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Coliform Fecal","cf/100ml","2005-09-26","2010-09-20",4.9835616438356167,58,0.91305110027008896,null,102.5,160,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Copper Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Copper Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Dissolved Oxygen (Field)","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,10.98,11.89]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Dissolved Solids Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,132,136,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Fluoride Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,0.2,0.2,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Hardness Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,64,69,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Iron Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,38,44,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Iron Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,148,172,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Lead Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,1,1,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Lead Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,1,1,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Magnesium Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,6.79,7.22]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Manganese Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,4.0999999999999996,4.5,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Manganese Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,6.9499999999999993,10.199999999999999,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Nickel Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Nickel Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Nitrate as N Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,60,0.90753901892707578,null,1.27,1.35,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Nitrite as N Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,60,0.90753901892707578,null,0.04,0.04,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Nitrogen Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,60,0.90753901892707578,null,1.42,1.48,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Orthophosphate Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,60,0.90753901892707578,null,1.2999999999999999E-2,1.4999999999999999E-2,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Osmotic Pressure","mosm/kg","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,2,3]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","pH","ph units","2005-09-26","2010-09-20",4.9835616438356167,61,0.96038298510150011,7.7,7.8150000000000004,7.89]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Phenols Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,5,5,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Phosphorus Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,2.1000000000000001E-2,2.3E-2,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Specific Conductance","umhos/cm","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,169.45,178]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Sulfate Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,11.2,11.5,null,"Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Suspended Solids Total","mg/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,5,5,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Temperature Water (Field)","c","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,9.49,12.78]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Zinc Dissolved","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,5,5,"<","Y"]
["WQN0196","WEST BR PERKIOMEN CRK","250 M upstr of Anthony's Mill Rd Br; along Forgedale Rd","Zinc Total","ug/l","2005-09-26","2010-09-20",4.9835616438356167,61,0.92782256149907727,null,5,5,"<","Y"]

{"sheet":"WQN0197","index":12,"n_rows":41,"n_cols":15,"rows_kept":41,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Alkalinity (Lab)","mg/l","2005-10-19","2010-09-13",4.9013698630136986,54,0.92409527051089835,4.5999999999999996,5,5.2,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Aluminum Dissolved","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,30.7,35.049999999999997,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Aluminum Total","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,46.05,55.3,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Ammonia as N Total","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,0.02,0.02,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Arsenic Dissolved","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,4,4,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Barium Total","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,18.3,18.7]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Cadmium Dissolved","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,0.2,0.2,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Calcium Total","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,3.54,3.64,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,0.9,1.1000000000000001,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Chloride Total","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,10.95,11.7,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Coliform Fecal","cf/100ml","2005-09-21","2010-09-13",4.978082191780822,56,0.91857318539049337,null,20,20,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Copper Dissolved","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,4,4,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Copper Total","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,4,4,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Dissolved Oxygen (Field)","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,11.16,11.68]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Dissolved Solids Total","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,60,64,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Fluoride Total","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,0.2,0.2,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Hardness Total","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,13,13,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Iron Dissolved","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,48.5,63,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Iron Total","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,83,95,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Lead Dissolved","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,1,1,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Lead Total","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,1,1,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Magnesium Total","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,1.0245,1.0509999999999999]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Manganese Dissolved","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,3.85,5.3,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Manganese Total","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,13.1,17.8,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Nickel Dissolved","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,4,4,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Nickel Total","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,4,4,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Nitrate as N Total","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,0.04,0.04,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Nitrite as N Total","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,0.04,0.04,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Nitrogen Total","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,0.18,0.21,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Orthophosphate Total","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,0.01,0.01,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Osmotic Pressure","mosm/kg","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,1,1,"<"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","pH","ph units","2005-09-21","2010-09-13",4.978082191780822,58,0.95205967592833274,6.7249999999999996,6.79,6.8949999999999996]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Phenols Total","ug/l","2005-09-21","2010-09-13",4.978082191780822,57,0.93726331964417142,null,5,5,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Phosphorus Total","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,1.4999999999999999E-2,1.6E-2,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Specific Conductance","umhos/cm","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,67.075000000000003,72.849999999999994]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Sulfate Total","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,6.1875,6.51,null,"Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Suspended Solids Total","mg/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,5,5,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Temperature Water (Field)","c","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,9.620000000000001,11.46]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Zinc Dissolved","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,5,5,"<","Y"]
["WQN0197","BLOOMING GROVE CRK","300 m upstr of T 494 Br","Zinc Total","ug/l","2005-09-21","2010-09-13",4.978082191780822,58,0.91305110027008896,null,5,5,"<","Y"]

{"sheet":"WQN0199","index":13,"n_rows":44,"n_cols":15,"rows_kept":44,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Alkalinity (Lab)","mg/l","2005-10-17","2010-09-13",4.9068493150684933,48,0.94053662474622968,5,5.4,6,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Aluminum Dissolved","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,23.7,30.4,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Aluminum Total","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,40.4,46.4,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Ammonia as N Total","mg/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,0.02,0.02,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Arsenic Dissolved","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Barium Total","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,22.4,23.1]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Cadmium Dissolved","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,0.2,0.2,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Calcium Dissolved","mg/l","2005-09-20","2010-09-13",4.9808219178082194,59,0.93255538809921068,null,3.99,4.1959999999999997]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Calcium Total","mg/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,4.03,4.29,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Carbon Total Organic","mg/l","2005-09-20","2010-09-13",4.9808219178082194,59,0.93255538809921068,null,2.2200000000000002,2.62]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2005-09-20","2010-09-13",4.9808219178082194,60,0.90753901892707578,null,0.9,1.2,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Chloride Total","mg/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,4.26,4.4400000000000004,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Coliform Fecal","cf/100ml","2005-09-20","2010-09-13",4.9808219178082194,59,0.93255538809921068,null,20,20,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Copper Dissolved","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Copper Total","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Dissolved Oxygen (Field)","mg/l","2005-09-20","2010-09-13",4.9808219178082194,60,0.90753901892707578,10.94,11.525]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Dissolved Solids Total","mg/l","2005-09-20","2010-09-13",4.9808219178082194,57,0.93726331964417142,null,46,50,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Fluoride Total","mg/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,0.2,0.2,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Hardness Total","mg/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,13,14,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Iron Dissolved","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,43,46,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Iron Total","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,90,103,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Lead Dissolved","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,1,1,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Lead Total","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,1,1,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Magnesium Dissolved","mg/l","2005-09-20","2010-09-13",4.9808219178082194,59,0.93255538809921068,null,0.71699999999999997,0.73799999999999999]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Magnesium Total","mg/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,0.73099999999999998,0.75600000000000001]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Manganese Dissolved","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,15.9,18.600000000000001,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Manganese Total","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,20,25.1,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Nickel Dissolved","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Nickel Total","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,4,4,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Nitrate as N Total","mg/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,0.08,0.1,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Nitrite as N Total","mg/l","2005-09-20","2010-09-13",4.9808219178082194,60,0.90753901892707578,null,0.04,0.04,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Nitrogen Total","mg/l","2005-10-17","2010-09-13",4.9068493150684933,59,0.93255538809921068,null,0.24,0.26,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Orthophosphate Total","mg/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,0.01,0.01,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Osmotic Pressure","mosm/kg","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,1,1,"<"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","pH","ph units","2005-09-20","2010-09-13",4.9808219178082194,60,0.9726598661319219,6.57,6.6950000000000003,6.76]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Phenols Total","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,5,5,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Phosphorus Total","mg/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,1.2999999999999999E-2,1.4E-2,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Specific Conductance","umhos/cm","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,45.35,47.5]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Sulfate Total","mg/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,5.8,5.93,null,"Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Suspended Solids Total","mg/l","2005-09-20","2010-09-13",4.9808219178082194,60,0.90753901892707578,null,5,5,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Temperature Water (Field)","c","2005-09-20","2010-09-13",4.9808219178082194,59,0.93255538809921068,null,10.08,14.02]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Zinc Dissolved","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,5,5,"<","Y"]
["WQN0199","KINTZ CREEK","20 m upstr of conf w/ Mozette Ck","Zinc Total","ug/l","2005-09-20","2010-09-13",4.9808219178082194,61,0.92782256149907727,null,5,5.0999999999999996,"<","Y"]

{"sheet":"WQN0275","index":14,"n_rows":41,"n_cols":15,"rows_kept":41,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Alkalinity (Lab)","mg/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,17.600000000000001,24,33.200000000000003,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Aluminum Dissolved","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,16.3,19.5,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Aluminum Total","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,60.349999999999987,67.400000000000006,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Ammonia as N Total","mg/l","2005-09-19","2010-09-01",4.9506849315068493,61,0.92782256149907727,null,0.02,0.02,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Arsenic Dissolved","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,4,4,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Barium Total","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,27.65,28.9]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Cadmium Dissolved","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,0.2,0.2,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Calcium Total","mg/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,7.9024999999999999,11.5,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,0.7,0.9,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Chloride Total","mg/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,1.5649999999999999,1.66,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Coliform Fecal","cf/100ml","2005-09-19","2010-09-01",4.9506849315068493,60,0.90753901892707578,null,40,40,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Copper Dissolved","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,4,4,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Copper Total","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,4,4,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Dissolved Oxygen (Field)","mg/l","2005-09-19","2010-08-02",4.8684931506849312,58,0.91305110027008896,10.45,11.28]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Dissolved Solids Total","mg/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,62,74,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Fluoride Total","mg/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,0.2,0.2,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Hardness Total","mg/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,27,38,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Iron Dissolved","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,31,36,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Iron Total","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,124,134,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Lead Dissolved","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,1,1,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Lead Total","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,1,1,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Magnesium Total","mg/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,1.91,2.3559999999999999]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Manganese Dissolved","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,14.4,15.4,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Manganese Total","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,18.649999999999999,21.5,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Nickel Dissolved","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,4,4,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Nickel Total","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,4,4,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Nitrate as N Total","mg/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,0.27,0.36,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Nitrite as N Total","mg/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,0.04,0.04,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Nitrogen Total","mg/l","2005-09-19","2010-09-01",4.9506849315068493,59,0.93255538809921068,null,0.39,0.46,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Orthophosphate Total","mg/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,0.01,0.01,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Osmotic Pressure","mosm/kg","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,1,1]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","pH","ph units","2005-09-19","2010-09-01",4.9506849315068493,62,0.96998413565093256,7.33,7.5125000000000002,7.6]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Phenols Total","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,5,5,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Phosphorus Total","mg/l","2005-09-19","2010-09-01",4.9506849315068493,61,0.92782256149907727,null,0.01,0.01,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Specific Conductance","umhos/cm","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,65.025000000000006,83.85]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Sulfate Total","mg/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,5.4349999999999996,5.54,null,"Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Suspended Solids Total","mg/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,5,5,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Temperature Water (Field)","c","2005-09-19","2010-09-01",4.9506849315068493,61,0.92782256149907727,null,10,13.6]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Zinc Dissolved","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,5,5,"<","Y"]
["WQN0275","CONODOGUINET CREEK","650 m upstr of SGL 76 Boundary","Zinc Total","ug/l","2005-09-19","2010-09-01",4.9506849315068493,62,0.90204555948049248,null,5,5,"<","Y"]

{"sheet":"WQN0276","index":15,"n_rows":41,"n_cols":15,"rows_kept":41,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Alkalinity (Lab)","mg/l","2005-09-08","2010-09-02",4.9835616438356167,60,0.90753901892707578,13.2,15.95,22.4,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Aluminum Dissolved","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,12.1,15.3,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Aluminum Total","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,48,55.4,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Ammonia as N Total","mg/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,0.02,0.02,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Arsenic Dissolved","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Barium Total","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,23.3,25.8]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Cadmium Dissolved","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,0.2,0.2,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Calcium Total","mg/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,6.2830000000000004,8.4990000000000006,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,0.5,0.7,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Chloride Total","mg/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,0.88,0.94,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Coliform Fecal","cf/100ml","2005-09-20","2010-09-02",4.9506849315068493,57,0.93726331964417142,null,20,40,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Copper Dissolved","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Copper Total","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Dissolved Oxygen (Field)","mg/l","2005-09-08","2010-09-02",4.9835616438356167,60,0.90753901892707578,10.56,11.255000000000001]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Dissolved Solids Total","mg/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,54,62,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Fluoride Total","mg/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,0.2,0.2,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Hardness Total","mg/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,22,29,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Iron Dissolved","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,22,28,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Iron Total","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,77,92,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Lead Dissolved","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,1,1,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Lead Total","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,1,1,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Magnesium Total","mg/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,1.665,1.79]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Manganese Dissolved","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,6.67,7.1,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Manganese Total","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,10.3,13.9,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Nickel Dissolved","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Nickel Total","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Nitrate as N Total","mg/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,0.26,0.3,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Nitrite as N Total","mg/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,0.04,0.04,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Nitrogen Total","mg/l","2005-09-08","2010-09-02",4.9835616438356167,60,0.90753901892707578,null,0.35,0.44,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Orthophosphate Total","mg/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,0.01,0.01,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Osmotic Pressure","mosm/kg","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,1,1,"<"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","pH","ph units","2005-09-08","2010-09-02",4.9835616438356167,60,0.9726598661319219,7.38,7.4950000000000001,7.55]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Phenols Total","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,5,5,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Phosphorus Total","mg/l","2005-09-08","2010-09-02",4.9835616438356167,60,0.90753901892707578,null,0.01,0.01,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Specific Conductance","umhos/cm","2005-09-08","2010-09-02",4.9835616438356167,60,0.90753901892707578,null,53.4,62.75]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Sulfate Total","mg/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,6.07,6.3849999999999998,null,"Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Suspended Solids Total","mg/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,5,5,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Temperature Water (Field)","c","2005-09-08","2010-09-02",4.9835616438356167,60,0.90753901892707578,null,10.44,12.67]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Zinc Dissolved","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,5,5,"<","Y"]
["WQN0276","EAST LICKING CREEK","First Br above Clearview Res on SR4002","Zinc Total","ug/l","2005-09-20","2010-09-02",4.9506849315068493,59,0.93255538809921068,null,5,5,"<","Y"]

{"sheet":"WQN0279","index":16,"n_rows":48,"n_cols":15,"rows_kept":48,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Alkalinity (Lab)","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,10.4,11.8,13.8,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Aluminum Dissolved","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,15,15,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Aluminum Total","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,41.9,57.1,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Ammonia as N Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,0.02,0.02,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Arsenic Dissolved","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,3,3,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Barium Total","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,46.1,48.8]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Boron Total","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,200,200,"<"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Bromide Total","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,25,25,"<"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Cadmium Dissolved","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,0.2,0.2,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Calcium Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,5.5640000000000001,6.4619999999999997,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,0.9,1.01,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Chloride Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,6.7,8.06,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Coliform Fecal","cf/100ml","2015-09-29","2020-09-15",4.9617486338797816,53,0.90162935155950785,null,25,25,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Copper Dissolved","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,4,4,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Copper Total","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,4,4,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Dissolved Oxygen (Field)","mg/l","2015-09-29","2020-09-15",4.9617486338797816,56,0.91857318539049337,10.48,11.205]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Dissolved Solids Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,58,60,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","E. Coli","cf/100ml","2015-11-17","2020-09-15",4.8278688524590168,50,0.93509135292772771,null,25,25]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Hardness Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,24,27,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Iron Dissolved","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,100,100,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Iron Total","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,100,110,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Lead Dissolved","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,1,1,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Lead Total","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,1,1,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Lithium Dissolved","ug/l","2016-03-15","2020-09-15",4.5041095890410956,50,0.93509135292772771,null,25,25,"<"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Lithium Total","ug/l","2016-03-15","2020-09-15",4.5041095890410956,50,0.93509135292772771,null,25,25,"<"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Magnesium Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,2.3519999999999999,2.66]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Manganese Dissolved","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,2.15,2.62,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Manganese Total","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,7.37,8.2799999999999994,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Nickel Dissolved","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,8,8,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Nickel Total","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,8,8,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Nitrate as N Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,0.99,1.07,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Nitrite as N Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,0.04,0.04,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Nitrogen Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,1.06,1.1399999999999999,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Orthophosphate Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,54,0.92409527051089835,null,1.6E-2,1.7999999999999999E-2,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Osmotic Pressure","mosm/kg","2015-09-29","2018-12-11",3.2,34,0.94238732708618034,null,1,1,"<"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","pH","ph units","2015-09-29","2020-09-15",4.9617486338797816,57,0.96685603221249439,7.335,7.4250000000000007,7.49]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Phosphorus Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,2.3E-2,2.5000000000000001E-2,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Potassium Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,1.1000000000000001,1.196]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Selenium Total","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,7,7,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Sodium Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,4.43,4.766]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Specific Conductance","umhos/cm","2015-09-29","2020-09-15",4.9617486338797816,57,0.93726331964417142,null,79,87.1]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Strontium Total","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,29,33]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Sulfate Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,8.51,8.7899999999999991,null,"Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Suspended Solids Total","mg/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,5,5,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Temperature Water (Field)","c","2015-09-29","2020-09-15",4.9617486338797816,57,0.93726331964417142,null,9.6,12.3]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Zinc Dissolved","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,5,5,"<","Y"]
["WQN0279","BOB'S CREEK","SR869 dwnstr of confl with Wallack's Br","Zinc Total","ug/l","2015-09-29","2020-09-15",4.9617486338797816,55,0.94193585320759066,null,5,5,"<","Y"]

{"sheet":"WQN0290","index":17,"n_rows":55,"n_cols":15,"rows_kept":55,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Alkalinity (Lab)","mg/l","2020-10-28","2024-01-30",3.2568306010928958,36,0.93475466477684654,13.8,15,16.600000000000001,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Aluminum Dissolved","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,15,15,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Aluminum Total","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,50,69,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Ammonia as N Dissolved","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,0.02,0.02,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Ammonia as N Total","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,0.02,0.02,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Barium Total","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,17.899999999999999,19.3]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Boron Total","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,200,200,"<"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Bromide Total","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,25,25,"<"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Cadmium Dissolved","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,0.2,0.2,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Calcium Dissolved","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,5.92,6.19]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Calcium Total","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,5.98,6.34,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Carbon Dioxide Total","mg/l","2020-10-28","2023-11-13",3.043715846994536,34,0.94238732708618034,null,19.350000000000001,21.2]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Carbon Dissolved Organic","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,2.13,2.2400000000000002]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Carbon Total Organic","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,2.13,2.31]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,1.5,1.95,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Chloride Total","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,0.67,0.69,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Coliform Fecal","cf/100ml","2020-10-28","2024-01-30",3.2568306010928958,36,0.93475466477684654,null,25,25,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Copper Dissolved","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,4,4,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Copper Total","ug/l","2020-10-28","2024-01-30",3.2568306010928958,36,0.93475466477684654,null,4,4,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Dissolved Oxygen (Field)","mg/l","2020-10-28","2024-04-03",3.4316939890710381,38,0.92704861148376938,10.029999999999999,10.71]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Dissolved Solids Total","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,32,37,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","E. Coli","cf/100ml","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,25,25,"<"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Hardness Total","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,18,20,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Iron Dissolved","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,100,100,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Iron Total","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,124,180,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Lead Dissolved","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,1,1,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Lead Total","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,1,1,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Lithium Dissolved","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,25,25,"<"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Lithium Total","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,25,25,"<"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Magnesium Dissolved","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,0.85,0.89]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Magnesium Total","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,0.87,0.91]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Manganese Dissolved","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,3.12,3.47,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Manganese Total","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,11.5,21.8,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Nickel Dissolved","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,8,8,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Nickel Total","ug/l","2020-10-28","2024-01-30",3.2568306010928958,36,0.93475466477684654,null,8,8,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Nitrate + Nitrite as N Dissolved","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,0.45,0.49,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Nitrate + Nitrite as N Total","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,0.45,0.49,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Nitrogen Total","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,0.64,0.75,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Orthophosphate Dissolved","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,0.01,0.01,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Orthophosphate Total","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,0.01,0.01,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Osmotic Pressure","mosm/kg","2020-10-28","2024-01-30",3.2568306010928958,30,0.90126285329461109,null,1,1,"<"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","pH","ph units","2020-10-28","2024-04-03",3.4316939890710381,38,0.96644756032037538,6.82,6.9224999999999994,6.9849999999999994]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Phosphorus Dissolved","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,0.01,0.01,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Phosphorus Total","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,1.2E-2,1.4999999999999999E-2,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Potassium Total","mg/l","2021-02-25","2024-01-30",2.9287671232876709,34,0.94238732708618034,null,1,1,"<"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Selenium Total","ug/l","2020-10-28","2024-01-30",3.2568306010928958,36,0.93475466477684654,null,7,7,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Sodium Total","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,0.81,0.86]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Specific Conductance","umhos/cm","2020-10-28","2024-04-03",3.4316939890710381,38,0.92704861148376938,null,41.724999999999987,43]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Strontium Total","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,15,16]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Sulfate Total","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,3.48,3.67,null,"Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Suspended Solids Total","mg/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,20,20,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Temperature Water (Field)","c","2020-10-28","2024-04-03",3.4316939890710381,38,0.92704861148376938,null,9.75,12.2]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Zinc Dissolved","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,5,5,"<","Y"]
["WQN0290","Sherman Creek","Along Big Valley Road (T-769)","Zinc Total","ug/l","2020-10-28","2024-01-30",3.2568306010928958,37,0.90112825040705469,null,5,5,"<","Y"]

{"sheet":"WQN0291","index":18,"n_rows":55,"n_cols":15,"rows_kept":55,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Alkalinity (Lab)","mg/l","2020-10-27","2024-03-21",3.3989071038251359,37,0.90112825040705469,9.1999999999999993,10.199999999999999,11.8,null,"Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Aluminum Dissolved","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,15,15,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Aluminum Total","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,46.75,59.1,null,"Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Ammonia as N Dissolved","mg/l","2020-10-27","2024-03-21",3.3989071038251359,37,0.90112825040705469,null,0.02,0.02,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Ammonia as N Total","mg/l","2020-10-27","2024-03-21",3.3989071038251359,37,0.90112825040705469,null,0.02,0.02,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Barium Total","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,29.05,30.7]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Boron Total","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,200,200,"<"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Bromide Total","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,25,25,"<"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Cadmium Dissolved","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,0.2,0.2,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Calcium Dissolved","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,3.2349999999999999,3.55]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Calcium Total","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,3.2444999999999999,3.59,null,"Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Carbon Dioxide Total","mg/l","2020-10-27","2023-11-13",3.0464480874316942,34,0.94238732708618034,null,14.85,18.5]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Carbon Dissolved Organic","mg/l","2020-10-27","2024-01-30",3.2595628415300548,37,0.90112825040705469,null,1.1299999999999999,1.31]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Carbon Total Organic","mg/l","2020-10-27","2024-01-30",3.2595628415300548,37,0.90112825040705469,null,1.19,1.31]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,1.07,1.34,null,"Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Chloride Total","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,0.64,0.66,null,"Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Coliform Fecal","cf/100ml","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,25,25,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Copper Dissolved","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,4,4,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Copper Total","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,4,4,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Dissolved Oxygen (Field)","mg/l","2020-10-27","2024-03-21",3.3989071038251359,39,0.94674808590207227,10.57,11.48]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Dissolved Solids Total","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,24,28,null,"Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","E. Coli","cf/100ml","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,25,25,"<"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Hardness Total","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,12,13,null,"Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Iron Dissolved","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,100,100,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Iron Total","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,100,100,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Lead Dissolved","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,1,1,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Lead Total","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,1,1,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Lithium Dissolved","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,25,25,"<"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Lithium Total","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,25,25,"<"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Magnesium Dissolved","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,0.87,0.96]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Magnesium Total","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,0.89,1]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Manganese Dissolved","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,2,2,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Manganese Total","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,4.415,5.63,null,"Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Nickel Dissolved","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,8,8,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Nickel Total","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,8,8,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Nitrate + Nitrite as N Dissolved","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,0.26500000000000001,0.32,null,"Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Nitrate + Nitrite as N Total","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,0.26500000000000001,0.33,null,"Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Nitrogen Total","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,0.375,0.43,null,"Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Orthophosphate Dissolved","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,0.01,0.01,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Orthophosphate Total","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,0.01,0.01,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Osmotic Pressure","mosm/kg","2020-10-27","2024-03-21",3.3989071038251359,30,0.90126285329461109,null,1,1,"<"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","pH","ph units","2020-10-27","2024-03-21",3.3989071038251359,39,0.97629729752952699,6.6849999999999996,6.82,6.875]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Phosphorus Dissolved","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,0.01,0.01,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Phosphorus Total","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,1.0999999999999999E-2,1.2E-2,null,"Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Potassium Total","mg/l","2020-12-29","2024-03-21",3.2267759562841531,36,0.93475466477684654,null,1,1,"<"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Selenium Total","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,7,7,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Sodium Total","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,0.89,0.95]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Specific Conductance","umhos/cm","2020-10-27","2024-03-21",3.3989071038251359,39,0.94674808590207227,null,29.5,31.7]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Strontium Total","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,13,14]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Sulfate Total","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,4.0150000000000006,4.1500000000000004,null,"Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Suspended Solids Total","mg/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,20,20,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Temperature Water (Field)","c","2020-10-27","2024-03-21",3.3989071038251359,39,0.94674808590207227,null,8.4,10.8]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Zinc Dissolved","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,5,5,"<","Y"]
["WQN0291","Faulkner Brook","Penn-York Road (T-780) 75 meters upstr of culvert","Zinc Total","ug/l","2020-10-27","2024-03-21",3.3989071038251359,38,0.92704861148376938,null,5,5,"<","Y"]

{"sheet":"WQN0292","index":19,"n_rows":55,"n_cols":15,"rows_kept":55,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Alkalinity (Lab)","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,3.8,3.9,4.2,null,"Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Aluminum Dissolved","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,15,15,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Aluminum Total","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,16.45,18.8,null,"Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Ammonia as N Dissolved","mg/l","2020-11-03","2024-03-20",3.377049180327869,39,0.94674808590207227,null,0.02,0.02,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Ammonia as N Total","mg/l","2020-11-03","2024-03-20",3.377049180327869,39,0.94674808590207227,null,0.02,0.02,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Barium Total","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,4.7450000000000001,5.0449999999999999]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Boron Total","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,200,200,"<"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Bromide Total","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,25,25,"<"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Cadmium Dissolved","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.2,0.2,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Calcium Dissolved","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.89,0.93]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Calcium Total","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.91700000000000004,0.95399999999999996,null,"Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Carbon Dioxide Total","mg/l","2020-11-03","2023-11-14",3.0300546448087431,36,0.93475466477684654,null,6.8000000000000007,8]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Carbon Dissolved Organic","mg/l","2020-11-03","2024-02-21",3.3005464480874318,38,0.92704861148376938,null,1,1,"<"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Carbon Total Organic","mg/l","2020-11-03","2024-02-21",3.3005464480874318,38,0.92704861148376938,null,1,1,"<"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.79500000000000004,1.095,null,"Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Chloride Total","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.88749999999999996,0.91,null,"Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Coliform Fecal","cf/100ml","2020-11-03","2024-03-20",3.377049180327869,39,0.94674808590207227,null,25,25,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Copper Dissolved","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,4,4,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Copper Total","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,4,4,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Dissolved Oxygen (Field)","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,10.71,11.025]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Dissolved Solids Total","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,20,20,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","E. Coli","cf/100ml","2020-11-03","2024-03-20",3.377049180327869,39,0.94674808590207227,null,25,25,"<"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Hardness Total","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,4,4,null,"Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Iron Dissolved","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,100,100,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Iron Total","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,100,100,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Lead Dissolved","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,1,1,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Lead Total","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,1,1,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Lithium Dissolved","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,25,25,"<"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Lithium Total","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,25,25,"<"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Magnesium Dissolved","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.51,0.51]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Magnesium Total","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.51,0.52]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Manganese Dissolved","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,2,2,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Manganese Total","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,3.4674999999999998,4.29,null,"Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Nickel Dissolved","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,8,8,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Nickel Total","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,8,8,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Nitrate + Nitrite as N Dissolved","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.05,0.05,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Nitrate + Nitrite as N Total","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.05,0.05,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Nitrogen Total","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.25,0.25,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Orthophosphate Dissolved","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.01,0.01,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Orthophosphate Total","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.01,0.01,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Osmotic Pressure","mosm/kg","2020-11-03","2024-03-20",3.377049180327869,35,0.91046892106533028,null,1,1,"<"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","pH","ph units","2020-11-03","2024-03-20",3.377049180327869,40,0.96152269171579974,6.3049999999999997,6.3849999999999998,6.4250000000000007]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Phosphorus Dissolved","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.01,0.01,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Phosphorus Total","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.01,0.01,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Potassium Total","mg/l","2021-01-25","2024-03-20",3.1502732240437159,37,0.90112825040705469,null,1,1,"<"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Selenium Total","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,7,7,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Sodium Total","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,0.70499999999999996,0.72]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Specific Conductance","umhos/cm","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,12.565,12.775]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Strontium Total","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,10,10,"<"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Sulfate Total","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,1.34,1.39,null,"Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Suspended Solids Total","mg/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,20,20,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Temperature Water (Field)","c","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,8.6499999999999986,10]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Zinc Dissolved","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,5,5,"<","Y"]
["WQN0292","Bowers Creek","Hypsy Gap Road (T-633), 75 meters upstr of culvert","Zinc Total","ug/l","2020-11-03","2024-03-20",3.377049180327869,40,0.91930953224800727,null,5,5,"<","Y"]

{"sheet":"WQN0294","index":20,"n_rows":52,"n_cols":15,"rows_kept":52,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Alkalinity (Lab)","mg/l","2020-10-08","2024-03-14",3.4316939890710381,36,0.93475466477684654,9.8000000000000007,13.1,15.4,null,"Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Aluminum Dissolved","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,15,15,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Aluminum Total","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,24.6,27.4,null,"Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Ammonia as N Dissolved","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,0.02,0.02,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Ammonia as N Total","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,0.02,0.02,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Barium Total","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,21.6,23]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Boron Total","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,200,200,"<"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Bromide Total","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,25,25,"<"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Cadmium Dissolved","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,0.2,0.2,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Calcium Dissolved","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,4.21,4.79]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Calcium Total","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,4.25,4.782,null,"Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Carbon Dissolved Organic","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,1.05,1.2250000000000001]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Carbon Total Organic","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,0.94,1.02]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,1.02,1.33,null,"Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Chloride Total","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,1.1599999999999999,1.3,null,"Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Copper Dissolved","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,4,4,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Copper Total","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,4,4,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Dissolved Oxygen (Field)","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,11,11.96]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Dissolved Solids Total","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,30,32,null,"Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Hardness Total","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,15,17,null,"Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Iron Dissolved","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,100,100,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Iron Total","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,100,100,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Lead Dissolved","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,1,1,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Lead Total","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,1,1,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Lithium Dissolved","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,25,25,"<"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Lithium Total","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,25,25,"<"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Magnesium Dissolved","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,1.03,1.1299999999999999]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Magnesium Total","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,1.03,1.1499999999999999]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Manganese Dissolved","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,2,2,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Manganese Total","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,2.4500000000000002,2.79,null,"Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Nickel Dissolved","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,8,8,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Nickel Total","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,8,8,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Nitrate + Nitrite as N Dissolved","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,0.08,0.11,null,"Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Nitrate + Nitrite as N Total","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,0.08,0.11,null,"Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Nitrogen Total","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,0.25,0.25,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Orthophosphate Dissolved","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,0.01,0.01,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Orthophosphate Total","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,0.01,0.01,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Osmotic Pressure","mosm/kg","2020-10-08","2024-03-14",3.4316939890710381,31,0.92924445401877165,null,1,1,"<"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","pH","ph units","2020-10-08","2024-03-14",3.4316939890710381,38,0.96644756032037538,6.8449999999999998,6.9625000000000004,7.0449999999999999]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Phosphorus Dissolved","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,1.0999999999999999E-2,1.2999999999999999E-2,null,"Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Phosphorus Total","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,1.0999999999999999E-2,1.2999999999999999E-2,null,"Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Potassium Total","mg/l","2020-10-08","2024-03-14",3.4316939890710381,36,0.93475466477684654,null,1,1,"<"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Selenium Total","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,7,7,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Sodium Total","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,1.1200000000000001,1.25]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Specific Conductance","umhos/cm","2020-10-08","2024-03-14",3.4316939890710381,38,0.92704861148376938,null,39.325000000000003,43.1]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Strontium Total","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,22,25]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Sulfate Total","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,5.56,5.74,null,"Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Suspended Solids Total","mg/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,20,20,"<","Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Temperature Water (Field)","c","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,7.1,10.9]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Zinc Dissolved","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,5.39,5.79,null,"Y"]
["WQN0294","Slate Run","About 500 ft upstr from confl with Pine Creek","Zinc Total","ug/l","2020-10-08","2024-03-14",3.4316939890710381,37,0.90112825040705469,null,5,5,"<","Y"]

{"sheet":"WQN0296","index":21,"n_rows":55,"n_cols":15,"rows_kept":55,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Alkalinity (Lab)","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,7.6,10.3,12,null,"Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Aluminum Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,17.05,18.5,null,"Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Aluminum Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,101.3,130,null,"Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Ammonia as N Dissolved","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.02,0.02,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Ammonia as N Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.02,0.02,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Barium Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,28.7,30.6]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Boron Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,200,200,"<"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Bromide Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,25,25,"<"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Cadmium Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.2,0.2,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Calcium Dissolved","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,3.1850000000000001,3.7]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Calcium Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,3.28,3.73,null,"Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Carbon Dioxide Total","mg/l","2020-10-14","2024-01-03",3.221311475409836,39,0.94674808590207227,null,14.9,18.100000000000001]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Carbon Dissolved Organic","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1.125,1.2749999999999999]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Carbon Total Organic","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1.1000000000000001,1.26]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1.1299999999999999,1.3,null,"Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Chloride Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.99,1.1000000000000001,null,"Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Coliform Fecal","cf/100ml","2020-10-14","2024-03-12",3.4098360655737712,41,0.94041611198190356,null,25,31.25,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Copper Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,4,4,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Copper Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,4,4,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Dissolved Oxygen (Field)","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,10.210000000000001,11.105]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Dissolved Solids Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,32,36,null,"Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","E. Coli","cf/100ml","2020-10-14","2024-03-12",3.4098360655737712,41,0.94041611198190356,null,25,50,"<"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Hardness Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,14,16,null,"Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Iron Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,100,100,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Iron Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,151,213,null,"Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Lead Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1,1,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Lead Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1,1,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Lithium Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,25,25,"<"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Lithium Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,25,25,"<"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Magnesium Dissolved","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1.38,1.51]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Magnesium Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1.3825000000000001,1.58]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Manganese Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,2,2.27,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Manganese Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,13.9,17.3,null,"Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Nickel Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,8,8,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Nickel Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,8,8,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Nitrate + Nitrite as N Dissolved","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.24,0.26,null,"Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Nitrate + Nitrite as N Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.24,0.26,null,"Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Nitrogen Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,41,0.94041611198190356,null,0.33,0.36,null,"Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Orthophosphate Dissolved","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.01,0.01,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Orthophosphate Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.01,0.01,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Osmotic Pressure","mosm/kg","2020-10-14","2024-03-12",3.4098360655737712,33,0.91985668754205108,null,1,1,"<"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","pH","ph units","2020-10-14","2024-03-12",3.4098360655737712,42,0.95644147807615809,6.6750000000000007,6.8075000000000001,6.89]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Phosphorus Dissolved","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.01,0.01,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Phosphorus Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.01,1.2E-2,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Potassium Total","mg/l","2021-01-12","2024-03-12",3.1639344262295079,39,0.94674808590207227,null,1,1,"<"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Selenium Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,7,7,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Sodium Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1.18,1.5]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Specific Conductance","umhos/cm","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,37.524999999999999,43.6]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Strontium Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,21,25]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Sulfate Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,7.65,7.91,null,"Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Suspended Solids Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,20,20,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Temperature Water (Field)","c","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,8.3500000000000014,11]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Zinc Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,5,5,"<","Y"]
["WQN0296","Sibbald Run","60 yds upstr of Rt 62 rd crossing","Zinc Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,5,5,"<","Y"]

{"sheet":"WQN0297","index":22,"n_rows":55,"n_cols":15,"rows_kept":55,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Alkalinity (Lab)","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,9.4,10.3,11.2,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Aluminum Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,23.8,25.65,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Aluminum Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,42.95,49.4,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Ammonia as N Dissolved","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.02,0.02,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Ammonia as N Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.02,0.02,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Barium Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,30.95,32.799999999999997]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Boron Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,200,200,"<"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Bromide Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,25,25,"<"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Cadmium Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.2,0.2,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Calcium Dissolved","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,4.2175000000000002,4.53]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Calcium Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,4.2650000000000006,4.5780000000000003,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Carbon Dioxide Total","mg/l","2020-10-14","2023-11-14",3.084699453551913,38,0.92704861148376938,null,15.55,18.8]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Carbon Dissolved Organic","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1.155,1.38]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Carbon Total Organic","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1.17,1.28]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1.2224999999999999,1.66,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Chloride Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1.83,1.92,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Coliform Fecal","cf/100ml","2020-10-14","2024-03-12",3.4098360655737712,41,0.94041611198190356,null,25,25,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Copper Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,4,4,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Copper Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,4,4,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Dissolved Oxygen (Field)","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,10.82,11.23]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Dissolved Solids Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,32,34,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","E. Coli","cf/100ml","2020-10-14","2024-03-12",3.4098360655737712,41,0.94041611198190356,null,25,25,"<"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Hardness Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,14.75,16,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Iron Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,100,100,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Iron Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,100,100,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Lead Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1,1,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Lead Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1,1,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Lithium Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,25,25,"<"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Lithium Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,25,25,"<"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Magnesium Dissolved","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.97750000000000004,1.08]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Magnesium Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.97,1.0900000000000001]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Manganese Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,8.1649999999999991,12.5,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Manganese Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,13.3,17,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Nickel Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,8,8,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Nickel Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,8,8,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Nitrate + Nitrite as N Dissolved","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.36499999999999999,0.4,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Nitrate + Nitrite as N Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.36499999999999999,0.4,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Nitrogen Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,41,0.94041611198190356,null,0.44,0.49,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Orthophosphate Dissolved","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.01,0.01,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Orthophosphate Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.01,0.01,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Osmotic Pressure","mosm/kg","2020-10-14","2024-03-12",3.4098360655737712,36,0.93475466477684654,null,1,1,"<"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","pH","ph units","2020-10-14","2024-03-12",3.4098360655737712,42,0.95644147807615809,6.6400000000000006,6.7549999999999999,6.88]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Phosphorus Dissolved","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.01,0.01,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Phosphorus Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,0.01,0.01,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Potassium Total","mg/l","2021-01-12","2024-03-12",3.1639344262295079,39,0.94674808590207227,null,1,1,"<"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Selenium Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,7,7,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Sodium Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,1.3525,1.57]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Specific Conductance","umhos/cm","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,41.975000000000001,43.95]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Strontium Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,21,23]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Sulfate Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,5.82,5.97,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Suspended Solids Total","mg/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,20,20,"<","Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Temperature Water (Field)","c","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,6.9499999999999993,9.6]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Zinc Dissolved","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,9.1849999999999987,10.3,null,"Y"]
["WQN0297","Stanton Brook","Stanton Brook Rd crossing","Zinc Total","ug/l","2020-10-14","2024-03-12",3.4098360655737712,42,0.9115704530122456,null,8.57,10.9,null,"Y"]

{"sheet":"WQN0409","index":23,"n_rows":54,"n_cols":15,"rows_kept":54,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Alkalinity (Lab)","mg/l","2019-04-08","2024-03-18",4.942622950819672,59,0.93255538809921068,12.4,13.4,17,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Aluminum Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,24,27.8,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Aluminum Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,48.55,57.6,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Ammonia as N Dissolved","mg/l","2021-01-27","2024-03-18",3.139344262295082,39,0.94674808590207227,null,0.02,0.02,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Ammonia as N Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,59,0.93255538809921068,null,0.02,0.02,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Barium Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,24.6,25.4]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Boron Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,200,200,"<"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Bromide Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,25,25,"<"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Cadmium Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,0.2,0.2,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Calcium Dissolved","mg/l","2021-01-27","2024-03-18",3.139344262295082,39,0.94674808590207227,null,6.82,7.26]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Calcium Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,6.9725000000000001,7.18,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Carbon Dissolved Organic","mg/l","2021-01-27","2024-03-18",3.139344262295082,39,0.94674808590207227,null,1.08,1.24]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Carbon Total Organic","mg/l","2021-01-27","2024-03-18",3.139344262295082,39,0.94674808590207227,null,1,1.1399999999999999]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2019-04-08","2024-03-18",4.942622950819672,59,0.93255538809921068,null,0.82,1.04,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Chloride Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,3.2749999999999999,3.45,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Coliform Fecal","cf/100ml","2019-04-08","2024-03-18",4.942622950819672,57,0.93726331964417142,null,25,25,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Copper Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,4,4,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Copper Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,4,4,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Dissolved Oxygen (Field)","mg/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,10.5,10.935]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Dissolved Solids Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,59,0.93255538809921068,null,46,48,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","E. Coli","cf/100ml","2019-04-08","2024-03-18",4.942622950819672,51,0.90808545018414566,null,25,40,"<"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Hardness Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,23,24,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Iron Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,100,100,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Iron Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,100,100,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Lead Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,1,1,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Lead Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,1,1,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Lithium Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,25,25,"<"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Lithium Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,25,25,"<"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Magnesium Dissolved","mg/l","2021-01-27","2024-03-18",3.139344262295082,39,0.94674808590207227,null,1.35,1.4]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Magnesium Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,1.365,1.41]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Manganese Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,12.2,14,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Manganese Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,15.85,18.3,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Nickel Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,8,8,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Nickel Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,8,8,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Nitrate + Nitrite as N Dissolved","mg/l","2021-01-27","2024-03-18",3.139344262295082,38,0.92704861148376938,null,0.51500000000000001,0.6,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Nitrate + Nitrite as N Total","mg/l","2021-01-27","2024-03-18",3.139344262295082,38,0.92704861148376938,null,0.51500000000000001,0.61,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Nitrogen Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,59,0.93255538809921068,null,0.62,0.67,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Orthophosphate Dissolved","mg/l","2021-01-27","2024-03-18",3.139344262295082,39,0.94674808590207227,null,0.01,0.01,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Orthophosphate Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,0.01,0.01,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Osmotic Pressure","mosm/kg","2020-10-27","2024-03-18",3.3907103825136611,36,0.93475466477684654,null,1,1,"<"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","pH","ph units","2019-04-08","2024-03-18",4.942622950819672,60,0.9726598661319219,6.83,6.8849999999999998,6.98]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Phosphorus Dissolved","mg/l","2021-01-27","2024-03-18",3.139344262295082,39,0.94674808590207227,null,0.01,0.01,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Phosphorus Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,59,0.93255538809921068,null,0.01,0.01,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Potassium Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,1,1,"<"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Selenium Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,7,7,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Sodium Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,2.3199999999999998,2.4]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Specific Conductance","umhos/cm","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,63.05,64.599999999999994]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Strontium Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,33.5,35]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Sulfate Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,7.4,7.65,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Suspended Solids Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,20,20,"<","Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Temperature Water (Field)","c","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,10.210000000000001,13.2]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Zinc Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,5.2200000000000006,6.06,null,"Y"]
["WQN0409","LYCOMING CREEK","T840 Br - Camp Susque (Nr Gray)","Zinc Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,60,0.90753901892707578,null,5.8650000000000002,7.37,null,"Y"]

{"sheet":"WQN0411","index":24,"n_rows":44,"n_cols":15,"rows_kept":44,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Alkalinity (Lab)","mg/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,20.2,22.3,26.4,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Aluminum Dissolved","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,16.95,20.100000000000001,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Aluminum Total","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,65.7,79.7,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Ammonia as N Total","mg/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,0.02,0.02,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Arsenic Dissolved","ug/l","2010-10-13","2015-09-16",4.9260273972602739,53,0.90162935155950785,null,3,3,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Barium Total","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,25.7,29]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Boron Total","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,200,200,"<"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Bromide Total","ug/l","2012-06-26","2015-09-16",3.224043715846995,35,0.91046892106533028,null,25,25,"<"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Cadmium Dissolved","ug/l","2010-10-13","2015-09-16",4.9260273972602739,53,0.90162935155950785,null,0.2,0.2,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Calcium Total","mg/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,9.6440000000000001,10.8,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,1.1000000000000001,1.2,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Chloride Total","mg/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,4.43,5.14,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Coliform Fecal","cf/100ml","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,10,18,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Copper Dissolved","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,4,4,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Copper Total","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,4,4,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Dissolved Oxygen (Field)","mg/l","2010-10-13","2015-09-16",4.9260273972602739,55,0.94193585320759066,10.74,11.66]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Dissolved Solids Total","mg/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,69,76,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Hardness Total","mg/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,34,37,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Iron Dissolved","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,27,31,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Iron Total","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,102,137,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Lead Dissolved","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,1,1,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Lead Total","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,1,1,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Magnesium Total","mg/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,2.3319999999999999,2.4510000000000001]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Manganese Dissolved","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,29.5,34,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Manganese Total","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,46.05,55.4,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Nickel Dissolved","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,4,4,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Nickel Total","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,4,4,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Nitrate as N Total","mg/l","2010-10-13","2015-09-16",4.9260273972602739,53,0.90162935155950785,null,0.24,0.32,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Nitrite as N Total","mg/l","2010-10-13","2015-09-16",4.9260273972602739,53,0.90162935155950785,null,0.04,0.04,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Nitrogen Total","mg/l","2010-10-13","2015-09-16",4.9260273972602739,53,0.90162935155950785,null,0.38,0.41,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Orthophosphate Total","mg/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,0.01,0.01,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Osmotic Pressure","mosm/kg","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,1,2]
["WQN0411","Pine Creek","T762 Br - Cedar Run","pH","ph units","2010-10-13","2015-09-16",4.9260273972602739,55,0.96997105458810751,7.41,7.5350000000000001,7.6550000000000002]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Phosphorus Total","mg/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,1.4E-2,1.4999999999999999E-2,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Selenium Total","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,7,7,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Sodium Total","mg/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,3.35,3.6360000000000001]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Specific Conductance","umhos/cm","2010-10-13","2015-09-16",4.9260273972602739,55,0.94193585320759066,null,97.85,107]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Strontium Total","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,35,39]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Sulfate Total","mg/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,13.44,14.04,null,"Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Suspended Solids Total","mg/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,5,5,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Temperature Water (Field)","c","2010-10-13","2015-09-16",4.9260273972602739,55,0.94193585320759066,null,9.6,13.93]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Zinc Dissolved","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,5,6.16,"<","Y"]
["WQN0411","Pine Creek","T762 Br - Cedar Run","Zinc Total","ug/l","2010-10-13","2015-09-16",4.9260273972602739,54,0.92409527051089835,null,7.0750000000000002,7.7,null,"Y"]

{"sheet":"WQN0428","index":25,"n_rows":47,"n_cols":15,"rows_kept":47,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Alkalinity (Lab)","mg/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,11.8,12.2,14.8,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Aluminum Dissolved","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,17.600000000000001,21.6,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Aluminum Total","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,33.4,43.4,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Ammonia as N Total","mg/l","2010-10-19","2015-09-16",4.9095890410958907,54,0.92409527051089835,null,0.02,0.02,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Arsenic Dissolved","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,3,3,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Barium Total","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,25.6,26.7]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Boron Total","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,200,200,"<"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Bromide Total","ug/l","2012-06-27","2015-09-16",3.221311475409836,35,0.91046892106533028,null,25,25,"<"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Cadmium Dissolved","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,0.2,0.2,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Calcium Dissolved","mg/l","2010-11-03","2015-09-16",4.8684931506849312,54,0.92409527051089835,null,6.6035000000000004,7.0369999999999999]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Calcium Total","mg/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,6.6239999999999997,7.1959999999999997,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Carbon Total Organic","mg/l","2010-11-03","2015-09-16",4.8684931506849312,53,0.90162935155950785,null,1.58,1.71]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2010-10-19","2015-09-16",4.9095890410958907,54,0.92409527051089835,null,1,1.2,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Chloride Total","mg/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,3.9,4.32,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Coliform Fecal","cf/100ml","2010-10-19","2015-09-16",4.9095890410958907,53,0.90162935155950785,null,10,18,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Copper Dissolved","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,4,4,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Copper Total","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,4,4,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Dissolved Oxygen (Field)","mg/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,9.93,11.11]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Dissolved Solids Total","mg/l","2010-10-19","2015-09-16",4.9095890410958907,54,0.92409527051089835,null,50,52,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Hardness Total","mg/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,21,22,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Iron Dissolved","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,20,20,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Iron Total","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,44,53,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Lead Dissolved","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,1,1,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Lead Total","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,1,1,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Magnesium Dissolved","mg/l","2010-11-03","2015-09-16",4.8684931506849312,54,0.92409527051089835,null,1.0725,1.1200000000000001]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Magnesium Total","mg/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,1.089,1.1379999999999999]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Manganese Dissolved","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,7.6,8.6999999999999993,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Manganese Total","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,10.73,13.3,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Nickel Dissolved","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,4,4,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Nickel Total","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,4,4,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Nitrate as N Total","mg/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,0.21,0.26,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Nitrite as N Total","mg/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,0.04,0.04,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Nitrogen Total","mg/l","2010-10-19","2015-09-16",4.9095890410958907,54,0.92409527051089835,null,0.32,0.34,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Orthophosphate Total","mg/l","2010-10-19","2015-09-16",4.9095890410958907,54,0.92409527051089835,null,0.01,0.01,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Osmotic Pressure","mosm/kg","2010-10-19","2015-09-16",4.9095890410958907,54,0.92409527051089835,null,1,1,"<"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","pH","ph units","2010-10-19","2015-09-16",4.9095890410958907,55,0.96997105458810751,7.2,7.2949999999999999,7.3949999999999996]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Phosphorus Total","mg/l","2010-10-19","2015-09-16",4.9095890410958907,54,0.92409527051089835,null,0.01,0.01,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Selenium Total","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,7,7,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Sodium Total","mg/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,2.5790000000000002,2.7320000000000002]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Specific Conductance","umhos/cm","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,63.15,67.650000000000006]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Strontium Total","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,37,39]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Sulfate Total","mg/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,7.43,7.54,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Suspended Solids Total","mg/l","2010-10-19","2015-09-16",4.9095890410958907,54,0.92409527051089835,null,5,5,"<","Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Temperature Water (Field)","c","2010-10-19","2015-09-16",4.9095890410958907,53,0.90162935155950785,null,11.5,14.68]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Zinc Dissolved","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,5.43,6.6,null,"Y"]
["WQN0428","LOYALSOCK CRK","SR 87 N of Hillsgrove","Zinc Total","ug/l","2010-10-19","2015-09-16",4.9095890410958907,55,0.94193585320759066,null,5.7,6.7,null,"Y"]

{"sheet":"WQN0443","index":26,"n_rows":47,"n_cols":15,"rows_kept":47,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Alkalinity (Lab)","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,6.4,7.3,8.1999999999999993,null,"Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Aluminum Dissolved","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,10,10,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Aluminum Total","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,20.7,23.1,null,"Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Ammonia as N Total","mg/l","2010-10-27","2015-09-02",4.8493150684931514,55,0.94193585320759066,null,0.02,0.02,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Arsenic Dissolved","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,3,3,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Barium Total","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,19.149999999999999,19.8]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Boron Total","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,200,200,"<"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Bromide Total","ug/l","2012-06-27","2015-09-02",3.183060109289618,36,0.93475466477684654,null,25,25,"<"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Cadmium Dissolved","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,0.2,0.2,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Calcium Dissolved","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,3.6469999999999998,4.0309999999999997]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Calcium Total","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,3.7364999999999999,3.89,null,"Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Carbon Total Organic","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,1,1]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,0.85000000000000009,1,null,"Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Chloride Total","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,1.2450000000000001,1.4,null,"Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Coliform Fecal","cf/100ml","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,10,10,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Copper Dissolved","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Copper Total","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Dissolved Oxygen (Field)","mg/l","2010-10-27","2015-09-02",4.8493150684931514,55,0.94193585320759066,10.89,11.31]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Dissolved Solids Total","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,35,38,null,"Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Hardness Total","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,13,14,null,"Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Iron Dissolved","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,20,20,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Iron Total","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,40,45,null,"Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Lead Dissolved","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Lead Total","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Magnesium Dissolved","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,0.89250000000000007,0.97399999999999998]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Magnesium Total","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,0.92500000000000004,0.97199999999999998]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Manganese Dissolved","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,2.25,2.7,null,"Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Manganese Total","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,4.9000000000000004,5.46,null,"Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Nickel Dissolved","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Nickel Total","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Nitrate as N Total","mg/l","2010-10-27","2015-09-02",4.8493150684931514,55,0.94193585320759066,null,0.2,0.2,null,"Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Nitrite as N Total","mg/l","2010-10-27","2015-09-02",4.8493150684931514,55,0.94193585320759066,null,0.04,0.04,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Nitrogen Total","mg/l","2010-10-27","2015-09-02",4.8493150684931514,55,0.94193585320759066,null,0.25,0.27,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Orthophosphate Total","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Osmotic Pressure","mosm/kg","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,1,1,"<"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","pH","ph units","2010-10-27","2015-09-02",4.8493150684931514,56,0.95595345389784914,6.8599999999999994,6.96,7.1]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Phosphorus Total","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Selenium Total","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,7,7,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Sodium Total","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,1.0155000000000001,1.0660000000000001]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Specific Conductance","umhos/cm","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,38.225000000000001,39.650000000000013]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Strontium Total","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,24,26]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Sulfate Total","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,6.49,6.57,null,"Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Suspended Solids Total","mg/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Temperature Water (Field)","c","2010-10-27","2015-09-02",4.8493150684931514,55,0.94193585320759066,null,9.6,11.95]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Zinc Dissolved","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0443","YOUNG WOMANS CRK","0.3 miles dwnstr of Laurelly Fork","Zinc Total","ug/l","2010-10-27","2015-09-02",4.8493150684931514,56,0.91857318539049337,null,5,5,"<","Y"]

{"sheet":"WQN0452","index":27,"n_rows":52,"n_cols":15,"rows_kept":52,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Alkalinity (Lab)","mg/l","2020-10-26","2024-03-14",3.3825136612021862,35,0.91046892106533028,189.6,192.4,198.8,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Aluminum Dissolved","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,15,15,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Aluminum Total","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,48.55,65.800000000000011,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Ammonia as N Dissolved","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,0.02,2.1000000000000001E-2,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Ammonia as N Total","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,0.02,0.02,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Barium Total","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,36.549999999999997,37.799999999999997]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Boron Total","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,200,200,"<"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Bromide Total","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,25,25,"<"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Cadmium Dissolved","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,0.2,0.2,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Calcium Dissolved","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,55.445,56.5]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Calcium Total","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,55.505000000000003,57.16,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Carbon Dissolved Organic","mg/l","2020-10-26","2024-03-14",3.3825136612021862,37,0.90112825040705469,null,1,1.06]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Carbon Total Organic","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,0.89,0.99]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,1.73,2.65,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Chloride Total","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,14.285,14.71,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Copper Dissolved","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,4,4,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Copper Total","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,4,4,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Dissolved Oxygen (Field)","mg/l","2020-10-26","2024-03-14",3.3825136612021862,38,0.92704861148376938,12.25,12.365]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Dissolved Solids Total","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,258,264,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Hardness Total","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,224.5,228,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Iron Dissolved","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,100,100,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Iron Total","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,100,156.5,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Lead Dissolved","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,1,1,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Lead Total","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,1,1,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Lithium Dissolved","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,25,25,"<"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Lithium Total","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,25,25,"<"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Magnesium Dissolved","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,20.55,20.94]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Magnesium Total","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,20.475000000000001,21.07]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Manganese Dissolved","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,4.76,6.07,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Manganese Total","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,8.2850000000000001,9.0950000000000006,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Nickel Dissolved","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,8,8,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Nickel Total","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,8,8,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Nitrate + Nitrite as N Dissolved","mg/l","2020-10-26","2024-03-14",3.3825136612021862,34,0.94238732708618034,null,3.8849999999999998,4.03,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Nitrate + Nitrite as N Total","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,3.8650000000000002,4.07,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Nitrogen Total","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,4.1349999999999998,4.2949999999999999,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Orthophosphate Dissolved","mg/l","2020-10-26","2024-03-14",3.3825136612021862,34,0.94238732708618034,null,1.0999999999999999E-2,1.2999999999999999E-2,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Orthophosphate Total","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,1.0999999999999999E-2,1.2E-2,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Osmotic Pressure","mosm/kg","2020-10-26","2024-03-14",3.3825136612021862,30,0.90126285329461109,null,5,5]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","pH","ph units","2020-10-26","2024-03-14",3.3825136612021862,37,0.95296897256048385,8.1649999999999991,8.1999999999999993,8.3249999999999993]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Phosphorus Dissolved","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,1.55E-2,1.7000000000000001E-2,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Phosphorus Total","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,2.35E-2,2.9499999999999998E-2,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Potassium Total","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,1.4,1.5]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Selenium Total","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,7,7,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Sodium Total","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,6.23,6.41]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Specific Conductance","umhos/cm","2020-10-26","2024-03-14",3.3825136612021862,38,0.92704861148376938,null,437.15,449.55]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Strontium Total","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,177.25,181]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Sulfate Total","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,15.515000000000001,15.75,null,"Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Suspended Solids Total","mg/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,20,20,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Temperature Water (Field)","c","2020-10-26","2024-03-14",3.3825136612021862,38,0.92704861148376938,null,9.9499999999999993,11.4]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Zinc Dissolved","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,5,5,"<","Y"]
["WQN0452","CEDAR RUN","0.5 mi upstr of SR 64 Br and 100 ft upstr of private BR","Zinc Total","ug/l","2020-10-26","2024-03-14",3.3825136612021862,36,0.93475466477684654,null,5.3249999999999993,6.15,null,"Y"]

{"sheet":"WQN0453","index":28,"n_rows":41,"n_cols":15,"rows_kept":41,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Alkalinity (Lab)","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,11,12.4,14.4,null,"Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Aluminum Dissolved","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,10,10,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Aluminum Total","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,19.7,25.7,null,"Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Ammonia as N Total","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,0.02,0.02,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Arsenic Dissolved","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Barium Total","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,21.7,24.3]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Cadmium Dissolved","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,0.2,0.2,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Calcium Total","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,5.5750000000000002,6.2439999999999998,null,"Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2005-10-26","2010-09-14",4.8849315068493153,58,0.91305110027008896,null,0.7,1,null,"Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Chloride Total","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,0.66,0.75,null,"Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Coliform Fecal","cf/100ml","2005-10-26","2010-09-14",4.8849315068493153,57,0.93726331964417142,null,20,20,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Copper Dissolved","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Copper Total","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Dissolved Oxygen (Field)","mg/l","2005-10-26","2010-09-14",4.8849315068493153,58,0.91305110027008896,11.03,11.74]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Dissolved Solids Total","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,44,50,null,"Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Fluoride Total","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,0.2,0.2,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Hardness Total","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,19,21,null,"Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Iron Dissolved","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,20,20,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Iron Total","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,20,23,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Lead Dissolved","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,1,1,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Lead Total","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,1,1,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Magnesium Total","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,1.1419999999999999,1.25]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Manganese Dissolved","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,2,2,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Manganese Total","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,2,2,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Nickel Dissolved","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Nickel Total","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Nitrate as N Total","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,0.08,0.1,null,"Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Nitrite as N Total","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,0.04,0.04,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Nitrogen Total","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,0.15,0.18,null,"Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Orthophosphate Total","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,1.2E-2,1.2999999999999999E-2,null,"Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Osmotic Pressure","mosm/kg","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,1,1,"<"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","pH","ph units","2005-10-26","2010-09-14",4.8849315068493153,59,0.96365682004294606,7.2200000000000006,7.34,7.41]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Phenols Total","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,5,5,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Phosphorus Total","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,1.6E-2,1.7999999999999999E-2,null,"Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Specific Conductance","umhos/cm","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,47.8,51.85]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Sulfate Total","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,7.45,7.57,null,"Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Suspended Solids Total","mg/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,5,5,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Temperature Water (Field)","c","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,8.73,12.36]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Zinc Dissolved","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,5,5,"<","Y"]
["WQN0453","CEDAR RUN","Most southern crossing of SR 3001","Zinc Total","ug/l","2005-10-26","2010-09-14",4.8849315068493153,59,0.93255538809921068,null,5,5,"<","Y"]

{"sheet":"WQN0454","index":29,"n_rows":41,"n_cols":15,"rows_kept":41,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Alkalinity (Lab)","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,10,11,13.4,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Aluminum Dissolved","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,10,10,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Aluminum Total","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,37.6,45.6,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Ammonia as N Total","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,0.02,0.02,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Arsenic Dissolved","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,4,4,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Barium Total","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,17.2,18.2]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Cadmium Dissolved","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,0.2,0.2,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Calcium Total","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,5.3639999999999999,5.9219999999999997,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,0.9,1,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Chloride Total","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,2.61,3.46,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Coliform Fecal","cf/100ml","2005-10-18","2010-09-22",4.9287671232876713,56,0.91857318539049337,null,20,20,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Copper Dissolved","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,4,4,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Copper Total","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,4,4,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Dissolved Oxygen (Field)","mg/l","2005-10-18","2010-09-22",4.9287671232876713,54,0.92409527051089835,11.19,11.89]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Dissolved Solids Total","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,52,62,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Fluoride Total","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,0.2,0.2,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Hardness Total","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,20,22,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Iron Dissolved","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,25,35,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Iron Total","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,128,146,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Lead Dissolved","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,1,1,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Lead Total","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,1,1,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Magnesium Total","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,1.5640000000000001,1.7190000000000001]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Manganese Dissolved","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,6.4,7.5,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Manganese Total","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,10.9,13.4,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Nickel Dissolved","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,4,4,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Nickel Total","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,4,4,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Nitrate as N Total","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,0.34,0.4,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Nitrite as N Total","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,0.04,0.04,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Nitrogen Total","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,0.41,0.46,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Orthophosphate Total","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,0.01,0.01,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Osmotic Pressure","mosm/kg","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,1,2]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","pH","ph units","2005-10-18","2010-09-22",4.9287671232876713,57,0.96685603221249439,7.165,7.2850000000000001,7.5500000000000007]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Phenols Total","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,5,5,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Phosphorus Total","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,1.2E-2,1.2999999999999999E-2,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Specific Conductance","umhos/cm","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,59.1,64]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Sulfate Total","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,8.09,8.3000000000000007,null,"Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Suspended Solids Total","mg/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,5,5,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Temperature Water (Field)","c","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,9.56,14.45]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Zinc Dissolved","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,5,5,"<","Y"]
["WQN0454","FIRST FORK SINNEMAHONING CRK","At Potter/Cameron Co Line","Zinc Total","ug/l","2005-10-18","2010-09-22",4.9287671232876713,57,0.93726331964417142,null,5,5,"<","Y"]

{"sheet":"WQN0455","index":30,"n_rows":41,"n_cols":15,"rows_kept":41,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Alkalinity (Lab)","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,10.4,12.6,20.6,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Aluminum Dissolved","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,10,10,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Aluminum Total","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,56.9,68.900000000000006,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Ammonia as N Total","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,0.02,0.02,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Arsenic Dissolved","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,4,4,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Barium Total","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,47.5,51.3]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Cadmium Dissolved","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,0.2,0.2,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Calcium Total","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,7.63,9.98,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,0.7,0.9,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Chloride Total","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,4.28,4.38,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Coliform Fecal","cf/100ml","2006-04-18","2010-09-28",4.4465753424657537,51,0.90808545018414566,null,40,60,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Copper Dissolved","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,4,4,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Copper Total","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,4,4,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Dissolved Oxygen (Field)","mg/l","2006-03-21","2010-09-28",4.5232876712328771,52,0.9296057789329375,9.5500000000000007,10.605]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Dissolved Solids Total","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,72,74,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Fluoride Total","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,0.2,0.2,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Hardness Total","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,31,38,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Iron Dissolved","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,30,33,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Iron Total","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,218,286,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Lead Dissolved","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,1,1,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Lead Total","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,1,1,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Magnesium Total","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,2.83,3.2839999999999998]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Manganese Dissolved","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,15.5,16,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Manganese Total","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,20.399999999999999,23.6,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Nickel Dissolved","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,4,4,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Nickel Total","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,4,4,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Nitrate as N Total","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,0.53,0.65,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Nitrite as N Total","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,0.04,0.04,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Nitrogen Total","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,0.64,0.73,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Orthophosphate Total","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,0.01,0.01,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Osmotic Pressure","mosm/kg","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,1,1,"<"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","pH","ph units","2006-03-21","2010-09-28",4.5232876712328771,53,0.97299168234627753,7.085,7.2149999999999999,7.51]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Phenols Total","ug/l","2006-03-21","2010-09-28",4.5232876712328771,52,0.9296057789329375,null,5,5,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Phosphorus Total","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,0.01,0.01,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Specific Conductance","umhos/cm","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,85,96.05]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Sulfate Total","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,14.7,15.2,null,"Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Suspended Solids Total","mg/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,5,5,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Temperature Water (Field)","c","2006-03-21","2010-09-28",4.5232876712328771,52,0.9296057789329375,null,7.5350000000000001,14.4]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Zinc Dissolved","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,5,5,"<","Y"]
["WQN0455","KILLBUCK RUN","0.85 strm miles upstrm of SR1021 Br","Zinc Total","ug/l","2006-03-21","2010-09-28",4.5232876712328771,53,0.90162935155950785,null,5,5,"<","Y"]

{"sheet":"WQN0456","index":31,"n_rows":47,"n_cols":15,"rows_kept":47,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Alkalinity (Lab)","mg/l","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,10,10.6,11.8,null,"Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Aluminum Dissolved","ug/l","2010-10-26","2015-09-01",4.8493150684931514,55,0.94193585320759066,null,10,10,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Aluminum Total","ug/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,27.5,30.1,null,"Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Ammonia as N Total","mg/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,0.02,0.02,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Arsenic Dissolved","ug/l","2010-10-26","2015-09-01",4.8493150684931514,55,0.94193585320759066,null,3,3,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Barium Total","ug/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,12.85,13.2]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Boron Total","ug/l","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,null,200,200,"<"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Bromide Total","ug/l","2012-06-27","2015-09-01",3.180327868852459,37,0.90112825040705469,null,25,25,"<"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Cadmium Dissolved","ug/l","2010-10-26","2015-09-01",4.8493150684931514,55,0.94193585320759066,null,0.2,0.2,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Calcium Dissolved","mg/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,4.9800000000000004,5.2270000000000003]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Calcium Total","mg/l","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,null,5.0039999999999996,5.3029999999999999,null,"Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Carbon Total Organic","mg/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,0.92500000000000004,1.01]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,0.9,1.1000000000000001,null,"Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Chloride Total","mg/l","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,null,1.74,1.93,null,"Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Coliform Fecal","cf/100ml","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,null,10,18,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Copper Dissolved","ug/l","2010-10-26","2015-09-01",4.8493150684931514,55,0.94193585320759066,null,4,4,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Copper Total","ug/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Dissolved Oxygen (Field)","mg/l","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,10.63,11.47]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Dissolved Solids Total","mg/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,43,46,null,"Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Hardness Total","mg/l","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,null,18,19,null,"Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Iron Dissolved","ug/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,20.5,23,null,"Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Iron Total","ug/l","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,null,119,136,null,"Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Lead Dissolved","ug/l","2010-10-26","2015-09-01",4.8493150684931514,55,0.94193585320759066,null,1,1,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Lead Total","ug/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Magnesium Dissolved","mg/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,1.2470000000000001,1.3089999999999999]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Magnesium Total","mg/l","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,null,1.2609999999999999,1.3380000000000001]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Manganese Dissolved","ug/l","2010-10-26","2015-09-01",4.8493150684931514,55,0.94193585320759066,null,8.6,10.5,null,"Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Manganese Total","ug/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,12.95,16.2,null,"Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Nickel Dissolved","ug/l","2010-10-26","2015-09-01",4.8493150684931514,55,0.94193585320759066,null,4,4,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Nickel Total","ug/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Nitrate as N Total","mg/l","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,null,0.46,0.5,null,"Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Nitrite as N Total","mg/l","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,null,0.04,0.04,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Nitrogen Total","mg/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,0.51500000000000001,0.56000000000000005,null,"Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Orthophosphate Total","mg/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Osmotic Pressure","mosm/kg","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,null,1,1,"<"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","pH","ph units","2010-10-26","2015-09-01",4.8493150684931514,57,0.96685603221249439,6.915,7.0250000000000004,7.165]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Phosphorus Total","mg/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Selenium Total","ug/l","2010-11-16","2015-09-01",4.7917808219178077,55,0.94193585320759066,null,7,7,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Sodium Total","mg/l","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,null,1.2529999999999999,1.345]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Specific Conductance","umhos/cm","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,null,47.15,50.15]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Strontium Total","ug/l","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,null,19,20]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Sulfate Total","mg/l","2010-10-26","2015-09-01",4.8493150684931514,57,0.93726331964417142,null,6.25,6.43,null,"Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Suspended Solids Total","mg/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Temperature Water (Field)","c","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,9.6900000000000013,12.8]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Zinc Dissolved","ug/l","2010-10-26","2015-09-01",4.8493150684931514,55,0.94193585320759066,null,5,5,"<","Y"]
["WQN0456","West Branch Pine Creek","Union St Br @ Galeton","Zinc Total","ug/l","2010-10-26","2015-09-01",4.8493150684931514,56,0.91857318539049337,null,5,5,"<","Y"]

{"sheet":"WQN0457","index":32,"n_rows":47,"n_cols":15,"rows_kept":47,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Alkalinity (Lab)","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,21.8,25.4,29,null,"Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Aluminum Dissolved","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,10,10,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Aluminum Total","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,23.2,27.7,null,"Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Ammonia as N Total","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,0.02,0.02,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Arsenic Dissolved","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,3,3,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Barium Total","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,31.25,34.700000000000003]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Boron Total","ug/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,200,200,"<"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Bromide Total","ug/l","2012-06-19","2015-09-14",3.237704918032787,38,0.92704861148376938,null,25,25,"<"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Cadmium Dissolved","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,0.2,0.2,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Calcium Dissolved","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,9.86,11.2]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Calcium Total","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,10.3,11.4,null,"Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Carbon Total Organic","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,1.3,1.44]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,0.8,1.1000000000000001,null,"Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Chloride Total","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,11.32,12.39,null,"Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Coliform Fecal","cf/100ml","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,18,20,null,"Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Copper Dissolved","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Copper Total","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Dissolved Oxygen (Field)","mg/l","2010-10-18","2015-09-14",4.9068493150684933,58,0.91305110027008896,10.81,11.28]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Dissolved Solids Total","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,74,78,null,"Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Hardness Total","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,32,36,null,"Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Iron Dissolved","ug/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,20,20,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Iron Total","ug/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,53,62,null,"Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Lead Dissolved","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Lead Total","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Magnesium Dissolved","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,1.524,1.752]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Magnesium Total","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,1.5349999999999999,1.7]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Manganese Dissolved","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,7.25,7.8,null,"Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Manganese Total","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,11.7,12.2,null,"Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Nickel Dissolved","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Nickel Total","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Nitrate as N Total","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,0.4,0.51,null,"Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Nitrite as N Total","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,0.04,0.04,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Nitrogen Total","mg/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,0.53,0.6,null,"Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Orthophosphate Total","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,0.01,0.01,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Osmotic Pressure","mosm/kg","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,1,3]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","pH","ph units","2010-10-18","2015-09-14",4.9068493150684933,58,0.95205967592833274,7.4,7.4875000000000007,7.5549999999999997]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Phosphorus Total","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,0.01,1.0999999999999999E-2,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Selenium Total","ug/l","2010-11-01","2015-09-14",4.8684931506849312,55,0.94193585320759066,null,7,7,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Sodium Total","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,6.31,7.4349999999999996]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Specific Conductance","umhos/cm","2010-10-18","2015-09-14",4.9068493150684933,58,0.91305110027008896,null,103.875,115.7]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Strontium Total","ug/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,40,48]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Sulfate Total","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,7.79,8.17,null,"Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Suspended Solids Total","mg/l","2010-10-18","2015-09-14",4.9068493150684933,57,0.93726331964417142,null,5,5,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Temperature Water (Field)","c","2010-10-18","2015-09-14",4.9068493150684933,58,0.91305110027008896,null,8.3949999999999996,12.59]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Zinc Dissolved","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0457","Blockhouse Creek","SR 284 Nr English Center","Zinc Total","ug/l","2010-10-18","2015-09-14",4.9068493150684933,56,0.91857318539049337,null,5,5.35,"<","Y"]

{"sheet":"WQN0458","index":33,"n_rows":55,"n_cols":15,"rows_kept":55,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Alkalinity (Lab)","mg/l","2019-04-08","2024-03-18",4.942622950819672,57,0.93726331964417142,9.8000000000000007,11.4,13.6,null,"Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Aluminum Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,15,15,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Aluminum Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,30.3,32.299999999999997,null,"Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Ammonia as N Dissolved","mg/l","2020-11-23","2024-03-18",3.316939890710382,40,0.91930953224800727,null,0.02,0.02,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Ammonia as N Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,57,0.93726331964417142,null,0.02,0.02,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Barium Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,20.6,21.3]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Boron Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,200,200,"<"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Bromide Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,25,25,"<"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Cadmium Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,0.2,0.2,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Calcium Dissolved","mg/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,4.6449999999999996,5.0599999999999996]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Calcium Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,4.6349999999999998,5.18,null,"Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Carbon Dioxide Total","mg/l","2020-11-23","2023-11-20",2.9917808219178079,27,0.94776101410388947,null,15.9,21.8]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Carbon Dissolved Organic","mg/l","2020-12-09","2024-03-18",3.2732240437158469,39,0.94674808590207227,null,1,1]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Carbon Total Organic","mg/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,1,1]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2019-04-08","2024-03-18",4.942622950819672,57,0.93726331964417142,null,0.75,0.9,null,"Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Chloride Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,1.4450000000000001,1.51,null,"Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Coliform Fecal","cf/100ml","2019-04-08","2024-03-18",4.942622950819672,55,0.94193585320759066,null,25,25,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Copper Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,4,4,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Copper Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,4,4,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Dissolved Oxygen (Field)","mg/l","2019-04-08","2024-03-18",4.942622950819672,59,0.93255538809921068,10.65,11.04]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Dissolved Solids Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,32,34,null,"Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","E. Coli","cf/100ml","2019-04-08","2024-03-18",4.942622950819672,49,0.91456686684260546,null,25,25,"<"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Hardness Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,15.5,17,null,"Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Iron Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,100,100,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Iron Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,100,100,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Lead Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,1,1,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Lead Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,1,1,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Lithium Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,25,25,"<"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Lithium Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,25,25,"<"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Magnesium Dissolved","mg/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,1.01,1.1000000000000001]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Magnesium Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,1.02,1.1000000000000001]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Manganese Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,2,2,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Manganese Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,4.875,5.58,null,"Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Nickel Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,8,8,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Nickel Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,8,8,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Nitrate + Nitrite as N Dissolved","mg/l","2020-11-23","2024-03-18",3.316939890710382,39,0.94674808590207227,null,0.26,0.3,null,"Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Nitrate + Nitrite as N Total","mg/l","2020-09-30","2024-03-18",3.4644808743169402,41,0.94041611198190356,null,0.27,0.3,null,"Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Nitrogen Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,57,0.93726331964417142,null,0.35,0.38,null,"Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Orthophosphate Dissolved","mg/l","2020-11-23","2024-03-18",3.316939890710382,40,0.91930953224800727,null,0.01,0.01,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Orthophosphate Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,0.01,0.01,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Osmotic Pressure","mosm/kg","2020-10-27","2024-03-18",3.3907103825136611,35,0.91046892106533028,null,1,1,"<"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","pH","ph units","2019-04-08","2024-03-18",4.942622950819672,59,0.96365682004294606,6.81,6.88,6.9950000000000001]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Phosphorus Dissolved","mg/l","2020-11-23","2024-03-18",3.316939890710382,39,0.94674808590207227,null,0.01,0.01,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Phosphorus Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,57,0.93726331964417142,null,0.01,0.01,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Potassium Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,56,0.91857318539049337,null,1,1,"<"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Selenium Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,7,7,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Sodium Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,0.88,1.01]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Specific Conductance","umhos/cm","2019-04-08","2024-03-18",4.942622950819672,59,0.93255538809921068,null,40.65,47.6]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Strontium Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,23,26]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Sulfate Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,5.1950000000000003,5.26,null,"Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Suspended Solids Total","mg/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,20,20,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Temperature Water (Field)","c","2019-04-08","2024-03-18",4.942622950819672,59,0.93255538809921068,null,9.84,11.18]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Zinc Dissolved","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,5,5,"<","Y"]
["WQN0458","Hoagland Run","25 ft upstr of Rt 973","Zinc Total","ug/l","2019-04-08","2024-03-18",4.942622950819672,58,0.91305110027008896,null,5,5,"<","Y"]

{"sheet":"WQN0459","index":34,"n_rows":54,"n_cols":15,"rows_kept":54,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Alkalinity (Lab)","mg/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,11.2,11.8,14,null,"Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Aluminum Dissolved","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,15,15,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Aluminum Total","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,26.8,35.1,null,"Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Ammonia as N Dissolved","mg/l","2020-11-03","2024-03-26",3.3934426229508201,40,0.91930953224800727,null,0.02,0.02,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Ammonia as N Total","mg/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,0.02,0.02,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Barium Total","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,18.100000000000001,19.399999999999999]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Boron Total","ug/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,200,200,"<"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Bromide Total","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,25,25,"<"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Cadmium Dissolved","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,0.2,0.2,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Calcium Dissolved","mg/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,4.9649999999999999,5.49]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Calcium Total","mg/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,5.04,5.4770000000000003,null,"Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Carbon Dissolved Organic","mg/l","2020-10-26","2024-02-26",3.3360655737704921,40,0.91930953224800727,null,0.98499999999999999,1.1399999999999999]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Carbon Total Organic","mg/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,0.92500000000000004,1.04]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,1.1000000000000001,1.36,null,"Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Chloride Total","mg/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,1.87,2.02,null,"Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Coliform Fecal","cf/100ml","2019-04-17","2024-03-26",4.9398907103825138,54,0.92409527051089835,null,25,25,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Copper Dissolved","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,4,4,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Copper Total","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,4,4,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Dissolved Oxygen (Field)","mg/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,10.8,11.59]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Dissolved Solids Total","mg/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,39,42,null,"Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","E. Coli","cf/100ml","2019-04-17","2024-03-26",4.9398907103825138,54,0.92409527051089835,null,25,38]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Hardness Total","mg/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,18,19,null,"Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Iron Dissolved","ug/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,100,100,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Iron Total","ug/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,100,104,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Lead Dissolved","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,1,1,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Lead Total","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,1,1,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Lithium Dissolved","ug/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,25,25,"<"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Lithium Total","ug/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,25,25,"<"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Magnesium Dissolved","mg/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,1.2250000000000001,1.29]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Magnesium Total","mg/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,1.2450000000000001,1.34]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Manganese Dissolved","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,5.37,6.48,null,"Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Manganese Total","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,9.5399999999999991,12.2,null,"Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Nickel Dissolved","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,8,8,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Nickel Total","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,8,8,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Nitrate + Nitrite as N Dissolved","mg/l","2020-11-03","2024-03-26",3.3934426229508201,40,0.91930953224800727,null,0.51500000000000001,0.59,null,"Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Nitrate + Nitrite as N Total","mg/l","2020-10-26","2024-03-26",3.415300546448087,41,0.94041611198190356,null,0.5,0.59,null,"Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Nitrogen Total","mg/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,0.57999999999999996,0.64,null,"Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Orthophosphate Dissolved","mg/l","2020-11-03","2024-03-26",3.3934426229508201,40,0.91930953224800727,null,0.01,0.01,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Orthophosphate Total","mg/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,0.01,0.01,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Osmotic Pressure","mosm/kg","2020-10-26","2024-03-26",3.415300546448087,33,0.91985668754205108,null,1,1,"<"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","pH","ph units","2019-04-17","2024-03-26",4.9398907103825138,57,0.96685603221249439,6.8849999999999998,7.03,7.12]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Phosphorus Dissolved","mg/l","2020-11-03","2024-02-26",3.3142076502732238,39,0.94674808590207227,null,0.01,0.01,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Phosphorus Total","mg/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,1.0999999999999999E-2,1.2999999999999999E-2,null,"Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Potassium Total","mg/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,1,1,"<"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Selenium Total","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,7,7,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Sodium Total","mg/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,1.45,1.55]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Specific Conductance","umhos/cm","2019-04-17","2024-03-26",4.9398907103825138,57,0.93726331964417142,null,46.75,53.6]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Strontium Total","ug/l","2019-04-17","2024-02-26",4.860655737704918,54,0.92409527051089835,null,21,23]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Sulfate Total","mg/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,5.53,5.66,null,"Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Suspended Solids Total","mg/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,20,20,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Temperature Water (Field)","c","2019-04-17","2024-03-26",4.9398907103825138,56,0.91857318539049337,null,8.7259999999999991,12.4]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Zinc Dissolved","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,5,5,"<","Y"]
["WQN0459","Kettle Creek","Just upstr of former Rt 318 Br @ Cross Fork","Zinc Total","ug/l","2019-04-17","2024-03-26",4.9398907103825138,55,0.94193585320759066,null,5,5,"<","Y"]

{"sheet":"WQN0463","index":35,"n_rows":51,"n_cols":15,"rows_kept":51,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Alkalinity (Lab)","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,4.8,5.4,6.3999999999999986,null,"Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Aluminum Dissolved","ug/l","2014-10-02","2019-09-17",4.9589041095890414,49,0.91456686684260546,null,28,33.9,null,"Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Aluminum Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,55,0.94193585320759066,null,41,49,null,"Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Ammonia as N Dissolved","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,0.02,0.02,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Ammonia as N Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,0.02,0.02,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Barium Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,14.8,15]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Boron Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,200,200,"<"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Bromide Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,25,25,"<"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Cadmium Dissolved","ug/l","2016-02-03","2019-09-17",3.6191780821917812,44,0.90385824557938566,null,0.2,0.2,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Calcium Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,3.1920000000000002,3.415,null,"Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Carbon Total Organic","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,1.01,1.1399999999999999]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Chloride Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,1.55,1.64,null,"Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Coliform Fecal","cf/100ml","2016-07-07","2019-09-17",3.1967213114754101,36,0.93475466477684654,null,25,25,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Copper Dissolved","ug/l","2014-10-02","2019-09-17",4.9589041095890414,51,0.90808545018414566,null,4,4,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Copper Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,4,4,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Dissolved Oxygen (Field)","mg/l","2014-10-01","2019-09-17",4.9616438356164387,75,0.93605008353293306,10.58,11.16]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Dissolved Solids Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,32,36,null,"Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","E. Coli","cf/100ml","2016-07-07","2019-09-17",3.1967213114754101,36,0.93475466477684654,null,25,25,"<"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Hardness Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,11,12,null,"Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Iron Dissolved","ug/l","2014-10-02","2019-09-17",4.9589041095890414,51,0.90808545018414566,null,100,100,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Iron Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,100,100,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Lead Dissolved","ug/l","2014-10-02","2019-09-17",4.9589041095890414,51,0.90808545018414566,null,1,1,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Lead Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,1,1,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Lithium Dissolved","ug/l","2016-03-17","2019-09-17",3.502732240437159,43,0.93400596554420179,null,25,25,"<"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Lithium Total","ug/l","2016-03-17","2019-09-17",3.502732240437159,43,0.93400596554420179,null,25,25,"<"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Magnesium Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,0.754,0.8]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Manganese Dissolved","ug/l","2014-10-02","2019-09-17",4.9589041095890414,51,0.90808545018414566,null,10,10,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Manganese Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,10,10,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Nickel Dissolved","ug/l","2015-11-18","2019-09-17",3.8301369863013699,46,0.94592396814113033,null,50,50,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Nickel Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,50,50,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Nitrate + Nitrite as N Dissolved","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,0.26,0.28000000000000003,null,"Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Nitrate + Nitrite as N Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,54,0.92409527051089835,null,0.248,0.28000000000000003,null,"Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Nitrogen Dissolved","mg/l","2014-10-02","2019-09-17",4.9589041095890414,27,0.94776101410388947,null,0.38900000000000001,0.45,null,"Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Nitrogen Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,0.3,0.34,null,"Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Orthophosphate Dissolved","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,0.01,0.01,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Orthophosphate Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,0.01,0.01,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Osmotic Pressure","mosm/kg","2014-10-02","2018-12-05",4.1753424657534248,17,0.950958251953125,null,1,1,"<"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","pH","ph units","2014-10-01","2019-09-17",4.9616438356164387,74,0.95260702449594825,6.6970000000000001,6.7450000000000001,6.85]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Phosphorus Dissolved","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,0.01,0.01,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Phosphorus Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,0.01,0.01,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Potassium Total","mg/l","2015-09-16","2019-09-17",4.0027322404371581,50,0.93509135292772771,null,1,1,"<"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Selenium Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,7,7,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Sodium Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,1.004,1.0569999999999999]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Specific Conductance","umhos/cm","2014-10-01","2019-09-17",4.9616438356164387,76,0.91535390732916411,null,32.25,34]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Strontium Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,21,23]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Sulfate Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,5.16,5.28,null,"Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Suspended Solids Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,57,0.93726331964417142,null,5,5,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Temperature Water (Field)","c","2014-10-01","2019-09-17",4.9616438356164387,76,0.91535390732916411,null,9.0500000000000007,11.1]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Zinc Dissolved","ug/l","2014-10-02","2018-12-05",4.1753424657534248,43,0.93400596554420179,null,10,12,"<","Y"]
["WQN0463","Rock Run Lycoming County","800 m upstr of confl with Lycoming Crk","Zinc Total","ug/l","2014-10-02","2018-11-07",4.0986301369863014,48,0.94053662474622968,null,10,11,"<","Y"]

{"sheet":"WQN0464","index":36,"n_rows":51,"n_cols":15,"rows_kept":51,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Alkalinity (Lab)","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,5.6,6.25,7.8,null,"Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Aluminum Dissolved","ug/l","2014-10-02","2019-09-17",4.9589041095890414,49,0.91456686684260546,null,15,15,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Aluminum Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,54,0.92409527051089835,null,19.175000000000001,21.5,null,"Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Ammonia as N Dissolved","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,0.02,0.02,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Ammonia as N Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,0.02,0.02,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Barium Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,20,22]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Boron Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,200,200,"<"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Bromide Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,55,0.94193585320759066,null,25,25,"<"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Cadmium Dissolved","ug/l","2016-02-03","2019-09-17",3.6191780821917812,44,0.90385824557938566,null,0.2,0.2,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Calcium Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,3.3607499999999999,3.7635000000000001,null,"Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Carbon Total Organic","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,1,1]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Chloride Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,2.2719999999999998,2.5099999999999998,null,"Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Coliform Fecal","cf/100ml","2016-07-07","2019-09-17",3.1967213114754101,37,0.90112825040705469,null,25,25,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Copper Dissolved","ug/l","2014-10-02","2019-09-17",4.9589041095890414,51,0.90808545018414566,null,4,4,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Copper Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Dissolved Oxygen (Field)","mg/l","2014-10-01","2019-09-17",4.9616438356164387,77,0.93245074854097354,10.55,10.984999999999999]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Dissolved Solids Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,37.5,40,null,"Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","E. Coli","cf/100ml","2016-07-07","2019-09-17",3.1967213114754101,37,0.90112825040705469,null,25,25,"<"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Hardness Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,12.25,14,null,"Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Iron Dissolved","ug/l","2014-10-02","2019-09-17",4.9589041095890414,51,0.90808545018414566,null,100,100,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Iron Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,100,100,null,"Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Lead Dissolved","ug/l","2014-10-02","2019-09-17",4.9589041095890414,51,0.90808545018414566,null,1,1,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Lead Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Lithium Dissolved","ug/l","2016-03-17","2019-09-17",3.502732240437159,43,0.93400596554420179,null,25,25,"<"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Lithium Total","ug/l","2016-03-17","2019-09-17",3.502732240437159,43,0.93400596554420179,null,25,25,"<"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Magnesium Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,0.99575000000000002,1.089]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Manganese Dissolved","ug/l","2014-10-02","2019-09-17",4.9589041095890414,51,0.90808545018414566,null,10,10,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Manganese Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,10,10,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Nickel Dissolved","ug/l","2015-11-18","2019-09-17",3.8301369863013699,46,0.94592396814113033,null,50,50,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Nickel Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,50,50,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Nitrate + Nitrite as N Dissolved","mg/l","2014-10-02","2019-09-17",4.9589041095890414,55,0.94193585320759066,null,0.18,0.2,null,"Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Nitrate + Nitrite as N Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,53,0.90162935155950785,null,0.18,0.19500000000000001,null,"Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Nitrogen Dissolved","mg/l","2014-10-02","2019-09-17",4.9589041095890414,25,0.95671474933624268,null,0.25,0.26350000000000001,null,"Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Nitrogen Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,0.25,0.25,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Orthophosphate Dissolved","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Orthophosphate Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Osmotic Pressure","mosm/kg","2014-10-02","2018-12-05",4.1753424657534248,18,0.90374755859375,null,1,1,"<"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","pH","ph units","2014-10-01","2019-09-17",4.9616438356164387,77,0.96046046712202227,6.75,6.83,6.88]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Phosphorus Dissolved","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Phosphorus Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Potassium Total","mg/l","2015-09-16","2019-09-17",4.0027322404371581,50,0.93509135292772771,null,1,1,"<"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Selenium Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,7,7,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Sodium Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,1.6315,1.76]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Specific Conductance","umhos/cm","2014-10-02","2019-09-17",4.9589041095890414,77,0.93245074854097354,null,41.9,44.7]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Strontium Total","ug/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,20.75,23]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Sulfate Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,6.9,6.95,null,"Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Suspended Solids Total","mg/l","2014-10-02","2019-09-17",4.9589041095890414,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Temperature Water (Field)","c","2014-10-01","2019-09-17",4.9616438356164387,78,0.91121757477792031,null,9.25,10.7]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Zinc Dissolved","ug/l","2014-10-02","2018-12-05",4.1753424657534248,44,0.90385824557938566,null,10,10,"<","Y"]
["WQN0464","Hyner Run","200 m upstr of Log Rd Hollow and 100 m dwnstr E Br Hyner","Zinc Total","ug/l","2014-10-02","2018-12-05",4.1753424657534248,49,0.91456686684260546,null,10,10,"<","Y"]

{"sheet":"WQN0465","index":37,"n_rows":50,"n_cols":15,"rows_kept":50,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Alkalinity (Lab)","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,5.4,6.8000000000000007,8,null,"Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Aluminum Dissolved","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,35.849999999999987,41.1,null,"Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Aluminum Total","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,66.075000000000003,73.8,null,"Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Ammonia as N Dissolved","mg/l","2017-10-03","2022-09-21",4.9671232876712326,47,0.92105930631851141,null,0.02,0.02,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Ammonia as N Total","mg/l","2017-10-03","2022-09-21",4.9671232876712326,47,0.92105930631851141,null,0.02,0.02,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Barium Total","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,10,10,"<"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Boron Total","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,200,200,"<"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Bromide Total","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,25,25,"<"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Cadmium Dissolved","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,0.2,0.2,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Calcium Total","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,1.3065,1.478,null,"Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Carbon Total Organic","mg/l","2017-10-03","2022-09-21",4.9671232876712326,47,0.92105930631851141,null,2.65,2.92]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Chloride Total","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,1.8,1.84,null,"Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Coliform Fecal","cf/100ml","2017-10-03","2022-09-21",4.9671232876712326,44,0.90385824557938566,null,25,25,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Copper Dissolved","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,4,4,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Copper Total","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,4,4,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Dissolved Oxygen (Field)","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,9.3699999999999992,10.62]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Dissolved Solids Total","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,40,42,null,"Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","E. Coli","cf/100ml","2017-10-03","2022-09-21",4.9671232876712326,45,0.92754573983745547,null,25,25,"<"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Hardness Total","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,6,6,null,"Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Iron Dissolved","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,104,125,null,"Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Iron Total","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,154.5,196,null,"Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Lead Dissolved","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,1,1,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Lead Total","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,1,1,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Lithium Dissolved","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,25,25,"<"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Lithium Total","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,25,25,"<"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Magnesium Total","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,0.60499999999999998,0.65]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Manganese Dissolved","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,10,10,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Manganese Total","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,11,15.5,null,"Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Nickel Dissolved","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,50,50,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Nickel Total","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,50,50,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Nitrate + Nitrite as N Dissolved","mg/l","2017-10-03","2022-09-21",4.9671232876712326,47,0.92105930631851141,null,0.08,0.09,null,"Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Nitrate + Nitrite as N Total","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,7.0000000000000007E-2,0.08,null,"Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Nitrogen Total","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,0.25,0.25,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Orthophosphate Dissolved","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,0.01,0.01,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Orthophosphate Total","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,0.01,0.01,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Osmotic Pressure","mosm/kg","2018-10-09","2022-09-21",3.9506849315068489,19,0.936431884765625,null,1,1,"<"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","pH","ph units","2017-10-03","2022-09-21",4.9671232876712326,49,0.95561583901285008,6.62,6.6950000000000003,6.7799999999999994]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Phosphorus Dissolved","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,0.01,0.01,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Phosphorus Total","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,0.01,0.01,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Potassium Total","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,1.2070000000000001,1.23]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Selenium Total","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,7,7,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Sodium Total","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,2.6459999999999999,2.72]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Specific Conductance","umhos/cm","2017-10-03","2022-09-21",4.9671232876712326,49,0.91456686684260546,null,27.75,29]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Strontium Total","ug/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,10,10,"<"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Sulfate Total","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,3.28,3.41,null,"Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Suspended Solids Total","mg/l","2017-10-03","2022-09-21",4.9671232876712326,48,0.94053662474622968,null,20,20,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Temperature Water (Field)","c","2017-10-03","2022-09-21",4.9671232876712326,49,0.91456686684260546,null,10.7,14.9]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Zinc Dissolved","ug/l","2017-10-03","2022-09-21",4.9671232876712326,32,0.94989754026755691,null,10,10,"<","Y"]
["WQN0465","Carbaugh Run","250 m upstr of confl with Clear Run Tributary","Zinc Total","ug/l","2017-10-03","2022-09-21",4.9671232876712326,32,0.94989754026755691,null,10,10,"<","Y"]

{"sheet":"WQN0466","index":38,"n_rows":51,"n_cols":15,"rows_kept":51,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Alkalinity (Lab)","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,8.4,9.6,10.8,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Aluminum Dissolved","ug/l","2015-04-02","2019-11-06",4.5956284153005464,54,0.92409527051089835,null,16.100000000000001,19,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Aluminum Total","ug/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,61.7,71.7,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Ammonia as N Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,0.02,0.02,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Arsenic Dissolved","ug/l","2015-04-02","2019-11-06",4.5956284153005464,55,0.94193585320759066,null,3,3,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Barium Total","ug/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,43.650000000000013,44.9]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Boron Total","ug/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,200,200,"<"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Bromide Total","ug/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,25,25,"<"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Cadmium Dissolved","ug/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,0.2,0.2,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Calcium Dissolved","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,3.6680000000000001,4.0030000000000001]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Calcium Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,3.6949999999999998,3.9060000000000001,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Carbon Total Organic","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,1.2350000000000001,1.49]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2015-04-02","2019-11-06",4.5956284153005464,54,0.92409527051089835,null,0.9,1.2,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Chloride Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,5.7750000000000004,6.34,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Coliform Fecal","cf/100ml","2016-07-06","2019-11-06",3.3360655737704921,40,0.91930953224800727,null,25,32.5,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Copper Dissolved","ug/l","2015-04-02","2019-11-06",4.5956284153005464,55,0.94193585320759066,null,4,4,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Copper Total","ug/l","2015-04-02","2019-11-06",4.5956284153005464,55,0.94193585320759066,null,4,4,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Dissolved Oxygen (Field)","mg/l","2016-01-14","2019-11-06",3.8109589041095888,43,0.93400596554420179,10.47,11.72]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Dissolved Solids Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,52,56,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","E. Coli","cf/100ml","2016-07-06","2019-11-06",3.3360655737704921,40,0.91930953224800727,null,25,30]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Hardness Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,16,16,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Iron Dissolved","ug/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,100,100,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Iron Total","ug/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,141,162,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Lead Dissolved","ug/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Lead Total","ug/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Lithium Dissolved","ug/l","2016-03-08","2019-11-06",3.6639344262295079,45,0.92754573983745547,null,25,25,"<"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Lithium Total","ug/l","2016-03-08","2019-11-06",3.6639344262295079,45,0.92754573983745547,null,25,25,"<"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Magnesium Dissolved","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,1.4950000000000001,1.6060000000000001]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Magnesium Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,1.5569999999999999,1.619]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Manganese Dissolved","ug/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,10,12.25,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Manganese Total","ug/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,21.35,24.7,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Nickel Dissolved","ug/l","2015-04-02","2019-08-08",4.3497267759562854,52,0.9296057789329375,null,4,4,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Nickel Total","ug/l","2015-04-02","2019-08-08",4.3497267759562854,52,0.9296057789329375,null,4,4,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Nitrate as N Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,0.45,0.46,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Nitrite as N Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,0.04,0.04,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Nitrogen Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,0.48499999999999999,0.52,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Orthophosphate Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,55,0.94193585320759066,null,0.01,0.01,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Osmotic Pressure","mosm/kg","2015-04-02","2018-12-17",3.70958904109589,40,0.91930953224800727,null,1,1,"<"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","pH","ph units","2015-04-02","2019-11-06",4.5956284153005464,56,0.95595345389784914,7.08,7.21,7.31]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Phosphorus Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Potassium Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,1,1.08,"<"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Selenium Total","ug/l","2015-04-02","2019-11-06",4.5956284153005464,55,0.94193585320759066,null,7,7,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Sodium Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,5.4924999999999997,5.99]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Specific Conductance","umhos/cm","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,66.050000000000011,70]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Strontium Total","ug/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,24,25]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Sulfate Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,8.9974999999999987,9.2200000000000006,null,"Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Suspended Solids Total","mg/l","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Temperature Water (Field)","c","2015-04-02","2019-11-06",4.5956284153005464,56,0.91857318539049337,null,8,11.5]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Zinc Dissolved","ug/l","2015-04-02","2019-11-06",4.5956284153005464,55,0.94193585320759066,null,5,6.49,"<","Y"]
["WQN0466","PORCUPINE CREEK","President Rd - President Township","Zinc Total","ug/l","2015-04-02","2019-11-06",4.5956284153005464,55,0.94193585320759066,null,5,5.32,"<","Y"]

{"sheet":"WQN0500","index":39,"n_rows":52,"n_cols":15,"rows_kept":52,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Alkalinity (Lab)","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,17.2,24.4,33,null,"Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Aluminum Dissolved","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,15,15,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Aluminum Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,51,57.2,null,"Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Ammonia as N Dissolved","mg/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,0.02,0.02,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Ammonia as N Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,0.02,0.02,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Barium Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,45.2,50.6]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Boron Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,200,200,"<"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Bromide Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,25,25,"<"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Cadmium Dissolved","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,0.2,0.2,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Calcium Dissolved","mg/l","2021-02-09","2024-03-26",3.12568306010929,34,0.94238732708618034,null,6.9950000000000001,8.7200000000000006]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Calcium Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,7.4729999999999999,8.73,null,"Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Carbon Dissolved Organic","mg/l","2021-02-09","2024-02-26",3.0464480874316942,33,0.91985668754205108,null,1.59,1.91]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Carbon Total Organic","mg/l","2020-09-17","2024-02-26",3.442622950819672,37,0.90112825040705469,null,1.72,1.92]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2021-02-09","2024-03-26",3.12568306010929,34,0.94238732708618034,null,1.04,1.39,null,"Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Chloride Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,4.4000000000000004,5.0999999999999996,null,"Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Copper Dissolved","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,4,4,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Copper Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,4,4,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Dissolved Oxygen (Field)","mg/l","2020-10-20","2024-03-26",3.4316939890710381,38,0.92704861148376938,9.77,10.79]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Dissolved Solids Total","mg/l","2020-09-17","2024-02-26",3.442622950819672,38,0.92704861148376938,null,52,64,null,"Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Hardness Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,30,35,null,"Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Iron Dissolved","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,100,100,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Iron Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,151,214,null,"Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Lead Dissolved","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,1,1,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Lead Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,1,1,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Lithium Dissolved","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,25,25,"<"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Lithium Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,25,25,"<"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Magnesium Dissolved","mg/l","2021-02-09","2024-03-26",3.12568306010929,34,0.94238732708618034,null,2.69,3.22]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Magnesium Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,2.86,3.19]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Manganese Dissolved","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,15,19,null,"Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Manganese Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,20.6,25.1,null,"Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Nickel Dissolved","ug/l","2021-02-09","2024-03-26",3.12568306010929,35,0.91046892106533028,null,8,8,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Nickel Total","ug/l","2021-02-09","2024-03-26",3.12568306010929,35,0.91046892106533028,null,8,8,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Nitrate + Nitrite as N Dissolved","mg/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,0.61,0.74,null,"Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Nitrate + Nitrite as N Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,0.625,0.75,null,"Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Nitrogen Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,0.76,0.88,null,"Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Orthophosphate Dissolved","mg/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,0.01,0.01,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Orthophosphate Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,0.01,0.01,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Osmotic Pressure","mosm/kg","2020-10-20","2024-03-26",3.4316939890710381,29,0.93857165426015854,null,1,1,"<"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","pH","ph units","2020-09-17","2024-03-26",3.5218579234972678,39,0.97629729752952699,6.84,7.01,7.28]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Phosphorus Dissolved","mg/l","2020-09-17","2024-02-26",3.442622950819672,36,0.93475466477684654,null,0.01,0.01,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Phosphorus Total","mg/l","2020-09-17","2024-02-26",3.442622950819672,38,0.92704861148376938,null,0.01,1.2E-2,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Potassium Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,1.79,1.96]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Selenium Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,7,7,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Sodium Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,3.47,3.76]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Specific Conductance","umhos/cm","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,89.75,96.35]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Strontium Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,42,51]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Sulfate Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,7.67,8.01,null,"Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Suspended Solids Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,20,20,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Temperature Water (Field)","c","2020-10-20","2024-03-26",3.4316939890710381,38,0.92704861148376938,null,10.15,14.4]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Zinc Dissolved","ug/l","2021-02-09","2024-03-26",3.12568306010929,35,0.91046892106533028,null,5,5,"<","Y"]
["WQN0500","East Branch Sideling Hill Creek","Just upstr of Amaranth Rd","Zinc Total","ug/l","2021-02-09","2024-03-26",3.12568306010929,35,0.91046892106533028,null,5,5.78,"<","Y"]

{"sheet":"WQN0514","index":40,"n_rows":48,"n_cols":15,"rows_kept":48,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Alkalinity (Lab)","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,16.399999999999999,23.6,25.6,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Aluminum Dissolved","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,15,15,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Aluminum Total","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,65.2,78.3,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Ammonia as N Total","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,0.02,0.02,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Arsenic Dissolved","ug/l","2016-05-31","2020-09-15",4.2931506849315069,52,0.9296057789329375,null,3,3,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Barium Total","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,32.6,34.700000000000003]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Boron Total","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,200,200,"<"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Bromide Total","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,25,25,"<"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Cadmium Dissolved","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,0.2,0.2,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Calcium Total","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,6.2140000000000004,7.056,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,1.1000000000000001,1.3,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Chloride Total","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,4.29,5.22,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Coliform Fecal","cf/100ml","2016-05-31","2020-11-16",4.463013698630137,54,0.92409527051089835,null,36,60,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Copper Dissolved","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Copper Total","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Dissolved Oxygen (Field)","mg/l","2016-05-31","2021-05-26",4.9863013698630141,58,0.91305110027008896,8.94,10.050000000000001]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Dissolved Solids Total","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,58,64,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","E. Coli","cf/100ml","2016-05-31","2020-11-16",4.463013698630137,53,0.90162935155950785,null,40,70]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Hardness Total","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,26,30,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Iron Dissolved","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,100,100,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Iron Total","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,186,202,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Lead Dissolved","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,1,1,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Lead Total","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,1,1,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Lithium Dissolved","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,25,25,"<"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Lithium Total","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,25,25,"<"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Magnesium Total","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,2.57,2.956]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Manganese Dissolved","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,9.23,13.004,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Manganese Total","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,15.1,21.1,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Nickel Dissolved","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,8,8,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Nickel Total","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,8,8,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Nitrate as N Total","mg/l","2016-05-31","2020-09-15",4.2931506849315069,52,0.9296057789329375,null,0.28000000000000003,0.44,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Nitrite as N Total","mg/l","2016-05-31","2020-09-15",4.2931506849315069,52,0.9296057789329375,null,0.04,0.04,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Nitrogen Total","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,0.41,0.61,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Orthophosphate Total","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,0.01,0.01,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Osmotic Pressure","mosm/kg","2016-05-31","2021-05-26",4.9863013698630141,29,0.93857165426015854,null,1,1,"<"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","pH","ph units","2016-05-31","2021-05-26",4.9863013698630141,59,0.96365682004294606,7.415,7.5,7.6]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Phosphorus Total","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,1.0999999999999999E-2,1.2999999999999999E-2,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Potassium Total","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,1.64,1.917]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Selenium Total","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,7,7,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Sodium Total","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,3.6120000000000001,4.218]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Specific Conductance","umhos/cm","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,74.95,85]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Strontium Total","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,39,44]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Sulfate Total","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,7.81,8.19,null,"Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Suspended Solids Total","mg/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,5,5,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Temperature Water (Field)","c","2016-05-31","2021-05-26",4.9863013698630141,58,0.91305110027008896,null,13.45,17.3]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Zinc Dissolved","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,5,5,"<","Y"]
["WQN0514","Sideling Hill Creek","Upstr of Hixon Rd Crossing","Zinc Total","ug/l","2016-05-31","2021-05-26",4.9863013698630141,59,0.93255538809921068,null,5,5,"<","Y"]

{"sheet":"WQN0626","index":41,"n_rows":51,"n_cols":15,"rows_kept":51,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Alkalinity (Lab)","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,7.6,8.6,9.8000000000000007,null,"Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Aluminum Dissolved","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,15.1,16.8,null,"Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Aluminum Total","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,72.424999999999997,93.8,null,"Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Ammonia as N Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,0.02,0.02,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Arsenic Dissolved","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,3,3,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Barium Total","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,14.75,16]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Boron Total","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,200,200,"<"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Bromide Total","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,25,25,"<"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Cadmium Dissolved","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,0.2,0.2,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Calcium Dissolved","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,3.484,3.7050000000000001]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Calcium Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,3.3919999999999999,3.6219999999999999,null,"Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Carbon Total Organic","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,1.31,1.48]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,0.92500000000000004,1.085,null,"Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Chloride Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,0.54500000000000004,0.59,null,"Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Coliform Fecal","cf/100ml","2016-07-05","2019-11-07",3.3415300546448088,40,0.91930953224800727,null,25,25,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Copper Dissolved","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Copper Total","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Dissolved Oxygen (Field)","mg/l","2016-09-06","2019-11-07",3.1693989071038251,37,0.90112825040705469,10.6,11.45]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Dissolved Solids Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,35.5,38,null,"Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","E. Coli","cf/100ml","2016-07-05","2019-11-07",3.3415300546448088,40,0.91930953224800727,null,25,25,"<"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Hardness Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,14,15,null,"Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Iron Dissolved","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,100,100,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Iron Total","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,128,191,null,"Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Lead Dissolved","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Lead Total","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Lithium Dissolved","ug/l","2016-03-09","2019-11-07",3.6639344262295079,45,0.92754573983745547,null,25,25,"<"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Lithium Total","ug/l","2016-03-09","2019-11-07",3.6639344262295079,45,0.92754573983745547,null,25,25,"<"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Magnesium Dissolved","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,1.2224999999999999,1.323]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Magnesium Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,1.2544999999999999,1.3779999999999999]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Manganese Dissolved","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,3.61,4.0599999999999996,null,"Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Manganese Total","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,7.63,9.5,null,"Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Nickel Dissolved","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,8,8,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Nickel Total","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,8,8,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Nitrate as N Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,0.14000000000000001,0.16,null,"Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Nitrite as N Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,0.04,0.04,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Nitrogen Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,0.25,0.25,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Orthophosphate Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Osmotic Pressure","mosm/kg","2015-04-02","2018-12-18",3.7123287671232879,39,0.94674808590207227,null,1,1,"<"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","pH","ph units","2015-04-02","2019-11-07",4.5983606557377046,56,0.95595345389784914,7.0449999999999999,7.1275000000000004,7.21]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Phosphorus Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,0.01,1.0999999999999999E-2,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Potassium Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,1,1,"<"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Selenium Total","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,7,7,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Sodium Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,0.88549999999999995,0.95]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Specific Conductance","umhos/cm","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,34.924999999999997,36.799999999999997]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Strontium Total","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,14,16]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Sulfate Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,5.8324999999999996,5.99,null,"Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Suspended Solids Total","mg/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Temperature Water (Field)","c","2015-04-02","2019-11-07",4.5983606557377046,55,0.94193585320759066,null,8.6,10.7]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Zinc Dissolved","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0626","North Branch Sugar Run","Approx. 0.5 miles upstr of SR 321, along Anf Rd","Zinc Total","ug/l","2015-04-02","2019-11-07",4.5983606557377046,56,0.91857318539049337,null,5,5,"<","Y"]

{"sheet":"WQN0627","index":42,"n_rows":51,"n_cols":15,"rows_kept":51,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Alkalinity (Lab)","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,17.8,21.8,26,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Aluminum Dissolved","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,15.5,16.600000000000001,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Aluminum Total","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,57.15,68.7,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Ammonia as N Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,0.02,0.02,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Arsenic Dissolved","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,3,3,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Barium Total","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,59,68.808000000000007]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Boron Total","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,200,200,"<"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Bromide Total","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,25,28.32,"<"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Cadmium Dissolved","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,0.2,0.2,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Calcium Dissolved","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,8.2720000000000002,9.4499999999999993]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Calcium Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,7.8884999999999996,9.3040000000000003,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Carbon Total Organic","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,1.4350000000000001,1.66]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,0.91500000000000004,1,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Chloride Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,5.2799999999999994,5.7,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Coliform Fecal","cf/100ml","2016-07-05","2019-10-09",3.262295081967213,39,0.94674808590207227,null,25,25,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Copper Dissolved","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Copper Total","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Dissolved Oxygen (Field)","mg/l","2016-09-06","2019-11-07",3.1693989071038251,37,0.90112825040705469,10.54,11.2]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Dissolved Solids Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,58,64,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","E. Coli","cf/100ml","2016-07-05","2019-10-09",3.262295081967213,39,0.94674808590207227,null,25,25,"<"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Hardness Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,26.5,31,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Iron Dissolved","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,100,100,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Iron Total","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,194.5,222,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Lead Dissolved","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Lead Total","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Lithium Dissolved","ug/l","2016-03-09","2019-11-07",3.6639344262295079,45,0.92754573983745547,null,25,25,"<"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Lithium Total","ug/l","2016-03-09","2019-11-07",3.6639344262295079,45,0.92754573983745547,null,25,25,"<"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Magnesium Dissolved","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,1.6515,1.8]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Magnesium Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,1.6067499999999999,1.8260000000000001]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Manganese Dissolved","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,10.45,11.4,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Manganese Total","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,18.850000000000001,21.1,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Nickel Dissolved","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,8,8,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Nickel Total","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,8,8,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Nitrate as N Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,0.20499999999999999,0.23,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Nitrite as N Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,0.04,0.04,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Nitrogen Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,0.27,0.31,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Orthophosphate Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Osmotic Pressure","mosm/kg","2015-04-01","2018-12-18",3.7150684931506852,40,0.91930953224800727,null,1,1,"<"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","pH","ph units","2015-04-01","2019-11-07",4.6010928961748636,56,0.95595345389784914,7.3949999999999996,7.4325000000000001,7.52]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Phosphorus Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,0.01,1.0999999999999999E-2,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Potassium Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,1,1,"<"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Selenium Total","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,7,7,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Sodium Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,3.8835000000000002,4.431]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Specific Conductance","umhos/cm","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,78.55,84.6]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Strontium Total","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,37.75,47]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Sulfate Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,6.79,6.88,null,"Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Suspended Solids Total","mg/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Temperature Water (Field)","c","2015-04-01","2019-11-07",4.6010928961748636,55,0.94193585320759066,null,8.4,11]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Zinc Dissolved","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0627","Buck Run","Approx. 100 m dwnstr of Lanigan Brook","Zinc Total","ug/l","2015-04-01","2019-11-07",4.6010928961748636,56,0.91857318539049337,null,5,5,"<","Y"]

{"sheet":"WQN0628","index":43,"n_rows":51,"n_cols":15,"rows_kept":51,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Alkalinity (Lab)","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,3,3.4,3.6,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Aluminum Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,63.349999999999987,70.5,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Aluminum Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,80.710000000000008,86.65,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Ammonia as N Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.02,0.02,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Arsenic Dissolved","ug/l","2015-12-08","2020-08-26",4.7158469945355188,53,0.90162935155950785,null,3,3,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Barium Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,16.105,16.600000000000001]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Boron Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,200,200,"<"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Bromide Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,25,25,"<"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Cadmium Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.2,0.2,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Calcium Dissolved","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,2.9902500000000001,3.12]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Calcium Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,2.9754999999999998,3.0950000000000002,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Carbon Total Organic","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,2.665,2.89]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.8,0.95,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Chloride Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,3.95,4.2850000000000001,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Coliform Fecal","cf/100ml","2016-07-13","2020-11-12",4.3342465753424646,48,0.94053662474622968,null,25,25,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Copper Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Copper Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Dissolved Oxygen (Field)","mg/l","2015-12-08","2020-11-12",4.9289617486338786,55,0.94193585320759066,9.7799999999999994,10.49]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Dissolved Solids Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,36,40,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","E. Coli","cf/100ml","2016-07-13","2020-11-12",4.3342465753424646,48,0.94053662474622968,null,25,25,"<"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Hardness Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,9,10,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Iron Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,100,100,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Iron Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,103.5,122,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Lead Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Lead Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Lithium Dissolved","ug/l","2016-03-09","2020-11-12",4.6794520547945204,53,0.90162935155950785,null,25,25,"<"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Lithium Total","ug/l","2016-03-09","2020-11-12",4.6794520547945204,53,0.90162935155950785,null,25,25,"<"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Magnesium Dissolved","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.44750000000000001,0.46]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Magnesium Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.44900000000000001,0.46600000000000003]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Manganese Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,5.8075000000000001,6.74,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Manganese Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,12.475,16.5,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Nickel Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,8,8,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Nickel Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,8,8,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Nitrate as N Total","mg/l","2015-12-08","2020-08-26",4.7158469945355188,53,0.90162935155950785,null,0.27,0.31,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Nitrite as N Total","mg/l","2015-12-08","2020-08-26",4.7158469945355188,53,0.90162935155950785,null,0.04,0.04,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Nitrogen Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.38750000000000001,0.42,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Orthophosphate Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Osmotic Pressure","mosm/kg","2015-12-08","2020-10-20",4.8661202185792352,33,0.91985668754205108,null,1,1,"<"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","pH","ph units","2015-12-08","2020-11-12",4.9289617486338786,56,0.95595345389784914,6.4550000000000001,6.54,6.585]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Phosphorus Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Potassium Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,1,1,"<"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Selenium Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,7,7,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Sodium Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,2.645,2.7974999999999999]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Specific Conductance","umhos/cm","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,37.325000000000003,39.35]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Strontium Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,11,12]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Sulfate Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,3.875,4.5599999999999996,null,"Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Suspended Solids Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Temperature Water (Field)","c","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,9.8000000000000007,13]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Zinc Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0628","Kitchen Creek","Approx. 200 m upstr of SR 118","Zinc Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,5,5,"<","Y"]

{"sheet":"WQN0629","index":44,"n_rows":50,"n_cols":15,"rows_kept":50,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Alkalinity (Lab)","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,1.4,1.6,1.8,null,"Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Aluminum Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,116.4725,124,null,"Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Aluminum Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,148.57599999999999,199,null,"Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Ammonia as N Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.02,0.02,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Arsenic Dissolved","ug/l","2015-12-08","2020-08-26",4.7158469945355188,53,0.90162935155950785,null,3,3,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Barium Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,11.8,12.65]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Boron Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,200,200,"<"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Bromide Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,25,25,"<"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Cadmium Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.2,0.2,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Calcium Dissolved","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,1.663,1.71]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Calcium Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,1.6779999999999999,1.7230000000000001,null,"Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Carbon Total Organic","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,2.99,3.79]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.75,0.9,null,"Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Chloride Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.59250000000000003,0.62,null,"Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Coliform Fecal","cf/100ml","2016-07-13","2020-11-12",4.3342465753424646,48,0.94053662474622968,null,25,25,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Copper Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Copper Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Dissolved Oxygen (Field)","mg/l","2015-12-08","2020-11-12",4.9289617486338786,55,0.94193585320759066,9.85,10.9]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Dissolved Solids Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,30,34,null,"Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","E. Coli","cf/100ml","2016-07-13","2020-11-12",4.3342465753424646,48,0.94053662474622968,null,25,25,"<"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Hardness Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,6,6,null,"Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Iron Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,100,100,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Iron Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,100,124,null,"Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Lead Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Lead Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Lithium Dissolved","ug/l","2016-03-09","2020-11-12",4.6794520547945204,53,0.90162935155950785,null,25,25,"<"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Lithium Total","ug/l","2016-03-09","2020-11-12",4.6794520547945204,53,0.90162935155950785,null,25,25,"<"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Magnesium Dissolved","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.45900000000000002,0.47]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Magnesium Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.48,0.5]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Manganese Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,9.39,14.87,null,"Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Manganese Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,11.11,15.9,null,"Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Nickel Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,8,8,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Nickel Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,8,8,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Nitrate as N Total","mg/l","2015-12-08","2020-08-26",4.7158469945355188,53,0.90162935155950785,null,0.12,0.18,null,"Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Nitrite as N Total","mg/l","2015-12-08","2020-08-26",4.7158469945355188,53,0.90162935155950785,null,0.04,0.04,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Nitrogen Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.25,0.28000000000000003,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Orthophosphate Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Osmotic Pressure","mosm/kg","2015-12-08","2020-11-12",4.9289617486338786,33,0.91985668754205108,null,1,1,"<"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Phosphorus Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Potassium Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,1,1,"<"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Selenium Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,7,7,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Sodium Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,0.53950000000000009,0.57999999999999996]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Specific Conductance","umhos/cm","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,18.5975,19.074999999999999]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Strontium Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,10,10]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Sulfate Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,3.8849999999999998,4.3099999999999996,null,"Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Suspended Solids Total","mg/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Temperature Water (Field)","c","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,9.5,13.6]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Zinc Dissolved","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,5.8049999999999997,6.93,null,"Y"]
["WQN0629","Stony Brook","Approx. 150 m upstr of SR 3001 Br (Windy Valley Rd)","Zinc Total","ug/l","2015-12-08","2020-11-12",4.9289617486338786,56,0.91857318539049337,null,6.0975000000000001,7.2249999999999996,null,"Y"]

{"sheet":"WQN0630","index":45,"n_rows":51,"n_cols":15,"rows_kept":51,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Alkalinity (Lab)","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,10.7,12.45,14.8,null,"Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Aluminum Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,15,15,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Aluminum Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,37.200000000000003,44.400000000000013,null,"Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Ammonia as N Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,55,0.94193585320759066,null,0.02,0.02,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Arsenic Dissolved","ug/l","2015-12-09","2020-08-27",4.7158469945355188,53,0.90162935155950785,null,3,3,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Barium Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,18.25,20.5]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Boron Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,200,200,"<"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Bromide Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,25,25,"<"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Cadmium Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,0.2,0.2,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Calcium Dissolved","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,5.5839999999999996,6.35]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Calcium Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,5.62575,6.274,null,"Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Carbon Total Organic","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,1.78,1.93]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,0.82500000000000007,1,null,"Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Chloride Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,0.64500000000000002,0.69,null,"Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Coliform Fecal","cf/100ml","2016-07-12","2020-11-16",4.3479452054794523,49,0.91456686684260546,null,25,25,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Copper Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Copper Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Dissolved Oxygen (Field)","mg/l","2015-12-09","2020-11-16",4.9371584699453557,55,0.94193585320759066,10.35,11.37]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Dissolved Solids Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,40,44,null,"Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","E. Coli","cf/100ml","2016-07-12","2020-11-16",4.3479452054794523,49,0.91456686684260546,null,25,25,"<"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Hardness Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,17.5,20,null,"Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Iron Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,100,100,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Iron Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,101.5,128,null,"Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Lead Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Lead Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Lithium Dissolved","ug/l","2016-03-10","2020-11-16",4.6876712328767134,53,0.90162935155950785,null,25,25,"<"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Lithium Total","ug/l","2016-03-10","2020-11-16",4.6876712328767134,53,0.90162935155950785,null,25,25,"<"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Magnesium Dissolved","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,0.76,0.89800000000000002]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Magnesium Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,0.81499999999999995,0.91800000000000004]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Manganese Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,2.8149999999999999,2.94,null,"Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Manganese Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,8.5949999999999989,10.4,null,"Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Nickel Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,8,8,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Nickel Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,8,8,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Nitrate as N Total","mg/l","2015-12-09","2020-08-27",4.7158469945355188,53,0.90162935155950785,null,0.18,0.2,null,"Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Nitrite as N Total","mg/l","2015-12-09","2020-08-27",4.7158469945355188,53,0.90162935155950785,null,0.04,0.04,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Nitrogen Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,0.29499999999999998,0.33,null,"Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Orthophosphate Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Osmotic Pressure","mosm/kg","2015-12-09","2020-11-16",4.9371584699453557,27,0.94776101410388947,null,1,1,"<"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","pH","ph units","2015-12-09","2020-11-16",4.9371584699453557,56,0.95595345389784914,7.11,7.19,7.28]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Phosphorus Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Potassium Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,1,1,"<"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Selenium Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,7,7,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Sodium Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,0.89549999999999996,0.95]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Specific Conductance","umhos/cm","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,41.4,44.75]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Strontium Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,15,18]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Sulfate Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,4.2300000000000004,4.38,null,"Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Suspended Solids Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Temperature Water (Field)","c","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,8.24,10.5]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Zinc Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0630","East Branch Hemlock Creek","Approx. 15 m upstr of Putman Hill Rd Culvert on SGL 70","Zinc Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,5,5,"<","Y"]

{"sheet":"WQN0634","index":46,"n_rows":51,"n_cols":15,"rows_kept":51,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Alkalinity (Lab)","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,11.4,12.4,15.4,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Aluminum Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,21.225000000000001,26.2,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Aluminum Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,69.25,81.349999999999994,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Ammonia as N Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,55,0.94193585320759066,null,0.02,0.02,"<","Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Arsenic Dissolved","ug/l","2015-12-09","2020-08-27",4.7158469945355188,53,0.90162935155950785,null,3,3,"<","Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Barium Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,22.1,26.1]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Boron Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,200,200,"<"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Bromide Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,25,25,"<"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Cadmium Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,0.2,0.2,"<","Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Calcium Dissolved","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,5.6449999999999996,6.7110000000000003]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Calcium Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,5.7752499999999998,6.78,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Carbon Total Organic","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,3.5049999999999999,4.12]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,1.1000000000000001,1.2,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Chloride Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,2.1949999999999998,2.42,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Coliform Fecal","cf/100ml","2016-07-12","2020-11-16",4.3479452054794523,49,0.91456686684260546,null,25,27,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Copper Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Copper Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Dissolved Oxygen (Field)","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,9.39,10.69]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Dissolved Solids Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,44,47,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","E. Coli","cf/100ml","2016-07-12","2020-11-16",4.3479452054794523,49,0.91456686684260546,null,25,36]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Hardness Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,17,19,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Iron Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,122,177,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Iron Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,282,327,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Lead Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Lead Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Lithium Dissolved","ug/l","2016-03-10","2020-11-16",4.6876712328767134,53,0.90162935155950785,null,25,25,"<"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Lithium Total","ug/l","2016-03-10","2020-11-16",4.6876712328767134,53,0.90162935155950785,null,25,25,"<"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Magnesium Dissolved","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,0.54,0.64100000000000001]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Magnesium Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,0.57050000000000001,0.65]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Manganese Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,23.7,28.15,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Manganese Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,32.049999999999997,47.8,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Nickel Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,8,8,"<","Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Nickel Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,8,8,"<","Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Nitrate as N Total","mg/l","2015-12-09","2020-08-27",4.7158469945355188,53,0.90162935155950785,null,0.12,0.15,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Nitrite as N Total","mg/l","2015-12-09","2020-08-27",4.7158469945355188,53,0.90162935155950785,null,0.04,0.04,"<","Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Nitrogen Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,0.32750000000000001,0.35,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Orthophosphate Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,0.01,0.01,"<","Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Osmotic Pressure","mosm/kg","2015-12-09","2020-11-16",4.9371584699453557,25,0.95671474933624268,null,1,1,"<"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","pH","ph units","2015-12-09","2020-11-16",4.9371584699453557,57,0.96685603221249439,6.95,7.02,7.13]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Phosphorus Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,1.9E-2,2.1000000000000001E-2,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Potassium Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,1,1,"<"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Selenium Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,7,7,"<","Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Sodium Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,1.7295,1.82]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Specific Conductance","umhos/cm","2015-12-09","2020-11-16",4.9371584699453557,57,0.93726331964417142,null,47.05,51.7]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Strontium Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,16,20]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Sulfate Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,2.71,2.95,null,"Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Suspended Solids Total","mg/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Temperature Water (Field)","c","2015-12-09","2020-11-16",4.9371584699453557,57,0.93726331964417142,null,8.41,12.8]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Zinc Dissolved","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0634","Crooked Creek","20 m upstr of stream ford coming from SGL 159 parking area along Crooked Crk Rd (T-724)","Zinc Total","ug/l","2015-12-09","2020-11-16",4.9371584699453557,56,0.91857318539049337,null,5,5,"<","Y"]

{"sheet":"WQN0723","index":47,"n_rows":44,"n_cols":15,"rows_kept":44,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Alkalinity (Lab)","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,13.4,15.2,21,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Aluminum Dissolved","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,10,10.8,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Aluminum Total","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,64.775000000000006,81.900000000000006,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Ammonia as N Total","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,0.02,0.02,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Arsenic Dissolved","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,3,3,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Barium Total","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,36.725000000000001,39.6]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Boron Total","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,200,200,"<"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Bromide Total","ug/l","2012-07-17","2015-08-04",3.0491803278688518,37,0.90112825040705469,null,25,25,"<"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Cadmium Dissolved","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,0.2,0.2,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Calcium Total","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,8.5434999999999999,9.89,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,1.1000000000000001,1.2,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Chloride Total","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,12.945,14.83,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Coliform Fecal","cf/100ml","2010-10-25","2015-08-04",4.7753424657534236,57,0.93726331964417142,null,50,80,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Copper Dissolved","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,4,4,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Copper Total","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,4,4,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Dissolved Oxygen (Field)","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,10,11.06]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Dissolved Solids Total","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,71,82,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Hardness Total","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,28.5,32,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Iron Dissolved","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,33.5,38,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Iron Total","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,232,291,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Lead Dissolved","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,1,1,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Lead Total","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,1,1,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Magnesium Total","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,1.7444999999999999,1.9139999999999999]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Manganese Dissolved","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,15.15,16.899999999999999,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Manganese Total","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,20.59,23.2,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Nickel Dissolved","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,4,4,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Nickel Total","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,4,4,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Nitrate as N Total","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,0.16,0.17,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Nitrite as N Total","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,0.04,0.04,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Nitrogen Total","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,0.25,0.25,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Orthophosphate Total","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,0.01,0.01,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Osmotic Pressure","mosm/kg","2010-10-25","2015-08-04",4.7753424657534236,57,0.93726331964417142,null,2,2]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","pH","ph units","2010-10-25","2015-08-04",4.7753424657534236,58,0.95205967592833274,7.31,7.3949999999999996,7.5299999999999994]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Phosphorus Total","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,0.01,0.01,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Selenium Total","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,7,7,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Sodium Total","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,7.6315,8.69]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Specific Conductance","umhos/cm","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,102.875,120.65]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Strontium Total","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,27.5,30]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Sulfate Total","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,11.215,11.38,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Suspended Solids Total","mg/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,5,5,"<","Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Temperature Water (Field)","c","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,10.4,13.4]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Zinc Dissolved","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,5.66,6.26,null,"Y"]
["WQN0723","Big Sandy Creek","SR2004 (Quebec Rd) Br @ Elliottsville","Zinc Total","ug/l","2010-10-25","2015-08-04",4.7753424657534236,58,0.91305110027008896,null,6,7,null,"Y"]

{"sheet":"WQN0724","index":48,"n_rows":44,"n_cols":15,"rows_kept":44,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Alkalinity (Lab)","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,12.2,13,15.4,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Aluminum Dissolved","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,21.7,26.1,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Aluminum Total","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,55.1,71.099999999999994,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Ammonia as N Total","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,0.02,0.02,"<","Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Arsenic Dissolved","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,3,3,"<","Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Barium Total","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,37.1,38.25]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Boron Total","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,200,200,"<"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Bromide Total","ug/l","2012-06-26","2015-09-08",3.2021857923497268,39,0.94674808590207227,null,25,25,"<"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Cadmium Dissolved","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,0.2,0.2,"<","Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Calcium Total","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,8.5440000000000005,8.952,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,1.1000000000000001,1.3,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Chloride Total","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,25.85,31.01,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Coliform Fecal","cf/100ml","2010-11-17","2015-09-08",4.8082191780821919,53,0.90162935155950785,null,36,55,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Copper Dissolved","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Copper Total","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Dissolved Oxygen (Field)","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,10.31,10.72]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Dissolved Solids Total","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,92,100,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Hardness Total","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,29,30,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Iron Dissolved","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,32,39,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Iron Total","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,121,153,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Lead Dissolved","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,1,1,"<","Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Lead Total","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,1,1,"<","Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Magnesium Total","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,1.7290000000000001,1.8260000000000001]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Manganese Dissolved","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,9.68,11.4,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Manganese Total","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,16.7,20.3,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Nickel Dissolved","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Nickel Total","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,4,4,"<","Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Nitrate as N Total","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,0.54,0.67,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Nitrite as N Total","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,0.04,0.04,"<","Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Nitrogen Total","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,0.67,0.74,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Orthophosphate Total","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,0.01,0.01,"<","Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Osmotic Pressure","mosm/kg","2010-10-28","2015-09-08",4.8630136986301373,57,0.93726331964417142,null,2,3]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","pH","ph units","2010-10-28","2015-09-08",4.8630136986301373,59,0.96365682004294606,7.335,7.4,7.5]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Phosphorus Total","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,0.01,0.01,"<","Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Selenium Total","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,7,7,"<","Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Sodium Total","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,14.1,15.9]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Specific Conductance","umhos/cm","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,143.5,156.69999999999999]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Strontium Total","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,30,33]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Sulfate Total","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,9.27,9.58,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Suspended Solids Total","mg/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,5,5,"<","Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Temperature Water (Field)","c","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,10.199999999999999,15.44]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Zinc Dissolved","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,6.33,7.5,null,"Y"]
["WQN0724","Laurel Hill Creek","SR 281 Br @ Ursina","Zinc Total","ug/l","2010-10-28","2015-09-08",4.8630136986301373,59,0.93255538809921068,null,7,7.8,null,"Y"]

{"sheet":"WQN0733","index":49,"n_rows":53,"n_cols":15,"rows_kept":53,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Alkalinity (Lab)","mg/l","2019-02-27","2024-02-21",4.9835616438356167,52,0.9296057789329375,10,11.5,14.2,null,"Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Aluminum Dissolved","ug/l","2019-02-27","2024-02-21",4.9835616438356167,52,0.9296057789329375,null,16.2,17.5,null,"Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Aluminum Total","ug/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,57,68.8,null,"Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Ammonia as N Dissolved","mg/l","2020-12-15","2024-02-21",3.1857923497267762,32,0.94989754026755691,null,0.02,0.02,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Ammonia as N Total","mg/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,0.02,0.02,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Barium Total","ug/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,36.299999999999997,38.4]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Boron Total","ug/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,200,200,"<"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Bromide Total","ug/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,25,25,"<"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Cadmium Dissolved","ug/l","2019-02-27","2024-02-21",4.9835616438356167,52,0.9296057789329375,null,0.2,0.2,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Calcium Dissolved","mg/l","2019-02-27","2024-02-21",4.9835616438356167,52,0.9296057789329375,null,6.82,7.49]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Calcium Total","mg/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,6.92,7.61,null,"Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Carbon Dissolved Organic","mg/l","2020-12-15","2024-02-21",3.1857923497267762,32,0.94989754026755691,null,1.01,1.27]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Carbon Total Organic","mg/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,0.9,1.1200000000000001]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,0.88,1.2,null,"Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Chloride Total","mg/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,4.5599999999999996,4.91,null,"Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Coliform Fecal","cf/100ml","2019-02-27","2024-01-30",4.9232876712328766,39,0.94674808590207227,null,25,50,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Copper Dissolved","ug/l","2019-02-27","2024-02-21",4.9835616438356167,52,0.9296057789329375,null,4,4,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Copper Total","ug/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,4,4,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Dissolved Oxygen (Field)","mg/l","2019-02-27","2024-02-21",4.9835616438356167,51,0.90808545018414566,9.8800000000000008,10.67]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Dissolved Solids Total","mg/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,50,54,null,"Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","E. Coli","cf/100ml","2019-02-27","2024-01-30",4.9232876712328766,38,0.92704861148376938,null,28.5,75]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Hardness Total","mg/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,24,25,null,"Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Iron Dissolved","ug/l","2019-02-27","2024-02-21",4.9835616438356167,52,0.9296057789329375,null,100,100,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Iron Total","ug/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,149,179,null,"Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Lead Dissolved","ug/l","2019-02-27","2024-02-21",4.9835616438356167,52,0.9296057789329375,null,1,1,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Lead Total","ug/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,1,1,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Lithium Dissolved","ug/l","2019-02-27","2024-02-21",4.9835616438356167,52,0.9296057789329375,null,25,25,"<"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Lithium Total","ug/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,25,25,"<"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Magnesium Dissolved","mg/l","2019-02-27","2024-02-21",4.9835616438356167,52,0.9296057789329375,null,1.51,1.55]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Magnesium Total","mg/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,1.52,1.61]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Manganese Dissolved","ug/l","2019-02-27","2024-02-21",4.9835616438356167,52,0.9296057789329375,null,11.95,13,null,"Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Manganese Total","ug/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,17.899999999999999,21.5,null,"Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Nickel Dissolved","ug/l","2019-02-27","2024-02-21",4.9835616438356167,52,0.9296057789329375,null,8,8,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Nickel Total","ug/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,8,8,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Nitrate + Nitrite as N Dissolved","mg/l","2020-12-15","2024-02-21",3.1857923497267762,32,0.94989754026755691,null,0.16,0.18,null,"Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Nitrate + Nitrite as N Total","mg/l","2020-09-29","2024-02-21",3.3961748633879778,36,0.93475466477684654,null,0.155,0.16,null,"Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Nitrogen Total","mg/l","2019-02-27","2024-02-21",4.9835616438356167,51,0.90808545018414566,null,0.25,0.26,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Orthophosphate Dissolved","mg/l","2020-12-15","2024-02-21",3.1857923497267762,32,0.94989754026755691,null,0.01,0.01,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Orthophosphate Total","mg/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,0.01,0.01,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Osmotic Pressure","mosm/kg","2020-10-27","2024-02-21",3.319672131147541,30,0.90126285329461109,null,1,1,"<"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","pH","ph units","2019-02-27","2024-02-21",4.9835616438356167,53,0.97299168234627753,6.83,7.0750000000000002,7.1950000000000003]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Phosphorus Dissolved","mg/l","2020-12-15","2024-02-21",3.1857923497267762,32,0.94989754026755691,null,0.01,0.01,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Phosphorus Total","mg/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,0.01,0.01,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Potassium Total","mg/l","2019-02-27","2024-02-21",4.9835616438356167,52,0.9296057789329375,null,1,1,"<"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Selenium Total","ug/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,7,7,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Sodium Total","mg/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,2.9,3.1]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Specific Conductance","umhos/cm","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,67.849999999999994,71.699999999999989]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Strontium Total","ug/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,24,26]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Suspended Solids Total","mg/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,20,20,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Temperature Water (Field)","c","2019-02-27","2024-02-21",4.9835616438356167,52,0.9296057789329375,null,9.3000000000000007,13.4]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Zinc Dissolved","ug/l","2019-02-27","2024-02-21",4.9835616438356167,52,0.9296057789329375,null,5,5.55,"<","Y"]
["WQN0733","MILL RUN","50 m dwnstr of Quebec Rd","Zinc Total","ug/l","2019-02-27","2024-02-21",4.9835616438356167,53,0.90162935155950785,null,5.99,6.43,null,"Y"]

{"sheet":"WQN0734","index":50,"n_rows":54,"n_cols":15,"rows_kept":54,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Alkalinity (Lab)","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,14.8,17.2,21,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Aluminum Dissolved","ug/l","2019-03-12","2024-02-20",4.942622950819672,48,0.94053662474622968,null,15.9,19.7,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Aluminum Total","ug/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,44.9,55.9,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Ammonia as N Dissolved","mg/l","2019-04-09","2024-02-20",4.8661202185792352,46,0.94592396814113033,null,0.02,0.02,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Ammonia as N Total","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,0.02,0.02,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Barium Total","ug/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,42.5,43.5]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Boron Total","ug/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,200,200,"<"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Bromide Total","ug/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,25,25,"<"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Cadmium Dissolved","ug/l","2019-03-12","2024-02-20",4.942622950819672,48,0.94053662474622968,null,0.2,0.2,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Calcium Dissolved","mg/l","2019-03-12","2024-02-20",4.942622950819672,47,0.92105930631851141,null,9.74,10.75]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Calcium Total","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,9.9700000000000006,11,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Carbon Dissolved Organic","mg/l","2020-10-15","2024-02-20",3.3497267759562841,33,0.91985668754205108,null,1,1]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Carbon Total Organic","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,1,1]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2019-03-12","2024-02-20",4.942622950819672,46,0.94592396814113033,null,0.86499999999999999,1.3,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Chloride Total","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,18.25,19.71,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Coliform Fecal","cf/100ml","2019-03-12","2024-01-23",4.8661202185792352,45,0.92754573983745547,null,25,25,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Copper Dissolved","ug/l","2019-03-12","2024-02-20",4.942622950819672,48,0.94053662474622968,null,4,4,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Copper Total","ug/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,4,4,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Dissolved Oxygen (Field)","mg/l","2019-03-12","2024-02-20",4.942622950819672,52,0.9296057789329375,10.17,10.744999999999999]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Dissolved Solids Total","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,70,74,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","E. Coli","cf/100ml","2019-03-12","2024-01-23",4.8661202185792352,45,0.92754573983745547,null,25,25,"<"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Hardness Total","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,30,33,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Iron Dissolved","ug/l","2019-03-12","2024-02-20",4.942622950819672,48,0.94053662474622968,null,100,100,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Iron Total","ug/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,100,100,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Lead Dissolved","ug/l","2019-03-12","2024-02-20",4.942622950819672,48,0.94053662474622968,null,1,1,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Lead Total","ug/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,1,1,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Lithium Dissolved","ug/l","2019-03-12","2024-02-20",4.942622950819672,48,0.94053662474622968,null,25,25,"<"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Lithium Total","ug/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,25,25,"<"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Magnesium Dissolved","mg/l","2019-03-12","2024-02-20",4.942622950819672,47,0.92105930631851141,null,1.24,1.33]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Magnesium Total","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,1.26,1.35]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Manganese Dissolved","ug/l","2019-03-12","2024-02-20",4.942622950819672,47,0.92105930631851141,null,4.25,4.83,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Manganese Total","ug/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,11.9,14.1,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Nickel Dissolved","ug/l","2019-03-12","2024-02-20",4.942622950819672,47,0.92105930631851141,null,8,8,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Nickel Total","ug/l","2019-03-12","2024-02-20",4.942622950819672,50,0.93509135292772771,null,8,8,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Nitrate + Nitrite as N Dissolved","mg/l","2019-07-02","2024-02-20",4.6366120218579239,43,0.93400596554420179,null,0.71,0.74,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Nitrate + Nitrite as N Total","mg/l","2019-04-09","2024-02-20",4.8661202185792352,45,0.92754573983745547,null,0.7,0.73,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Nitrogen Total","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,0.79,0.83,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Orthophosphate Dissolved","mg/l","2019-07-02","2024-02-20",4.6366120218579239,43,0.93400596554420179,null,0.01,0.01,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Orthophosphate Total","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,0.01,0.01,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Osmotic Pressure","mosm/kg","2020-10-15","2024-02-20",3.3497267759562841,29,0.93857165426015854,null,1,1,"<"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","pH","ph units","2019-03-12","2024-02-20",4.942622950819672,52,0.96351659999164008,6.9450000000000003,7.0325000000000006,7.1849999999999996]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Phosphorus Dissolved","mg/l","2019-04-09","2024-02-20",4.8661202185792352,46,0.94592396814113033,null,0.01,0.01,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Phosphorus Total","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,0.01,0.01,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Potassium Total","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,1,1,"<"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Selenium Total","ug/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,7,7,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Sodium Total","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,8.98,9.1849999999999987]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Specific Conductance","umhos/cm","2019-03-12","2024-02-20",4.942622950819672,52,0.9296057789329375,null,113.52500000000001,121.95]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Strontium Total","ug/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,20.5,23]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Sulfate Total","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,6.3,6.36,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Suspended Solids Total","mg/l","2019-03-12","2024-02-20",4.942622950819672,51,0.90808545018414566,null,20,20,"<","Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Temperature Water (Field)","c","2019-03-12","2024-02-20",4.942622950819672,52,0.9296057789329375,null,9,11.5]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Zinc Dissolved","ug/l","2019-03-12","2024-02-20",4.942622950819672,47,0.92105930631851141,null,5.44,6.5749999999999993,null,"Y"]
["WQN0734","Jones Mill Run","Along Laurel Hill State Rd","Zinc Total","ug/l","2019-03-12","2024-02-20",4.942622950819672,50,0.93509135292772771,null,7,7.1,null,"Y"]

{"sheet":"WQN0735","index":51,"n_rows":52,"n_cols":15,"rows_kept":52,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Alkalinity (Lab)","mg/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,76.599999999999994,84.199999999999989,100.4,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Aluminum Dissolved","ug/l","2019-03-25","2024-02-21",4.9098360655737707,51,0.90808545018414566,null,15,15,"<","Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Aluminum Total","ug/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,114,138,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Ammonia as N Dissolved","mg/l","2020-12-21","2024-02-21",3.1693989071038251,35,0.91046892106533028,null,0.02,0.02,"<","Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Ammonia as N Total","mg/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,0.02,0.02,"<","Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Barium Total","ug/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,42.35,45.2]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Boron Total","ug/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,200,200,"<"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Bromide Total","ug/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,25,25,"<"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Cadmium Dissolved","ug/l","2019-03-25","2024-02-21",4.9098360655737707,51,0.90808545018414566,null,0.2,0.2,"<","Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Calcium Dissolved","mg/l","2019-03-25","2024-02-21",4.9098360655737707,51,0.90808545018414566,null,30.22,34.1]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Calcium Total","mg/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,30.445,34.79,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Carbon Dissolved Organic","mg/l","2020-12-21","2024-02-21",3.1693989071038251,35,0.91046892106533028,null,2.11,2.3199999999999998]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Carbon Total Organic","mg/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,1.915,2.2400000000000002]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2019-03-25","2024-02-21",4.9098360655737707,53,0.90162935155950785,null,1.1000000000000001,1.3,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Chloride Total","mg/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,1.3149999999999999,1.43,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Copper Dissolved","ug/l","2019-03-25","2024-02-21",4.9098360655737707,51,0.90808545018414566,null,4,4,"<","Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Copper Total","ug/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,4,4,"<","Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Dissolved Oxygen (Field)","mg/l","2019-03-25","2024-02-21",4.9098360655737707,52,0.9296057789329375,9.1,10.125]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Dissolved Solids Total","mg/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,120,138,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Hardness Total","mg/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,95.5,108,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Iron Dissolved","ug/l","2019-03-25","2024-02-21",4.9098360655737707,51,0.90808545018414566,null,100,100,"<","Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Iron Total","ug/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,219,244,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Lead Dissolved","ug/l","2019-03-25","2024-02-21",4.9098360655737707,51,0.90808545018414566,null,1,1,"<","Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Lead Total","ug/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,1,1,"<","Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Lithium Dissolved","ug/l","2019-03-25","2024-02-21",4.9098360655737707,51,0.90808545018414566,null,25,25,"<"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Lithium Total","ug/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,25,25,"<"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Magnesium Dissolved","mg/l","2019-03-25","2024-02-21",4.9098360655737707,51,0.90808545018414566,null,4.4400000000000004,4.76]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Magnesium Total","mg/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,4.45,4.82]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Manganese Dissolved","ug/l","2019-03-25","2024-02-21",4.9098360655737707,51,0.90808545018414566,null,18.5,25.6,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Manganese Total","ug/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,29.4,35.700000000000003,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Nickel Dissolved","ug/l","2019-03-25","2024-02-21",4.9098360655737707,51,0.90808545018414566,null,8,8,"<","Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Nickel Total","ug/l","2019-03-25","2024-02-21",4.9098360655737707,53,0.90162935155950785,null,8,8,"<","Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Nitrate + Nitrite as N Dissolved","mg/l","2020-12-21","2024-02-21",3.1693989071038251,35,0.91046892106533028,null,0.11,0.14000000000000001,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Nitrate + Nitrite as N Total","mg/l","2020-09-30","2024-02-21",3.3934426229508201,39,0.94674808590207227,null,0.11,0.15,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Nitrogen Total","mg/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,0.28000000000000003,0.3,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Orthophosphate Dissolved","mg/l","2020-12-21","2024-02-21",3.1693989071038251,35,0.91046892106533028,null,1.2E-2,1.7000000000000001E-2,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Orthophosphate Total","mg/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,1.4500000000000001E-2,1.7999999999999999E-2,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Osmotic Pressure","mosm/kg","2020-11-18","2024-02-21",3.2595628415300548,29,0.93857165426015854,null,2,2]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","pH","ph units","2019-03-25","2024-02-21",4.9098360655737707,55,0.96997105458810751,7.7149999999999999,7.7949999999999999,7.875]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Phosphorus Dissolved","mg/l","2020-12-21","2024-02-21",3.1693989071038251,35,0.91046892106533028,null,1.4999999999999999E-2,0.02,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Phosphorus Total","mg/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,2.8500000000000001E-2,3.3000000000000002E-2,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Potassium Total","mg/l","2019-03-25","2024-02-21",4.9098360655737707,53,0.90162935155950785,null,1.62,1.83]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Selenium Total","ug/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,7,7,"<","Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Sodium Total","mg/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,3.43,3.94]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Specific Conductance","umhos/cm","2019-03-25","2024-02-21",4.9098360655737707,55,0.94193585320759066,null,196.6,212.85]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Strontium Total","ug/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,93,103]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Sulfate Total","mg/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,14.48,15.18,null,"Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Suspended Solids Total","mg/l","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,20,20,"<","Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Temperature Water (Field)","c","2019-03-25","2024-02-21",4.9098360655737707,54,0.92409527051089835,null,12.58,14.8]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Zinc Dissolved","ug/l","2019-03-25","2024-02-21",4.9098360655737707,51,0.90808545018414566,null,5,5,"<","Y"]
["WQN0735","House Run (UNT)","Bristoria Rd Crossing (SR3020)","Zinc Total","ug/l","2019-03-25","2024-02-21",4.9098360655737707,53,0.90162935155950785,null,5,5,"<","Y"]

{"sheet":"WQN0870","index":52,"n_rows":51,"n_cols":15,"rows_kept":51,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Alkalinity (Lab)","mg/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,3.2,4.2,5.2,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Aluminum Dissolved","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,94,107,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Aluminum Total","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,202,228,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Ammonia as N Total","mg/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,0.02,0.02,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Arsenic Dissolved","ug/l","2016-05-24","2020-09-08",4.2931506849315069,49,0.91456686684260546,null,3,3,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Barium Total","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,32.4,33.6]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Boron Total","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,200,200,"<"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Bromide Total","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,25,25,"<"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Cadmium Dissolved","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,0.2,0.2,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Calcium Dissolved","mg/l","2016-05-24","2021-05-17",4.9808219178082194,54,0.92409527051089835,null,3.6850000000000001,4.01]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Calcium Total","mg/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,3.7269999999999999,4.2050000000000001,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Carbon Total Organic","mg/l","2016-05-24","2021-05-17",4.9808219178082194,54,0.92409527051089835,null,1.74,2.02]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,0.84,0.95,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Chloride Total","mg/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,2.56,2.96,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Coliform Fecal","cf/100ml","2016-05-24","2021-05-17",4.9808219178082194,54,0.92409527051089835,null,25,25,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Copper Dissolved","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,4,4,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Copper Total","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,4,4,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Dissolved Oxygen (Field)","mg/l","2016-05-24","2021-05-17",4.9808219178082194,54,0.92409527051089835,9.9499999999999993,10.904999999999999]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Dissolved Solids Total","mg/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,38,42,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","E. Coli","cf/100ml","2016-05-24","2021-05-17",4.9808219178082194,38,0.92704861148376938,null,25,25,"<"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Hardness Total","mg/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,13,14,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Iron Dissolved","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,100,100,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Iron Total","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,202,220,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Lead Dissolved","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,1,1,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Lead Total","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,1,1,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Lithium Dissolved","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,25,25,"<"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Lithium Total","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,25,25,"<"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Magnesium Dissolved","mg/l","2016-05-24","2021-05-17",4.9808219178082194,54,0.92409527051089835,null,0.84299999999999997,0.88]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Magnesium Total","mg/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,0.84499999999999997,0.90800000000000003]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Manganese Dissolved","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,47,57.9,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Manganese Total","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,56.3,63.4,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Nickel Dissolved","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,8,8,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Nickel Total","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,8,8,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Nitrate as N Total","mg/l","2016-05-24","2020-09-08",4.2931506849315069,49,0.91456686684260546,null,0.31,0.34,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Nitrite as N Total","mg/l","2016-05-24","2020-09-08",4.2931506849315069,49,0.91456686684260546,null,0.04,0.04,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Nitrogen Total","mg/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,0.47,0.52,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Orthophosphate Total","mg/l","2016-05-24","2021-05-17",4.9808219178082194,54,0.92409527051089835,null,0.01,0.01,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Osmotic Pressure","mosm/kg","2016-05-24","2021-05-17",4.9808219178082194,32,0.94989754026755691,null,1,1,"<"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","pH","ph units","2016-05-24","2021-05-17",4.9808219178082194,55,0.96997105458810751,6.85,7.0350000000000001,7.21]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Phosphorus Total","mg/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,0.01,0.01,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Potassium Total","mg/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,1,1,"<"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Selenium Total","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,7,7,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Sodium Total","mg/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,1.62,1.76]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Specific Conductance","umhos/cm","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,40.900000000000013,42]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Strontium Total","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,15,16]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Sulfate Total","mg/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,7.66,8,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Suspended Solids Total","mg/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,5,5,"<","Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Temperature Water (Field)","c","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,9.9,14.4]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Zinc Dissolved","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,11.4,12.6,null,"Y"]
["WQN0870","CLEAR SHADE CREEK","250 ft upstr of SR160 (Dark Shade Rd) Br - Cairnbrook","Zinc Total","ug/l","2016-05-24","2021-05-17",4.9808219178082194,55,0.94193585320759066,null,13.7,14.6,null,"Y"]

{"sheet":"WQN0873","index":53,"n_rows":51,"n_cols":15,"rows_kept":51,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Alkalinity (Lab)","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,14.2,16.8,20.2,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Aluminum Dissolved","ug/l","2014-12-09","2019-11-06",4.9095890410958907,60,0.90753901892707578,null,19.55,21,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Aluminum Total","ug/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,98.5,107,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Ammonia as N Total","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,0.02,0.02,"<","Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Arsenic Dissolved","ug/l","2014-12-09","2019-11-06",4.9095890410958907,60,0.90753901892707578,null,3,3,"<","Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Barium Total","ug/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,17.2,18.8]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Boron Total","ug/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,200,200,"<"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Bromide Total","ug/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,25,25,"<"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Cadmium Dissolved","ug/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,0.2,0.2,"<","Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Calcium Dissolved","mg/l","2015-05-07","2019-11-06",4.5,54,0.92409527051089835,null,6.2720000000000002,6.7539999999999996]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Calcium Total","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,6.1840000000000002,7.1070000000000002,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Carbon Total Organic","mg/l","2015-05-07","2019-11-06",4.5,54,0.92409527051089835,null,2.08,2.2200000000000002]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2015-04-21","2019-11-06",4.5437158469945356,59,0.93255538809921068,null,1.1000000000000001,1.3,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Chloride Total","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,3.36,3.94,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Coliform Fecal","cf/100ml","2014-12-09","2019-11-06",4.9095890410958907,46,0.94592396814113033,null,38,70,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Copper Dissolved","ug/l","2014-12-09","2019-11-06",4.9095890410958907,60,0.90753901892707578,null,4,4,"<","Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Copper Total","ug/l","2014-12-09","2019-11-06",4.9095890410958907,60,0.90753901892707578,null,4,4,"<","Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Dissolved Oxygen (Field)","mg/l","2014-12-09","2019-11-06",4.9095890410958907,54,0.92409527051089835,9.92,11.154999999999999]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Dissolved Solids Total","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,57,62,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","E. Coli","cf/100ml","2016-07-06","2019-11-06",3.3360655737704921,39,0.94674808590207227,null,50,90]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Hardness Total","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,23,26,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Iron Dissolved","ug/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,154,210,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Iron Total","ug/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,463,507,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Lead Dissolved","ug/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,1,1,"<","Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Lead Total","ug/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,1,1,"<","Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Lithium Dissolved","ug/l","2016-03-08","2019-11-06",3.6639344262295079,44,0.90385824557938566,null,25,25,"<"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Lithium Total","ug/l","2016-03-08","2019-11-06",3.6639344262295079,44,0.90385824557938566,null,25,25,"<"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Magnesium Dissolved","mg/l","2015-05-07","2019-11-06",4.5,54,0.92409527051089835,null,1.7569999999999999,1.9]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Magnesium Total","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,1.8029999999999999,1.91]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Manganese Dissolved","ug/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,16.399999999999999,17.2,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Manganese Total","ug/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,21.7,24.74,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Nickel Dissolved","ug/l","2014-12-09","2019-08-08",4.6630136986301371,57,0.93726331964417142,null,4,4,"<","Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Nickel Total","ug/l","2014-12-09","2019-08-08",4.6630136986301371,57,0.93726331964417142,null,4,4,"<","Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Nitrate as N Total","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,0.39,0.49,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Nitrite as N Total","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,0.04,0.04,"<","Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Nitrogen Total","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,0.56000000000000005,0.6,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Orthophosphate Total","mg/l","2015-04-21","2019-11-06",4.5437158469945356,59,0.93255538809921068,null,0.01,0.01,"<","Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Osmotic Pressure","mosm/kg","2014-12-09","2018-11-13",3.9287671232876709,38,0.92704861148376938,null,1,1,"<"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","pH","ph units","2014-12-09","2019-11-06",4.9095890410958907,66,0.96441727554776824,7.2650000000000006,7.375,7.4450000000000003]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Phosphorus Total","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,1.6E-2,1.7999999999999999E-2,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Potassium Total","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,1.0209999999999999,1.18]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Selenium Total","ug/l","2014-12-09","2019-11-06",4.9095890410958907,60,0.90753901892707578,null,7,7,"<","Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Sodium Total","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,3.0779999999999998,3.2610000000000001]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Specific Conductance","umhos/cm","2014-12-09","2019-11-06",4.9095890410958907,66,0.93598249586277404,null,64.674999999999997,70.150000000000006]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Strontium Total","ug/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,26,29]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Sulfate Total","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,6.79,6.99,null,"Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Suspended Solids Total","mg/l","2014-12-09","2019-11-06",4.9095890410958907,61,0.92782256149907727,null,5,5,"<","Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Temperature Water (Field)","c","2014-12-09","2019-11-06",4.9095890410958907,67,0.91356276572652872,null,10.7,13]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Zinc Dissolved","ug/l","2014-12-09","2019-11-06",4.9095890410958907,60,0.90753901892707578,null,5,5,"<","Y"]
["WQN0873","WEST BRANCH CALDWELL CREEK","250 m upstr of Flat Rd (T304) Br NE of Selkirk","Zinc Total","ug/l","2014-12-09","2019-11-06",4.9095890410958907,60,0.90753901892707578,null,5,5,"<","Y"]

{"sheet":"WQN0877","index":54,"n_rows":41,"n_cols":15,"rows_kept":41,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Alkalinity (Lab)","mg/l","2005-10-19","2010-09-14",4.904109589041096,49,0.91456686684260546,4.4000000000000004,5.2,6.8,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Aluminum Dissolved","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,16.649999999999999,20.9,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Aluminum Total","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,80.699999999999989,89.4,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Ammonia as N Total","mg/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,0.02,0.02,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Arsenic Dissolved","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,4,4,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Barium Total","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,22.25,23]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Cadmium Dissolved","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,0.2,0.2,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Calcium Total","mg/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,2.64,2.87,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,0.7,0.8,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Chloride Total","mg/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,1.47,1.59,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Coliform Fecal","cf/100ml","2005-10-19","2010-09-14",4.904109589041096,48,0.94053662474622968,null,20,40,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Copper Dissolved","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,4,4,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Copper Total","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,4,4,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Dissolved Oxygen (Field)","mg/l","2005-10-19","2010-09-14",4.904109589041096,48,0.94053662474622968,10,10.35]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Dissolved Solids Total","mg/l","2005-10-19","2010-09-14",4.904109589041096,49,0.91456686684260546,null,44,50,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Fluoride Total","mg/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,0.2,0.2,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Hardness Total","mg/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,12,13,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Iron Dissolved","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,59,70,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Iron Total","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,376,464,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Lead Dissolved","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,1,1,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Lead Total","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,1,1,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Magnesium Total","mg/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,1.2909999999999999,1.369]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Manganese Dissolved","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,14.45,16.100000000000001,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Manganese Total","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,22.1,24.3,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Nickel Dissolved","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,4,4,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Nickel Total","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,4,4,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Nitrate as N Total","mg/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,0.13,0.16,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Nitrite as N Total","mg/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,0.04,0.04,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Nitrogen Total","mg/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,0.24,0.27,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Orthophosphate Total","mg/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,0.01,0.01,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Osmotic Pressure","mosm/kg","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,1,1,"<"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","pH","ph units","2005-10-19","2010-09-14",4.904109589041096,50,0.96716086243573141,6.59,6.8,6.9]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Phenols Total","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,5,5,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Phosphorus Total","mg/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,0.01,1.0999999999999999E-2,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Specific Conductance","umhos/cm","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,41.825000000000003,43.25]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Sulfate Total","mg/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,7.9050000000000002,8.3000000000000007,null,"Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Suspended Solids Total","mg/l","2005-10-19","2010-09-14",4.904109589041096,49,0.91456686684260546,null,5,5,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Temperature Water (Field)","c","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,10.3,12.9]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Zinc Dissolved","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,5,5,"<","Y"]
["WQN0877","EAST HICKORY CREEK","Upstr of Forest Service Rd 119 Nr Queen, PA","Zinc Total","ug/l","2005-10-19","2010-09-14",4.904109589041096,50,0.93509135292772771,null,5,5.2,"<","Y"]

{"sheet":"WQN0879","index":55,"n_rows":44,"n_cols":15,"rows_kept":44,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Alkalinity (Lab)","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,41.4,46.3,55.4,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Aluminum Dissolved","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,10,11,"<","Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Aluminum Total","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,86.85,93.5,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Ammonia as N Total","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,0.03,0.04,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Arsenic Dissolved","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Barium Total","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,17.45,20.100000000000001]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Cadmium Dissolved","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,0.2,0.2,"<","Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Calcium Dissolved","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,16.649999999999999,21]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Calcium Total","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,16.975000000000001,21.3,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Carbon Total Organic","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,3.895,4.1500000000000004]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,1.05,1.1499999999999999,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Chloride Total","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,9.2249999999999996,9.83,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Coliform Fecal","cf/100ml","2005-10-26","2010-09-22",4.9068493150684933,55,0.94193585320759066,null,80,180,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Copper Dissolved","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Copper Total","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Dissolved Oxygen (Field)","mg/l","2005-10-26","2010-09-22",4.9068493150684933,55,0.94193585320759066,8,9.4]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Dissolved Solids Total","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,116,124,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Fluoride Total","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,0.2,0.2,"<","Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Hardness Total","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,55.25,69,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Iron Dissolved","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,130,144,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Iron Total","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,569,739,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Lead Dissolved","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Lead Total","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,1,1,"<","Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Magnesium Dissolved","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,3.0924999999999998,3.8490000000000002]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Magnesium Total","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,3.25,3.923]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Manganese Dissolved","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,81.224999999999994,128.5,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Manganese Total","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,92,146,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Nickel Dissolved","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Nickel Total","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,4,4,"<","Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Nitrate as N Total","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,0.115,0.15,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Nitrite as N Total","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,0.04,0.04,"<","Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Nitrogen Total","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,0.41,0.46,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Orthophosphate Total","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,1.6500000000000001E-2,1.9E-2,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Osmotic Pressure","mosm/kg","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,2,2]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","pH","ph units","2005-10-26","2010-09-22",4.9068493150684933,56,0.95595345389784914,7.25,7.3250000000000002,7.4]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Phenols Total","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Phosphorus Total","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,2.5000000000000001E-2,3.2000000000000001E-2,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Specific Conductance","umhos/cm","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,142.125,167.7]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Sulfate Total","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,8.8550000000000004,9.35,null,"Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Suspended Solids Total","mg/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,5,6,"<","Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Temperature Water (Field)","c","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,12.2,16.5]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Zinc Dissolved","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,5,5,"<","Y"]
["WQN0879","WOODCOCK CREEK","50 m upstr of SR 2036 Br","Zinc Total","ug/l","2005-10-26","2010-09-22",4.9068493150684933,56,0.91857318539049337,null,5,5,"<","Y"]

{"sheet":"WQN0885","index":56,"n_rows":52,"n_cols":15,"rows_kept":52,"cut":false,"hidden":true,"merged":[]}
["WQN","Stream","Location","Parameter","Unit","minDate","maxDate","Period_of_Record_Years","n","coverage","lower","median","upper","DL","guidance"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Alkalinity (Lab)","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,4.2,5.2,6.8,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Aluminum Dissolved","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,36.799999999999997,44.4,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Aluminum Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,76.099999999999994,92.1,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Ammonia as N Dissolved","mg/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,0.02,0.02,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Ammonia as N Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,0.02,0.02,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Barium Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,30.3,31.3]
["WQN0885","Piney Run","Beside Easy Camp Rd","Boron Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,200,200,"<"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Bromide Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,25,25,"<"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Cadmium Dissolved","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,0.2,0.2,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Calcium Dissolved","mg/l","2021-02-09","2024-03-26",3.12568306010929,34,0.94238732708618034,null,2.665,3.15]
["WQN0885","Piney Run","Beside Easy Camp Rd","Calcium Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,2.74,3.2410000000000001,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Carbon Dissolved Organic","mg/l","2021-02-09","2024-02-26",3.0464480874316942,33,0.91985668754205108,null,0.88,1]
["WQN0885","Piney Run","Beside Easy Camp Rd","Carbon Total Organic","mg/l","2020-09-17","2024-02-26",3.442622950819672,38,0.92704861148376938,null,0.91999999999999993,1.06]
["WQN0885","Piney Run","Beside Easy Camp Rd","Carbonaceous Biochemical Oxygen Demand - 5 Day","mg/l","2021-02-09","2024-03-26",3.12568306010929,34,0.94238732708618034,null,0.76,1.04,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Chloride Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,0.88,0.92,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Copper Dissolved","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,4,4,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Copper Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,4,4,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Dissolved Oxygen (Field)","mg/l","2020-10-20","2024-03-26",3.4316939890710381,38,0.92704861148376938,10.51,11.475]
["WQN0885","Piney Run","Beside Easy Camp Rd","Dissolved Solids Total","mg/l","2020-09-17","2024-02-26",3.442622950819672,38,0.92704861148376938,null,24,28,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Hardness Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,10,11,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Iron Dissolved","ug/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,100,100,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Iron Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,109.5,131,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Lead Dissolved","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,1,1,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Lead Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,1,1,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Lithium Dissolved","ug/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,25,25,"<"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Lithium Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,25,25,"<"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Magnesium Dissolved","mg/l","2021-02-09","2024-03-26",3.12568306010929,34,0.94238732708618034,null,0.69,0.72]
["WQN0885","Piney Run","Beside Easy Camp Rd","Magnesium Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,0.7,0.74]
["WQN0885","Piney Run","Beside Easy Camp Rd","Manganese Dissolved","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,23,27.4,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Manganese Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,29.6,36,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Nickel Dissolved","ug/l","2021-02-09","2024-03-26",3.12568306010929,35,0.91046892106533028,null,8,8,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Nickel Total","ug/l","2021-02-09","2024-03-26",3.12568306010929,35,0.91046892106533028,null,8,8,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Nitrate + Nitrite as N Dissolved","mg/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,0.44,0.46,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Nitrate + Nitrite as N Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,0.45,0.49,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Nitrogen Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,0.51,0.55000000000000004,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Orthophosphate Dissolved","mg/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,0.01,0.01,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Orthophosphate Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,0.01,0.01,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Osmotic Pressure","mosm/kg","2020-10-20","2024-03-26",3.4316939890710381,30,0.90126285329461109,null,1,1,"<"]
["WQN0885","Piney Run","Beside Easy Camp Rd","pH","ph units","2020-09-17","2024-03-26",3.5218579234972678,39,0.97629729752952699,6.42,6.5750000000000002,6.8]
["WQN0885","Piney Run","Beside Easy Camp Rd","Phosphorus Dissolved","mg/l","2020-09-17","2024-02-26",3.442622950819672,35,0.91046892106533028,null,0.01,0.01,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Phosphorus Total","mg/l","2020-09-17","2024-02-26",3.442622950819672,36,0.93475466477684654,null,0.01,0.01,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Potassium Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,1,1,"<"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Selenium Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,7,7,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Sodium Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,0.5,0.52]
["WQN0885","Piney Run","Beside Easy Camp Rd","Specific Conductance","umhos/cm","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,26.75,28.8]
["WQN0885","Piney Run","Beside Easy Camp Rd","Strontium Total","ug/l","2020-09-17","2024-03-26",3.5218579234972678,38,0.92704861148376938,null,13,14]
["WQN0885","Piney Run","Beside Easy Camp Rd","Sulfate Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,4.66,4.82,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Suspended Solids Total","mg/l","2020-09-17","2024-03-26",3.5218579234972678,39,0.94674808590207227,null,20,20,"<","Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Temperature Water (Field)","c","2020-10-20","2024-03-26",3.4316939890710381,38,0.92704861148376938,null,5.75,10]
["WQN0885","Piney Run","Beside Easy Camp Rd","Zinc Dissolved","ug/l","2021-02-09","2024-02-26",3.0464480874316942,34,0.94238732708618034,null,7.6,8.9700000000000006,null,"Y"]
["WQN0885","Piney Run","Beside Easy Camp Rd","Zinc Total","ug/l","2021-02-09","2024-02-26",3.0464480874316942,34,0.94238732708618034,null,7.4250000000000007,8.65,null,"Y"]